IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| CR for CID 4036 | | | | |
| Date: 2022-03-09 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Xiaofei Wang | InterDigital Inc. | 111 West 33rd Street  New York, NY 10120  USA | +1-607-592-2727 | Xiaofei.wang@interdigital.com |
| Rui Yang |  |  |
| Antonio De La Oliva |  |  |  |

Abstract

This submission proposes the spec text for resolutions for the CID 4035. The baseline for this comment resolution document is 802.11bc Draft 4.0.

* Rev 0: first draft

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 4036 | John Wullert | 11.55.3.9 | 87.16 | The description of the termination uses the general term STA to refer to the broadcaster of the EPCS traffic streams. However, the processes for negotiation, in clauses 11.55.3.7 and 11.55.3.8, describe a non-AP STA interacting with an EBCS AP. This seems inconsistent | Adjust language to remove inconsistency (e.g., use AP terminology in 11.55.3.9) or add a note indicating how/why a non-AP STA would be sending a termination notice | Revised: agree with the comment. Clarification has been added that only AP transmits the EBCS DL traffic. |

**11.55.3.9 EBCS termination notice procedure**

The EBCS termination notice procedure allows a STA that is a broadcaster of EBCS traffic streams to indicate

that one or more of the EBCS traffic streams that it is broadcasting is to be terminated. In EBCS DL, the broadcaster of one or more EBCS traffic streams is an EBCS AP.