IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| LB266 CR on EHT PHY Introduction-2 | | | | |
| Date: 2022-09-13 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Kanke Wu | Qualcomm Inc |  |  | kankew@qti.qualcomm.com |
| Bin Tian | Qualcomm Inc |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This submission proposes resolutions for the following 15 comments from CC36 in P802.11be D2.0:

12575, 11630, 11631, 12576, 12529, 12134, 12547, 11330, 11331, 12518,

12519, 11333, 11334

This proposed text changes in this document are based on TGbe Draft 2.1


Revisions:

* Rev 0: Initial version of the document.

# CID 12575

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page.Line** | **Comment** | **Proposed Change** | **Resolutions** |
| 12575 | 36.1.1 | 542.05 | The EHT-MCS 14 means 'BPSK-DCM+DUP', it is not accurate to say 'EHT introduces EHT DUP mode as EHT-MCS 14'. | Revise it to mention the EHT DUP mode is introduced for single user transmission modulated using BPSK-DCM as EHT-MCS 14. | REVISED.  EHT DUP mode is newly introduced in 11be. The current sentence already mentioned this mode is for single user transmission with single spatial stream and LDPC coding. We will modify this sentence to further specify it uses BPSK+DCM as modulation method.  Instruction to the editor:  Please modify P554 L 7-8 in D2.1 as following:  The EHT PHY introduces EHT DUP mode for single user transmission with single spatial stream and LDPC coding using BPSK-DCM in the 6 GHz band as EHT-MCS 14. |

**Background:**



# CID 11630, 11631, 12576

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page.Line** | **Comment** | **Proposed Change** | **Resolution** |
| 11630 | 36.1.1 | 542.18 | Redundant sentence. No need to mention it as it directly derived from row 12 | Remove this line | REVISED.  Agree that this sentence is redundant. We will change the description of the main bullet to make it clear BCC is only used in specific situations.  Instruction to the editor:  Please modify P554 L 15 in D2.1 as following:  BCC coding (transmit and receive). BCC coding is ONLY supported for EHT PPDUs where all of the following conditions are satisfied:  Delete the following sentence at line 21: |
| 12576 | 36.1.1 | 542.18 | The sentence mentioning 'BCC coding is not supported in EHT PPDUs where...' is kind of redundant. | Delete the sentence, just to revise sentence of the second bullet to ' BCC coding is supported and only supported for EHT PPDUs where all of the following conditions are satisfied: | REVISED.  Agree with the comment in principle. The sentence is revised to reflect this information.  Instruction to the editor:  The resolution to this CID is the same as 11630 |
| 11631 | 36.1.1 | 542.11 | Descripction of BCC coding restriction doesn't belong to this section, as this section focuses on what STA needs to support | Keep the text "BCC coding (transmit and receive)" and move the rest before P542L8. It should be part of general description of EHT features | REJECTED  To keep the description consistent with LDPC case and provide complete information, the detailed cases where BCC is used is needed in this introduction section to avoid confusion that BCC may be needed in other cases. |

**Background:**

A picture containing text

Description automatically generated

# CID 12529

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page.Line** | **Comment** | **Proposed Change** | **Resolution** |
| 12529 | 36.1.1 | 542.35 | "EHT-MCS 15 (transmit and receive) for- 26-, 52-, 106-, 242-, 484-, and 996-tone RU if the STA declares support for larger than 20 MHz  PPDU"-Here to support 996 RU, the STA has to support atleast 80 Mhz Bandwidth. | We propose the change as "26-, 52-, 106-, 242-, 484-, and 996-tone RU if the STA declares support for larger than or equal to 80 MHz PPDU" | ACCEPTED  Note to the editor:  Located at P554L40 in D2.1 |

**Background:**

A picture containing diagram

Description automatically generated

# CID 12134

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page.Line** | **Comment** | **Proposed Change** | **Resolution** |
| 12134 | 36.1.1 | 542.42 | what does mean "transmit and receive for single user"? It is better to reword these three bullets for easy of understanding | Change "EHT MU PPDU with a 2xEHT-LTF and 0.8 Î¼s GI duration on the EHT-LTF and Data field OFDM symbols (transmit and receive for single user)." to "EHT MU PPDU addressed to a single user and with a 2xEHT-LTF and 0.8 Î¼s GI duration on the EHT-LTF and Data field OFDM symbols (transmit and receive)."  Change "EHT MU PPDU with a 2xEHT-LTF and 1.6 Î¼s GI duration on the EHT-LTF and Data field OFDM symbols (transmit and receive for single user)." to "EHT MU PPDU addressed to a single user and with a 2xEHT-LTF and 1.6 Î¼s GI duration on the EHT-LTF and Data field OFDM symbols (transmit and receive).  Change "EHT MU PPDU with a 4xEHT-LTF and 3.2 Î¼s GI duration on the EHT-LTF and Data field OFDM symbols (transmit and receive for single user)." to "EHT MU PPDU addressed to a single user and with a 4xEHT-LTF and 3.2 Î¼s GI duration on the EHT-LTF and Data field OFDM symbols (transmit and receive)." | ACCEPTED  Note to the editor:  Located at P554L47 in D2.1 |

**Background:**


Text

Description automatically generated

# CID 12547

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page.Line** | **Comment** | **Proposed Change** | **Resolution** |
| 12547 | 36.1.1 | 542.60 | This sentence is very vague. It needs to be rewritten to convey the intended meaning clearly. | The sentence may be rewritten as "- EHT-MCSs 8 to 13 (transmit and receive) if the STA is a 20  MHz-only non-AP STA and EHT-MCSs 10 to 13 (transmit and receive) if the STA is not a 20  MHz-only non-AP STA." | ACCEPTED  Note to the editor:  Located at P555L6 in D2.1 |


**Background:**



# CID 11330

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page.Line** | **Comment** | **Proposed Change** | **Resolution** |
| 11330 | 36.1.1 | 544.04 | Simplify "MU-MIMO reception on an RU or MRU in an EHT TB PPDU where the RU or MRU is of size larger than or equal to 242 tones in the supported bandwidth non-OFDMA transmission (UL MU-MIMO)" to "Receiption of a non-OFDMA EHT MU PPDU unitilizing MU-MIMO (DL MU-MIMO). This change is to align with the Tx requirements (2 bullets above). MU MIMO on >=242 tone RU has already been covered in P541 L 40 | as in the comment | REVISED  Agree with the suggested change. However, the requirement should be for Reception of EHT TB PPDU instead of EHT MU PPDU  Instruction to the editor:  Please modify P556 L8 in D2.1 as following:  Reception of a non-OFDMA EHT TB PPDU using MU-MIMO (UL MU-MIMO) where the RU or MRU is of size larger than or equal to 242 tones in the supported bandwidth when the AP is not capable of receiving equal to or more than 4 spatial streams |

**Background:**



# CID 11331

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page.Line** | **Comment** | **Proposed Change** | **Resolution** |
| 11331 | 36.1.1 | 544.22 | To differentiate from non-OFDMA tranmission, change "where the RU or MRU allocated to the non-AP STA" to "where there are mulitiple RU or MRUs and the one assigned to the non-AP STA". Make similar changes to the next bullet Tx support | as in the comment | REVISED.  Agree with the commenter. We will make similar changes to the next bullet as well.  Instruction to the editor:  Please modify P556 L26 in D2.1 as following:  —Reception of an EHT MU PPDU where there are multiple RU or MRUs and the RU or MRU allocated to the non-AP STA is not utilizing MU-MIMO (DL OFDMA).  —Transmission of an EHT TB PPDU where there are multiple RU or MRUs and the RU or MRU allocated to the non-AP STA is not utilizing MU-MIMO (UL OFDMA). |

**Background:**

Graphical user interface, text, Word

Description automatically generated

# CID 12519, 12518


|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page.Line** | **Comment** | **Proposed Change** | **Resolution** |
| 12519 | 36.1.1 | 544.28 | "A non-AP EHT STA shall support the following features:Reception of a non-OFDMA EHT MU PPDU utilizing MU-MIMO (DL MU-MIMO) in the supported bandwidth"-Regarding this, more clarity is needed with respect to AP's bandwidth. | For a 20 Mhz only STA, if the AP's bandwidth is greater than 20 Mhz, then Reception of 242 tone RU EHT MU PPDU is optional. Hence please clarify. | REJECTED  This bullet is specific to non-OFDMA reception. Based on the definition of non-OFDMA EHT PPDU, there is only a single RU or MRU occupying all the nonpunctured 20MHz channels within the PPDU bandwidth. The case mentioned by the commenter would hence be an OFDMA use case and won’t be covered by this requirement. |
| 12518 | 36.11 | 544.35 | "A non-AP EHT STA shall support the following features:MU-MIMO transmission in a non-OFDMA EHT TB PPDU (UL MU-MIMO)."- Regarding this, more clarity is needed with respect to AP's bandwidth. | For a 20 Mhz only STA, if the AP's bandwidth is greater than 20 Mhz, then transmission of 242 tone RU EHT TBPPDU is restricted. Hence please clarify. | REJECTED  This bullet is specific to non-OFDMA transmission. Based on the definition of non-OFDMA EHT PPDU, there is only a single RU or MRU occupying all the nonpunctured 20MHz channels within the PPDU bandwidth. The case mentioned by the commenter would hence be an OFDMA use case and won’t be covered by this requirement. |

**Background:**

A picture containing text

Description automatically generated

**In clause 3 definition of acronyms and abbreviations.**



# CID 11333

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page.Line** | **Comment** | **Proposed Change** | **Resolution** |
| 11333 | 36.1.1 | 546.10 | Change "when the BSS bandwidth is 320  MHz" to "for a 320 MHz PPDU" | as in the comment | ACCEPTED |

**Background:**

A picture containing text

Description automatically generated

# CID 11334

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page.Line** | **Comment** | **Proposed Change** | **Resolution** |
| 11334 | 36.1.1 | 546.14 | "LDPC coding if the maximum number of spatial streams the STA is capable of transmitting or receiving in an EHT MU PPDU is less than or equal to 4, if the non-AP STA is a 20  MHz only non-AP STA that does not support any of EHT-MCS  10, 11, 12 or 13." Too many ifs. May combine them using and/or | as in the comment | REVISED  Agree with the commenter that the current sentence is a bit hard to read.  Instruction to the editor:  Please modify P558 L14 in D2.1 as following:  — LDPC coding if the maximum number of spatial streams the STA is capable of transmitting or receiving in an EHT MU PPDU is less than or equal to 4, and the non-AP STA is a 20 MHz only non-AP STA that does not support any of the EHT-MCS 10, 11, 12 or 13. |

**Background:**

