IEEE P802.11
Wireless LANs

|  |
| --- |
| Comment Resolution for Instance CID  |
| Date: 2022-11-20 |
| Author(s): |
| Name | Affiliation | Address | Phone | Email |
| Anirudha Sahoo | NIST | 100 Bureau Dr, Gaithersburg, MD 20899 |  | anirudha.sahoo@nist.gov |
|  |  |  |  |  |

Abstract

This document resolves comment with CID 130

**Revision History:**

R0: Initial version

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Commentor** | **Clause Number** | **Page** | **Comment** | **Proposed Change** |
| 130 | Sigurd Schelstraete | 11.21.18.7 | 71.55 | "an Initiator-to-Responder (I2R) NDP". What is the format of the I2R NDP? what makes I2R different from R2I? | Clarify |

**Proposed Resolution:** Revise

**Discussion:** This has been addressed by document 11-22-1937r3 which has passed the motion. As per that document:

1. **TB sensing case**:
2. **NDPA sounding**:

When a PPDU bandwidth <= 160 MHz, the format of the SI2SR NDP shall be a HE Ranging NDP.

When the PPDU bandwidth= 320 MHz, the format of SI2SR NDP shall be an EHT sounding NDP.

b) **TF sounding**:

When a PPDU bandwidth <= 160 MHz, the format of the SR2SI shall be an HE TB Ranging NDP. 320 MHz operation is not supported.

2. **NTB sensing case**:

When a PPDU bandwidth <= 160 MHz, the format of both the SI2SR NDP and SR2SI NDP shall be a HE Ranging NDP. 320 MHz operation is not supported.

 **Modifications:** Editor: No modification is needed to the latest draft.