IEEE P802.11
Wireless LANs

|  |
| --- |
| **LB271 Comment Resolution for CID 16635** |
| **Date:** 2023-03-09 |
| **Author(s):** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Name** | **Affiliation** | **Address** | **Phone** | **Email** |
| Insik Jung | LG Electronics | 19, Yangjae-daero 11gil, Seocho-gu, Seoul 137-130, Korea  |   | insik0618.jung@lge.com |
| Eunsung Park |  | esung.park@lge.com |
| Dongguk Lim |  | dongguk.lim@lge.com |
| Jinyoung Chun |  | jiny.chun@lge.com |
| Jinsoo Choi |  | js.choi@lge.com |

Abstract

This submission proposes a resolution for CID 16635

Baseline document: TGbe D3.0 Draft

Revisions:

* Rev 0: Initial version of the document.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

#### *CID 16635*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **PP.LL** | **Comment** | **Proposed Change** | **Resolution** |
| 16635 | 36.3.4 | 729.02 | The non-AP STA will send only using allocated 20 MHz channels. Since "the pre-EHT modulation fields are sent only on the 20 MHz channels where the STA's EHT modulated fields are present", we don't need to mention "nonpunctured" 20 MHz channels" | replace "multiple nonpunctured 20 MHz channels" to "all 20 MHz channels EHT modulated fields are occupied" | Accepted |

Related spec text

**36.3.4 EHT PPDU formats**

**…**



