IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 802.11bh – CID 32 | | | | |
| Date: September 13, 2022 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Antonio de la Oliva | Interdigital Ltd, UC3M |  |  | aoliva@it.uc3m.es |
| Joseph Levy | Interdigital Ltd, |  |  |  |

Abstract

This submission tackles comment 32 of the IEEE 802.11bh/D0.2 resolution.

The comment text is the following:

* Which is correct description for Device ID? In Section6, it says, "Specifies the Device ID for the requesting STA. Optionally present if Device ID is supported, otherwise not present." but, In section 9, it says, "The Device ID element is optionally present when using FILS authentication; otherwise, it is not present" Is it equal "Device ID is supported" and "using FILS authentication"?

The resolutions should be:

* Revise. The description of the DeviceID MLME-SAP has been updated to indicate the Device ID is only included if supported and using FILS.

Proposed contribution

Editor please change the description of Device ID in the parameter description tables for clauses 6.3.7.2.2, 6.3.7.3.2, 6.3.7.4.2, 6.3.7.5.2 of IEEE 802.11bh/D0.2 as follows:

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Type | Valid Range | Description |
| Device ID | Device ID element | As defined in 9.4.2.296a (Device ID element) | Specifies the Device ID for the requesting STA. Optionally present if dot11FILSActivated is true and Device ID is supported, otherwise not present." |