IEEE P802.11
Wireless LANs

|  |
| --- |
| LB271 CID 17146 |
| Date: 2023-04-24 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Sigurd Schelstraete | MaxLinear |  |  | sschelstraete@maxlinear.com |
|  |  |  |  |  |

Abstract

This submission proposes a resolution for CID 17146.

# CIDs

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Must Be Satisfied** | **Clause** | **Page** | **Comment** | **Proposed Change** | **Resolution** |
| 17146 | Yes | B.4.40.1 | 933.28 | MRU is used in numerous instances, whereas M-RU is used only three instances. | Change instances of M-RU to MRU. | REVISEDChange “M-RU” to “MRU” in the following places:D3.0, P275L56D3.0, P284L25D3.0, P933L28NOTE: this resolution is covered by the proposed resolution of CIDs 17144 and 17145 in 11-23/0682r1 |

# Discussion

Although the comment is made on Annex B, the use of “M-RU” is found in three places in the draft D3.0:

On page 275, Line 56:



On Page 284, Line 25:



On Page 933, Line 28



Commenter is correct that the preferred term is “MRU” instead of “M-RU”.

The proposed resolution changes all occurrences of “M-RU” to “MRU”.