IEEE P802.11
Wireless LANs

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |
| --- |
| LB 272 CR for CID 2241 |
| Date: 2023-07-06 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Mahmoud Kamel | InterDigital |  |  | mahmoud.kamel@interdigital.com |
| Zinan Lin | InterDigital |  |  |  |
| Rui Yang | InterDigital |  |  |  |
| Claudio Da Silva | Meta |  |  | claudiodasilva@meta.com |
| Ali Raissinia | Qualcomm |  |  | alirezar@qti.qualcomm.com |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

 |

Abstract

This submission proposes resolutions for CID 2241 in subclause 11.55.1.4 in P802.11bf D1.0:

NOTE – Set the Track Changes Viewing Option in the MS Word to “All Markup” to clearly see the proposed text edits.

**Revision History:**

R0: Initial version

##  CID: 2241

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page.Line** | **Comment** | **Proposed Change** | **Resolution** |
| 2241 | 11.55.1.4 | 173.31 | It is better to have a separate subclause to talk about the sensing measurement set up with an unassociated non-AP STA | Add a separate subclause related to unassociated non-AP STA sensing measurement setup | **Revised**Agree in principle with the comment. Reorganization of the text is shown belowTGbf editor: please incorporate changes shown in 11-23/1157r3 below. |

***TGbf Editor: Please create a new subclause 11.55.1.4.1 Genaral in D1.2***

***TGbf Editor: Please create a new subclause 11.55.1.4.2 in D1.2 and insert the following paragraph under this subclause***

**11.55.1.4.2 Sensing Measurement Session for Unassociated STA**

If an unassociated non-AP STA intends to establish a sensing measurement session for a non-TB sensing measurement exchange, it shall transmit a Sensing Measurement Request frame to the AP and include a non-TB Specific subelement to set the parameters of the sensing measurement session.

***TGbf Editor: Please move the paragraph in P133L63 to P134L7 in D1.2 under the newly created subclause after the paragraph above.***

***TGbf Editor: Please move the paragraph in P134L9 to P134L19 in D1.2 under the newly created subclause after the paragraph above.***

***TGbf Editor: Please move the paragraph in P134L21 to P134L24 in D1.2 under the newly created subclause after the paragraph above.***

***TGbf Editor: Please move the paragraph in P134L26 to P134L30 in D1.2 under the newly created subclause after the paragraph above.***