IEEE P802.11
Wireless LANs

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

|  |
| --- |
| LB 272 CR for CIDs (1574, 1953) |
| Date: 2023-07-06 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Mahmoud Kamel | InterDigital |  |  | mahmoud.kamel@interdigital.com |
| Rui Yang |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

 |

Abstract

This submission proposes resolutions for 2 CIDs (1574, 1953) in subclause 11.55.1.4 in P802.11bf D1.0:

NOTE – Set the Track Changes Viewing Option in the MS Word to “All Markup” to clearly see the proposed text edits.

**Revision History:**

R0: Initial version

R1: The resolutions of the two CIDs are updated

##  CIDs: 1574, 1953

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page.Line** | **Comment** | **Proposed Change** | **Resolution** |
| 1574 | 11.55.1.4 | 172.54 | It is not clear how an unassociated non-AP STA can initiate a non-TB sensing measurement setup with an AP. | State explicitly the procedure by which an unassociated non-AP STA can initiate a non-TB sensing measurement setup with an AP. | **Reject**The procedure by which a non-AP STA (whether associated or unassociated) initiates a sensing measurement session already exists in D1.2 P135L53. |
| 1953 | 11.55.1.4 | 173.31 | There is description of how a non-AP STA may act as an unassociated responder, however there is no description of how a non-AP STA may act as an initiator with an unassociated AP as a responder. This will only be applicable for the non-TB measurement instance, and should be stated. | Insert the text following paragraph into section 11.55.1.4:"If an unassociated non-AP STA intends to act as a sensing initiator, it shall transmit a Sensing Measurement Setup Request frame to an AP STA of which the sensing capabilities are known, and include a non-TB Sensing Specific subelement in the Sensing Measurement Parameters element." | **Reject**The procedure by which a non-AP STA (whether associated or unassociated) initiates a sensing measurement session already exists in D1.2 P135L53. |