IEEE P802.11
Wireless LANs

|  |
| --- |
| LB272 comments SBP comments resolution Part 2 |
| Date: 2023.06.xx |
| Author(s): |
| Name | Company | Address | Phone | email |
| Rui Du | Huawei Technologies | F3, Huawei Base, Shenzhen, Guangdong, China, 518129 |  | Ray.du@huawei.com |
| Narengerile |  |  |
| Mengshi Hu |  |  |
| Zhuqing Tang |  |  |
| Yiyan Zhang |  |  |

Abstract

This submission contains the proposed comment resolutions for the CIDs 2072.

R0: initial document

# CID 1044

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Page.Line | Clause Number | Comment | Proposed Change | Resolution |
| 1044 | 191.45 | 11.55.2.2 | After receiving an SBP Response frame, with Status-Code parameter equal to REQUEST\_DECLINED or REJECTED\_WITH\_SUGGESTED\_CHANGES, the SBP procedure setup is defined to be unsuccessful. Then, why do we need the status code "REJECTED\_WITH\_SUGGESTED\_CHANGES" if there is no difference of the handling and result from a simple "REQUEST\_DECLINED"? | Either delete the Status-Code "REJECTED\_WITH\_SUGGESTED\_CHANGES" and related text or specify how it is used to differentiate from "REQUEST\_DECLINED". | RejectedAfter reciving a SBP response frame with Status Code other than SUCCESS, the setup of current SBP procedure is finished and it is regarded as unsuccessful.Status Code REQUEST\_DECLINED and REJECTED WITH SUGGESTED CHANGES provide different information for next round SBP procedure setup. |

# CID 1052

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Page.Line | Clause Number | Comment | Proposed Change | Resolution |
| 1052 | 217.05 | 11.55.4.2 | In DMG SBP setup procedure, after receiving an SBP Response frame, with Status-Code parameter equal to REQUEST\_DECLINED or REJECTED\_WITH\_SUGGESTED\_CHANGES, the DMG SBP procedure setup is defined to be unsuccessful. Then, why do we need the status code "REJECTED\_WITH\_SUGGESTED\_CHANGES" if there is no difference of the handling and result from a simple "REQUEST\_DECLINED"? | Either delete the Status-Code "REJECTED\_WITH\_SUGGESTED\_CHANGES" and related text or specify how it is used to differentiate from "REQUEST\_DECLINED". | RejectedAfter reciving a DMG SBP response frame with Status Code other than SUCCESS, the setup of current DMG SBP procedure is finished and it is regarded as unsuccessful.Status Code REQUEST\_DECLINED and REJECTED WITH SUGGESTED CHANGES provide different information for next round DMG SBP procedure setup. |

# SP

Do you support resolutions to the following CIDs and incorporate the text changes into the latest TGbf draft: 1044 and 1052 in 11-23/1203r0?

Y/N/A