IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 802.11bh D1.0 Comment Resolutions Section 12.7 | | | | |
| Date: 2023-07-12 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Kurt Lumbatis | ZaiNar | Dacula, GA USA | +17708289420 | Kurt.lumbatis@zainartech.com |
|  |  |  |  |  |

Abstract

This submission proposes resolutions to the following CIDs.

8, 9, 10, 11, 36, 236

Revisions:

* Rev 0 – Initial version of the document.
* Rev 1 – Correct a line number.
* Rev 2 – Remove CRs for 6, 37 & 207. Handled in other submissions. Add CRs 8, 9, 10

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in IEEE P802.11bh D1.0. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the IEEE P802.11bh D1.0. (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbh Editor: Editing instructions preceded by “TGbh Editor” are instructions to the TGbh editor to modify existing material in the TGbh draft. As a result of adopting the changes, the TGbh editor will execute the instructions rather than copy them to the TGbh Draft.***

| **CID** | **Commenter** | **Comment** | **Proposed Change** | **Resolution** |
| --- | --- | --- | --- | --- |
| 8 | Rojan Chitrakar | "The Device ID field contains a device ID or an opaque identifier (see Annex AD.1)." What's the format of device ID? If it can be either device ID or opaque identifier, how does the receiving STA differentiate the format? Furthermore, Annex AD is informative; is support for opaque id meant to be mandatory? | Clarify the format of device ID. Also specify whether support for opaque identifier is mandatory or optional. | Revised:  **TGbh Editor:** Modify 27.31 replacing ""variable"" with "0 - 64"  **TGbh Editor:** Replace 27.61 with the following:  "The Device ID field contains a device ID. The length of the device ID is between 0 and 64 octets. The device ID may be constructed as an opaque identifier (see Annex AD.1)." |
| 9 | Chaoming Luo | The sentence is confusing. Is an opaque identifier not a device ID? | Change to: The Device ID field contains a device ID. A device ID can be constructed as an opaque identifier (see Annex AD.1). |
| 10 | Chaoming Luo | The sentence is confusing. Is an opaque identifier not a device ID? | Change to: The Device ID field contains a device ID provided by an AP in the ESS. A device ID can be constructed as an opaque identifier (see AnnexAD.1) | Revised:  **TGbh Editor:** Replace 34.12 with the following:  "The Device ID field contains a device ID as defined in 9.4.2.307a. (Device ID element)." |
| 36 | Stephan Sand | In order to avoid duplicate sepc text remove the seentence | As in comment |
| 272 | Mark Hamilton | To be consistent with 9.4.2.307a, and changes Accepted in 11-22/1082r4, don't specify that the Device ID must be from an AP in an ESS. | Delete "provided by an AP in the ESS" |
| 11 | Chaoming Luo | The sentence is confusing. Is an opaque identifier not a device ID? | Change to: Device ID KDE is a KDE containing a device ID provided by an AP in the ESS. | Revised:  **TGbh Editor:** Replace 34.61 with the following:  Device ID KDE is a KDE containing a device ID as defined in 9.4.2.307a. |

**References:**