IEEE P802.11
Wireless LANs

|  |
| --- |
| LB276 CR for OST CIDs (11.5.1 Sensing Procedure) |
| Date: 2023-09-06 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Stephan Sand | German Aerospace Center (DLR) |  |  | stephan.sand@ieee.org |
|  |  |  |  |  |

Abstract

This submission discusses resolutions to the following 9 CIDs from LB276 of TGbf D2.0.

The CID list is:

3035, 3036, 3072, 3091, 3095, 3250, 3476, 3482, 3483

Proposed changes in this document are with reference to TGbf D2.0.

Revisions:

* Rev 0: Intitial version of the document

Proposed comment resolution

Presented and discussed, no open discussion points

Under discussion

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Cat** | **Page** | **Comment** | **Proposed Change** | **Resolution** |
| 3476 | E | 135.43 | Grammer | Change "... in the range of 0 to 62" to "... in the range from 0 to 62" | Accepted |
| 3035 | E | 135.46 | 95 percent -> 95% | As in comment | Accepted |
| 3036 | E | 137.21 | "Upon receiving" is not accurate. The receiving operation is spread over a fairly long time; the on-air duration of the frame. Also, incorrect use of "set to" (this is a tested condition). And missing article. | Change to "On receipt of a Probe Response frame with the Responder Needed field equal to 1,..." | Accepted |
| 3091 | G | 137.31 | Change "If a non-AP STA is not associated with an AP and intends to establish a sensing measurement session that is initiated by the AP" to "If an unassociated non-AP STA intends to establish a sensing measurement session that is initiated by an AP". | As in comment. | Accepted |
| 3072 | E | 138.11 | what is 'attempt to' means here? | Remove 'attempt to'. also in P138L15 | Accepted |
| 3095 | G | 138.23 | Change "The frame is sent by an AP and is addressed to a non-AP STA that is associated with this AP" to "The frame is sent by an AP and is addressed to a associated non-AP STA". | As in comment. | Revised**TGbf Editor:**Please change "The frame is sent by an AP and is addressed to a non-AP STA that is associated with this AP" to "The frame is sent by an AP and is addressed to an associated non-AP STA". |
| 3482 | E | 138.26 | Grammer, need to rephrase the sentence "The Comeback field of the Sensing Comeback Info field within the Sensing Measurement Request frame shall be set to 0 if the frame is sent by an AP, it is addressed to an unassociated non-AP STA". This contain two separate sentences. | As in comment. | RejectedThe comment does not consider the full sentence, which ends at L29 and is grammatically correct. |
| 3483 | E | 138.31 | Grammer, need to rephrase the sentence "The Comeback field of the Sensing Comeback Info field within the Sensing Measurement Request frame shall be set to 1 if the frame is sent by an AP, it is addressed to an unassociated non-AP STA". This contain two separate sentences. | As in comment. | RejectedThe comment does not consider the full sentence, which ends at L35 and is grammatically correct. |
| 3250 | E | 138.26 | Add NDP after SI2SI and after SR2SI | Change to "Upon receiving an SI2SR NDP, SR2SI NDP, or SR2SR NDP, | RevisedAgree with comment but the correct P.L is 143.26 |

# Straw Poll

Do you support the resolution of the following 9 CIDs and instruct TGbf editor to incorporate the changes into the latest TGbf draft: 3035, 3036, 3072, 3091, 3095, 3250, 3476, 3482, 3483?

Y/N/A