IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 11be lb275 CR for Clause 36.3.11 Mathematical description of signals | | | | |
| Date: 2023-09-12 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | Email |
| Yan Zhang | Apple |  |  | [yan\_zhang1010@apple.com](mailto:yan_zhang1010@apple.com) |

Abstract: This document contains proposed resolutions for comments in *Clauses 36.3.11* from 11be D4.0 with 2 CIDs below.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| ***Clause 36.3.11***  19009,19179 | | | |  | | |
|  | | | | | |  |
|  | | | | | |  |
|  | | | |  | | |
| 19009 | 36.3.11.4 | | 748.50 | "For EHT modulated fields in a nonpunctured non-OFDMA EHT PPDU that is  not in EHT DUP mode, is the set of subcarriers indices from to as defined in  Table 36-19 (Subcarrier allocation related constants for the EHT-modulated fields in a  nonpunctured non-OFDMA EHT PPDU) excluding DC subcarriers. " DC in table 36-19 doesn't includes null tones. the description is not correct for BW > 80MHz. especially for EHT-LTF. | change to ....excluding DC and null subcarriers. Or update table 36-19 to reflect DC and Nulls for BW>80 | | **Revised.**  Agree with the commentor that there are null tones besides the null tones at DC for BW > 80 MHz which are not modulated.  TGbe editor: Incorporate the changes in <https://mentor.ieee.org/802.11/dcn/23/11-23-1597-01-00be-11be-lb275-CR-for-Clause-36-3-11-mathematical-description-of-signals.docx> | | |

be editor: please make the following changes in D4.0 *Clause 36.3.11.4*:

* On P748L48 (CID #19009):

For EHT modulated fields in a nonpunctured non-OFDMA EHT PPDU that is not in EHT DUP mode, is the set of subcarriers indices from to excluding DC subcarriers as defined in Table 36-19 (Subcarrier allocation related constants for the EHT-modulated fields in a nonpunctured non-OFDMA EHT PPDU) and Null subcarriers as defined in Table 36-16 (Null subcarrier indices for 80 MHz, 160 MHz, and 320 MHz) if present.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 19179 | 36.3.11.4 | 750.30 | The power is scaled to ensure average power (or per tone energy) for  EHT-LTF and Data fields are the same (per tone power are not the same) | Change the text to "to ensure the field average power are the same for both EHT-LTF and Data fields" | **Rejected.**  This is to ensure per tone power are the same for EHT-LTF and data fields at receiver after FFT operation since 1x and 2x EHT-LTF are truncated to ¼ and ½ of data OFDM symbol time. |