IEEE P802.11
Wireless LANs

|  |
| --- |
| LB276 comment resolutions for measurement exchange  |
| Date: 2023.10.26 |
| Author(s): |
| Name | Company | Address | Phone | email |
| Zhuqing Tang | Huawei Technologies | Huawei Base, Shenzhen, Guangdong, China, 518129 |  | tangzhuqing@huawei.com |
| Rui Du |  |  |
| Narengerile |  |  |
| Mengshi Hu |  |  |
| Yiyan Zhang |  |  |

Abstract

This submission proposes resolutions to the following comments submitted in LB276 under measurement exchange topic.

CIDs: 3085, 3100 and 3316

Revision history:

R0: Original version

R1: Minor changes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Comment** | **Proposed change** | **Proposed resolution** |
| 3085 | 11.55.1.5.2.1 | 144.35 | It is not always possible to place all TB sensing measurement exchanges within a single sensing availability window. | Replace "All" by "Every" | RevisedTGbf Editor make changes specified in 1670r1.([https://mentor.ieee.org/802.11/dcn/23/11-23-1670-01-00bf-lb276-comment resolutions-for-measurement-exchange.docx](https://mentor.ieee.org/802.11/dcn/23/11-23-1670-01-00bf-lb276-comment%20resolutions-for-measurement-exchange.docx)) |
| 3100 | 11.55.1.5.2.1 | 144.35 | It is not always possible to place all TB sensing measurement exchanges within a single sensing availability window. | Replace "All" by "Every" | RevisedTGbf Editor make changes specified in 1670r1.([https://mentor.ieee.org/802.11/dcn/23/11-23-1670-01-00bf-lb276-comment resolutions-for-measurement- exchange.docx](https://mentor.ieee.org/802.11/dcn/23/11-23-1670-01-00bf-lb276-comment%20resolutions-for-measurement-%20exchange.docx)) |
| 3316 | 11.55.1.5.2.1 | 144.35 | "All TB sensing measurement exchanges shall take place within a sensing availability window." may mislead to all TB exchanges of a MS shall be within the same AVW (a huge AVW). | Change to: A TB sensing measurement exchange shall takeplace within a sensing availability window. | ~~Accepted~~RevisedTGbf Editor make changes specified in 1670r1.([https://mentor.ieee.org/802.11/dcn/23/11-23-1670-01-00bf-lb276-comment resolutions-for-measurement- exchange.docx](https://mentor.ieee.org/802.11/dcn/23/11-23-1670-01-00bf-lb276-comment%20resolutions-for-measurement-%20exchange.docx)) |

**Discussion:**

In the text, the sentence “***All*** *TB sensing measurement exchanges shall take place within a sensing availability window.*” is confusing which makes people think that all TB sensing measurement exchanges shall take place within one availability window. Replacing “all” by “every” is also confusing. Thus, we can use a general expression to rephrase this sentence:

**Resolution:**

***Instructions to the editor: please add the following sentence in red in P144L52 in the subclause 11.55.1.5.2.1 in D2.1 as shown below:***

 ~~All~~ The TB sensing measurement exchanges shall take place within a sensing availability window.

## SP

Do you support the proposed resolutions to the CIDs 3085, 3100 and 3316 and incorporate the text changes into the latest TGbf draft?

Y~~/N/A~~