IEEE P802.11  
Wireless LANs

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | LB 275 CR for CID 19545 on NDPA frame format | | | | | | Date: 2023-10-10 | | | | | | Author(s): | | | | | | Name | Affiliation | Address | Phone | email | | Mahmoud Kamel | InterDigital |  |  | mahmoud.kamel@interdigital.com | |  |  |  |  |  | |  |  |  |  |  | |  |  |  |  |  | |  |  |  |  |  | |  |  |  |  |  | |  |  |  |  |  | |  |  |  |  |  | |

Abstract

This submission proposes resolutions for CID 19545 in subclause 9.3.1.19 in P802.11be D4.0:

NOTE – Set the Track Changes Viewing Option in the MS Word to “All Markup” to clearly see the proposed text edits.

**Revision History:**

R0: Initial version

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page.Line** | **Comment** | **Proposed Change** | **Resolution** |
| 19545 | 9.3.1.19.3 | 0.00 | The proposed changes to Disabled from Disallowed (2 places) aren't consistent with Figure 9-75i (which still uses Disallowed) |  | **Reject**  In 11be D 4.1, the term *Disabled Subchannel Bitmap* is adopted and used in 62 occurrences with reference to this concept. In the two occurrences spotted by this comment, the term *Disallowed Subchannel Bitmap* is used in reference to the usage of this term in HE (see Table 9-42a and Figure 9-75i).  In fact, the term *Disallowed Subchannel Bitmap* is the term adopted in both 11ax-2021 (26 times) and in REVme D4.0.  Accordingly, this comment should be better submitted to and addressed in REVme.  TGbe editor: No further changes are required |