IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| LB276 CR for CID 3178 | | | | |
| Date: 2023-11-14 | | | | |
| Author(s): | | | | |
| Name | Company | Address | Phone | email |
| Dong Wei | NXP |  |  | dong.wei@nxp.com |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This document aims to resolve the following LB276 comment: CID 3178.

R0: Initial version

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Comment** | **Proposed Change** | **Resolution** |
| 3178 | 11.55.1.5.2.5 | 152.11 | Add new normative text in P152 after L11 to include transmissions of MSID and MEID | The corresponding text can be as follows or its equivalent  When transmitting an SR2SR Sounding Trigger frame as part of the TB sensing measurement exchange, an AP shall include the corresponding Measurement Session ID and the Measurement Exchange ID fields in the Trigger Dependent Common Info field. The AP maintains a modulo 64 counter for each TB sensing measurement exchange corresponding to a Measurement Session ID. When transmitting a SR2SR Sounding Trigger frame to one or more non-AP STAs, the Measurement Exchange ID shall be the value of this modulo 64 counter; after which the counter shall be incremented by 1. | Revised  Incorporate the changes in <https://mentor.ieee.org/802.11/dcn/23/11-23-2096-00-00bf-LB276-CR-for-CID-3178.docx> |

**Discussion:**

We agree with the commenter in principle.

*TGbf Editor: Please insert the following paragraph to the end of Clause 11.55.1.5.2.5 (TF sounding phase - SR2SR variant) of D2.0.*

When transmitting an SR2SR Sounding Trigger frame as part of the TB sensing measurement exchange, an AP shall include the corresponding Measurement Session ID and the Measurement Exchange ID fields in the Trigger Dependent Common Info field. The AP shall maintain a modulo 64 counter for each TB sensing measurement exchange corresponding to a Measurement Session ID. When transmitting a SR2SR Sounding Trigger frame to one or more non-AP STAs, the Measurement Exchange ID shall be the value of this modulo 64 counter; after which the counter shall be incremented by 1.

**SP:** Do you agree to the resolution provided in the document 11-23/2096r0for CID 3178?