IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| CR for CID 6006 | | | | |
| Date: 2024-1-9 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Xiaofei Wang | InterDigital Inc. | 111 West 33rd Street  Suite 1420  New York, NY, USA | +1-607-592-2727 | Xiaofei.wang@interdigital.com |
| Hanqing Lou |  |  |
| Rui Yang |  |  |

Abstract

This submission proposes resolutions for the CID 6006.The baseline for this comment resolution document is 802.11 RevME Draft 1.2.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Line** | **Comment** | **Proposed Change** | **Resolution** |
| 6006 | 26.7.4 | 3912 | 35 | The text is unclear how MU feedback should be segmented. For example, in each segment, does HE Compressed Beamforming/CQI frame need to include both HE Compressed Beamforming Report and HE MU Exclusive Beamforming Report? Or it may include HE Compressed Beamforming Report and/or HE MU Exclusive Beamforming Report? In other words, some HE Compressed Beamforming/CQI frame may include HE Compressed Beamforming Report only or HE MU Exclusive Beamforming Report only? This issue needs to be clarified since subsequent standards such as 11be are using the style 11ax as reference and may cause more confusions. | Please clarify how the segmentation is performed for SU feedback and MU feedback, e.g., adding the following sentences before the last sentence of the first paragraph of Subclause 26.7.4: If the Feedback Type subfield in the EHT MIMO Control field indicates SU, each feedback segment carried in an HE Compressed Beamforming/CQI frame may contain the HE compressed report information only; if the Feedback Type subfield in the HE MIMO Control field indicates MU, each feedback segment carried in an HE Compressed Beamforming/CQI frame may contain the HE compressed report information, and/or the HE MU exclusive beamforming report information. Plan to submit a contribution. | Revised: agree with the comment. Add the following sentences before the last sentence of the first paragraph of Subclause 26.7.4: “If the Feedback Type subfield in the EHT MIMO Control field indicates SU, each feedback segment carried in an HE Compressed Beamforming/CQI frame may contain the HE compressed report information only; if the Feedback Type subfield in the HE MIMO Control field indicates MU, each feedback segment carried in an HE Compressed Beamforming/CQI frame may contain the HE compressed report information, and/or the HE MU exclusive beamforming report information.” |