|  |
| --- |
| CR for CIDs in subclause 9.4 |
| Date: 2024-1-10 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Jay Yang | ZTE Corporation |  |  | Yang.zhijie@zte.com.cn |
| Yan Li | ZTE Corporation |  |  |  |
|  |  |  |  |  |

Abstract

This submission proposes resolutions for the following CIDs:

R0: initial the draft

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbh D2.0 Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbh D2.0 Draft. (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbh Editor: Editing instructions preceded by “TGbh Editor” are instructions to the TGbh editor to modify existing material in the TGbh draft. As a result of adopting the changes, the TGbh editor will execute the instructions rather than copy them to the TGbh Draft.***

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **CID** | **Page/Line** | **Comment** | **Proposed Change** | **Resolution** |
| 92 | 24/41 | Making the Device ID element non-extensible seems short-sighted to me | Change "No" in the penultimate column to "Yes" and add a Device ID Length field before the Device ID field in Figure 9-1054a--Device ID element format | **Note: the resolution is under the table** |
| 100 | 25/31 | "The measurement ID in measurement ID element exchanged between an AP in an ESS and a STA in a radio measurement procedure is a one time measurement ID assigned by AP. The measurement ID is different each time, and both the AP and the STA should drop it immediately after each radio measurement session." is behaviour (not very clear) | Move to Clause 11 and clarify | **Note: the resolution is under the table** |
| 4 | 25/28 | It's not clear how does the measurement ID help the using of RCM. The current spec text does not reveal it. | Remove the measurement ID from the specification. Or add text to address the issue. | **Revised--**Add more text to clarify it, the resolution is same as CID100 |
| 24 | 25/34 | "measurement ID assigned by AP" should be "measurement ID assigned by the associated AP" | change to "measurement ID assigned by the associated AP" | **Revised--**the resolution is same as CID100 |
| 203 | 25/35 | "both the Ap and the STA should dropt it immediately after each radio measurement session": no idea what 'drop' means in this context. If it is an action internal to the AP or the STA, this can't be measured anyway, so what is the point of asking for it? | Replace "The measurement ID is different each time, and both the AP and the STA should drop it immediately after each radio measurement session" with "the AP and the STA should refrain from reusing the same Measurement ID for another measurement exchange (possibly 'between the same AP and STA pair'))". | **Revised--** the resolution is same as CID100 |
| 217 | 25/35 | The sentence "When the Measurement ID subelement is present in a Beacon request, it indicates the requesting STA asks the responding STA to include the Measurement ID element in the Probe Request frame" is not clear, should the responding STA includes the same content? Consider revision, e.g: "When included in a Beacon request, it indicates the requesting STA asks the responding STA to include the provided Measurement ID element in its Probe Request frame". | As in comment | **Accepted--** |
| 97 | 25/37 | Can't have a shall in a NOTE (or in C9 either) | Replace the NOTE with "A Beacon request does not contain both an IRM Recommendation subelement and a Measurement ID subelement." | **Accepted--** |
| 18 | 25/37 | A normative text should not be in a note. | Change the note to a body text. | **Revised--**The resolution is same to CID97 |
| 249 | 25/37 | The Note contains normative mandatory behavior language "shall". Either eliminate the NOTE category and make the text in the NOTE as part of the last paragraph or change the text to informative behavior by removing the "shall" requirement as shown in the proposed change. | change "shall be not present" to " is not allowed" | **Revised--**The resolution is same to CID97 |
| 101 | 26/22 | "of the Device ID element" -- no need to state since we're in that very subclause | Delete the cited text | **Accepted--** |
| 103 | 26/26 | What if it's from PCP to non-AP STA? | Change "an AP" to "an AP or PCP" and in the table change "AP" to "AP/PCP" | **Rejected--**Not sure the non-AP STA use RCM in PBSS, and encounter the similar identification issue.The commenter fails to identify any identification issue with RCM in PBSS. |
| 105 | 26/44 | "The Device ID field contains a device ID." -- not clear what a "device ID" is | Add a definition | **Rejected--**Device ID definition is in subclause 3.2 |
| 110 | 27/44 | It is completely unclear what a "measurement ID" is, and even the name isn't clear | Add a definition | **Note: the resolution is under the table** |

**CID 92**

**Revised--**

**Agree in principle.**

**TGbh editor： Change "No" in the Extensible column to "Yes" in L24P41**

**TGbh editor： replace Figure 9-1054a—Device ID element format with the following:**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Element ID | Length | Element ID Extension | Device ID Length | Device ID Status | Device ID |

Octets: 1 1 1 1 1 variable

**CID 100**

**Revised--**

**Agree in principle.**

**TGbh editor： Please delete the following sentences in L31P25**

**“**The measurement ID in measurement ID element exchanged between an AP in an ESS and a STA in a radio measurement procedure is a one time measurement ID assigned by AP. The measurement ID is different each time, and both the AP and the STA should drop it immediately after each radio measurement session.**”**

**TGbh editor： Please insert the following sentences in subclause 11.10.9.1 Beacon report**

**....**

If the BSSID field in the Measurement Request contains a wildcard BSSID, all observed BSSs with the

requested SSID shall be reported in a separate Beacon report for each BSSID. If the SSID subelement is not

included in the Beacon request, all observed BSSs shall be reported in a separate Beacon report for each

BSSID. In active mode, Probe Response frames shall be evaluated regardless of whether the Probe Response

frame was triggered by the measuring STA’s Probe Request.

If dot11RMBeaconActiveMeasurementActivated is true and dot11DeviceIDActivated is true, the measurement mode in the measurement request is Active, the Beacon request may include a measurement ID subelement containing a measurement ID,which is as an identifier and is copied into Measurement ID field in Measurement ID element(see 9.4.2.313) in the measuring STA’s Probe Request. To enhance the privacy, the AP and the measuring STA should refrain from reusing the same Measurement ID for another measurement exchange (possibly 'between the same AP and measuring STA pair')

On accepting an active or passive mode Beacon request, a STA shall conduct measurements as follows:

**....**

**CID 110**

**Revised--**

**TGbh editor： Insert the following paragraph in subcluase 3.2**

**Measurement ID:** a transient device ID that a network can provide to a non-access-point (AP) station(STA) to allow the non-AP STA to identify itself to another AP in the same network during radio measurement procedure.