IEEE P802.11
Wireless LANs

|  |
| --- |
| Initial SA Resolution for CIDs related to R-TWT |
| Date: April 2, 2024 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| George Cherian | Qualcomm Technologies Inc. |  |  | gcherian at qti.qualcomm.com |

 Abstract

This submission proposes resolutions for following CID received for TGbe initial SA ballot:

* 22411

**Revisions:**

* Rev 0: Initial version of the document.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe Draft (i.e., they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Clause** | **Page** | **Comment** | **Proposed Change** | **Resolution** |
| 22411 | Chaoming Luo | 23 | 252.09 | According to clause 35.3.16.5.2 "An AP affiliated with an AP MLD shall not transmit a PPDU carrying an MPDU with SRS Control subfield to a non-AP STA affiliated with a non-AP MLD.", an non-AP STA would never receive a frame with an SRS Control subfield, so the capability of "support for the reception of a frame that carries an SRS Control subfield" for a non-AP does not mean much. | Either change the meaning of "SRS Support" for non-AP; Or make the field reserved for non-AP. | Revised –Agree in principle with the comment’ interpretation of that rule. However, as described in 35.4.20.1 an NSTR mobile AP MLD can transmit an SRS Control field to a STA that has indicated support of reception of SRS Control field. Hence the capability definition is correct, however the rule in 35.3.16.5.2 is missing the exception that points to 35.4.20.1. Proposed resolution adds such exception.TGbe Editor: please implement changes as shown in 11-24/0338r1 under all headings that include CID 22411. |

1. **Proposed Text:**

**35.3.16.5.2 End time alignment of response PPDUs using SRS Control subfield**

**TGbe Editor: *Please change the paragraphs of the subclause below (#CID 22411):***

An AP affiliated with an AP MLD shall not transmit a PPDU carrying an MPDU with SRS Control subfield to a non-AP STA affiliated with a non-AP MLD unless the AP MLD is an NSTR mobile AP MLD, in which case the AP MLD shall follow the rules in 35.3.19 (NSTR mobile AP MLD operation)*(#22411)*..

NOTE 1—If the received SRS Support subfield from an AP is equal to 0, a non-AP STA might not be able to perform multiple frame transmission in a TXOP over NSTR link pair(s) with the AP, unless the expected duration of solicited PPDU transmitted on NSTR link pair(s) are the same.