IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| CR for CID 23173 | | | | |
| Date: 2024-06-28 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Xiaofei Wang | InterDigital Inc. | 111 West 33rd Street  Suite 1420  New York, NY, USA | +1-607-592-2727 | Xiaofei.wang@interdigital.com |
| Rui Yang |  |  |
| Hanqing Lou |  |  |  |  |

Abstract

This submission proposes resolutions for CID 23173.

The baseline for this comment resolution document is 802.11be Draft 6.0.

R0: first draft

R1: minor editorial changes

R2: additional changes after Mark Hamilton found more issues with the definition

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Clause** | **Page** | **Comment** | **Proposed Change** | **Resolution** |
| 23173 | Xiaofei Wang | 3.1 | 55.34 | the bold part says "extended service set", while in square bracket it says "ESS transition", it needs to be made uniform. | add transition after "extended service set". | Revised: made the requested change with the necessary formatting.  802.11be Editor: please incorporate the changes as shown in 11-24/1007r2. |

***TGbe Editor: Please modify Subclause 3.1 (802.11be D6.0) as follows:***

**extended service set transition**: [ESS transition] Change of association by a station (STA) or a non-access point (non-AP) multi-link device (non-AP MLD) from one basic service set (BSS) or access point (AP) MLD (AP MLD) in one ESS to another BSS or AP MLD in a different ESS.