IEEE P802.11
Wireless LANs

|  |
| --- |
| Proposed resolution for miscellaneous comments on recirculation SA ballot on D6.0 |
| Date: 2024-06-26 |
| Author: |
| Name | Affiliation | Address | Phone | Email |
| Edward Au | Huawei Technologies | Ottawa, Ontario, Canada |  | edward.ks.au@gmail.com  |

#####

##### This submission present proposed resolutions for the following CID:

23141, 23142, 23176

##### The proposed changes are based on P802.11be D6.0.

##### Revision history:

##### R0 – Initial version

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Clause | Page | Line | Comment | Proposed Change |
| 23141 | 1.5 | 51 | 28 | Is this new max() function different from the MAX() function used in the base standard? Probably not. | change to max() or MAX() consistently throughout |
| 23142 | 1.5 | 51 | 26 | the minimum function min() as defined in clause 1.5 is lowercase; Is this different than the MIN() function already used in the standard? Probably not. | Change to min() or MIN() consistently throughout |

***Discussion:***

The uses of max(,) versus MAX(,) and min(,) versus MIN(,) are inconsistent in the baseline (c.f., REVme D6.0). The definitions of max(,) [or MAX(,)] and min(,) [or MIN(,)] are also missing in the baseline. By adopting the definitions of max(,) and min(,), the use of the functions are at least consistent in the P802.11be draft.

***Proposed resolution for CID 23141:***

Rejected.

This new max(,) function in Clause 1.5 is no different from the MAX() function used in the base standard. However, the baseline does not define the MAX(,) function and both the max(,) and the MAX(,) are used interchangeably.

By adopting this max(,) function, its use is at least consistent in the P802.11be draft.

***Proposed resolution for CID 23142:***

Rejected.

This new min(,) function in Clause 1.5 is no different from the MIN() function used in the base standard. However, the baseline does not define the MIN(,) function and both the min(,) and the MIN(,) are used interchangeably.

By adopting this min(,) function, its use is at least consistent in the P802.11be draft.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Clause | Page | Line | Comment | Proposed Change |
| 23176 | 12.11.2.3.5 | 454 | 24 | "bythe" should be "by the". | Put a space between "by" and "the". |

***Discussion:***

The commenter is correct that “bythe” should be “by the”.



***Proposed resolution for CID 23176:***

Accepted.