IEEE P802.11
Wireless LANs

|  |
| --- |
| SA1 comment resolution for OSC category |
| Date: 2024-06-20 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Ali Raissinia | Qualcomm Inc. |  |  | alirezar@qti.qualcomm.com |
|  |  |  |  |  |

Abstract

Comment resolution for CIDs 6026 and 6034 (total of 2 CIDs).

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Comment** | **Proposed Change** | **Resolution** |
| 6026 | 11.55.1.2 | 139.03 | Successfully set up is not well defined, and inconsistent with previous paragraphs and base standard. | Change has not successfully set up a PTKSA to has not established a PTKSA. |  Revise<https://mentor.ieee.org/802.11/dcn/24/11-24-1050-00-00bf-SA1-comment-resolution-for-OSC-category.docx> |
| 6034 | 11.55.1.2 | 138.58 | Specify how the PTKSA is to be established | Change an unassociated non-AP STA shall establish a PTKSA with that AP to an unassociated non-AP STA shall establish a PTKSA using PASN with that AP |  Revise<https://mentor.ieee.org/802.11/dcn/24/11-24-1050-00-00bf-SA1-comment-resolution-for-OSC-category.docx> |

TGBK editor, change the text in P139L1-5 as follows:

An AP shall discard Sensing Measurement Request frame, Sensing Measurement Query frame, and SBP

Request frame from an unassociated non-AP STA if a PTKSA was required and the unassociated STA has not established ~~successfully set up~~ a PTKSA to allow protection of all sensing and/or SBP management frames between the AP and the unassociated STA.

TGBK editor, change the text in P138L58-59 as follows:

If an AP has set the USNM-MFPR field in the RSNXE to 1, an unassociated non-AP STA shall establish a PTKSA using PASN with that AP prior to initiating a sensing measurement session with that AP.

**References: P802.11bfD4.0, P802.11REVme 6.0 and P802.11bkD2.0.**