IEEE P802.11
Wireless LANs

|  |
| --- |
| Tentative Table of Contents for TGbn D0.1 |
| Date: 2024-12-03 |
| Author: |
| Name | Affiliation | Address | Phone | Email |
| Ross Jian Yu | Huawei Technologies |  |  | ross.yujian@huawei.com |

##### This submission presents a tentative table of contents for TGbn D0.1. The subclause title without approved PDT will be removed.

R0: initial version

R1: added 38.3.15.5 Segment deparser, 38.3.15.6 Frequency domain duplication, 38.3.19 Transmit requirements for an UHR ELR PPDU

R2: remove 9.4.1 Fields are not elements, 9.4.1.aaa UHR MIMO Control field, 9.4.1.aab UHR Compressed Beamforming Report field, 9.4.1.aac UHR MU Exclusive Beamforming Report field, 38.3.20.2 UHR beamforming feedback matrix V, 38.3.20.3 UHR CQI feedback; change 38.3.20 from “Beamforming” to “Coordinated beamforming”; switch order of 38.3.8 Enhanced long range PPDU and 38.3.7 Transmitter block diagram; change “an UHR” to “a UHR”

1 Contents

2

3 [Contents 7](#_bookmark0)

4

5

6 Figures 13

7

8 Tables 15

9

10

11 Editorial Notes 17

12

13 3. Definitions, acronyms, and abbreviations 19

14

15 3.1 Definitions 19

16

17 3.4 Abbreviations and acronyms 19

18

19 4. General description 21

20

21 4.3 Components of the IEEE Std 802.11 architecture 21

22

23 4.3.15bUltra high reliability (UHR) STA 21

24

25 6. Layer management 23

26

27 6.3 MLME SAP interface 23

28

1. 6.3.7 Associate 23
2. 6.3.7.3 MLME-ASSOCIATE.confirm 23
3. 6.3.7.3.2Semantics of the service primitive 23
4. 6.3.7.5 MLME-ASSOCIATE.response 23
5. 6.3.7.5.2Semantics of the service primitive 23

34

1. 6.3.8 Reassociate 23
2. 6.3.8.3 MLME-REASSOCIATE.confirm 23
3. 6.3.8.3.2Semantics of the service primitive 23
4. 6.3.8.5 MLME-REASSOCIATE.response 23
5. 6.3.8.5.2Semantics of the service primitive 23

40

41 6.5 PLME SAP interface 23

42

43 9. Frame formats 25

44

45 9.2 MAC frame formats 25

46

1. 9.3 Format of individual frame types 25
2. 9.3.1 Control frames 25
3. 9.3.1.19 NDP Announcement frame format 25
4. 9.3.1.22 Trigger frame format 25

51 9.3.1.22.1General 25

52

1. 9.3.1.22.2Common Info field 25
2. 9.3.1.22.3Special User Info field 25
3. 9.3.1.22.5aUHR variant User Info field 25
4. 9.3.1.22.10BSRP Trigger frame format 25
5. 9.3.3 (PV0) Management frames 25

58

1. 9.3.3.2 Beacon frame format 25
2. 9.3.3.5 Association Request frame format 25
3. 9.3.3.6 Association Response frame format 26
4. 9.3.3.7 Reassociation Request frame format 26
5. 9.3.3.8 Reassociation Response frame format 26

64

65 9.3.3.9 Probe Request frame format 26

1. 9.3.3.10 Probe Response frame format 26
2. 9.3.3.aaaUHR Action frame details 26
3. 9.3.3.aabProtected UHR Action frame details 26
4. 9.4 Management and Extension frame body components 26

5

1. 9.4.2 Elements 26
2. 9.4.2.aaa UHR Operation Element 26
3. 9.4.2.aab UHR Capabilities 26
4. 9.4.2.aab.1UHR PHY Capabilities Information field 26
5. 9.4.2.aab.2UHR MAC Capabilities Information field 26

11

1. 9.6 Action frame format details 27
2. 9.7 Aggregate MPDU (A-MPDU) 27
3. 9.7.3 A-MPDU contents 27

15

16 10. MAC sublayer functional description 29

17

18

1. 10.2 MAC architecture 29
2. 10.2.7 MAC data service 29
3. 10.25Block acknowledgment (block ack) 29

22 10.25.2 29

23

24

25 11. MLME 31

26

27 11.1 Synchronization 31

28 11.1.3 Maintaining synchronization 31

29

30 11.1.4 31

31

32 12. Security 33

33

34 37. Ultra high reliability (UHR) MAC specification 35

35

36

1. 37.1 Introduction 35
2. 37.2 Enhanced channel access 35
3. 37.3 UHR BSS operation 35
4. 37.4 Buffer status report 35

41

1. 37.5 Nominal packet padding values selection rules 35
2. 37.6 UHR sounding operation 35
3. 37.7 Multi-AP coordination framework 35
4. 37.8 Coordinated beamforming 35
5. 37.9 Coordinated spatial reuse 35

47

1. 37.10Coordinated time division multiple access 35
2. 37.11Coordinated R-TWT 35
3. 37.12Roaming 35
4. 37.13Power save 36
5. 37.14Non-primary channel access 36

53

1. 37.15In-device coexistence 36
2. 37.16TWT SP management 36

56

57 38. Ultra high reliability (UHR) PHY specification 37

58

59

1. 38.1 Introduction 37
2. 38.1.1 Introduction to the UHR PHY 37
3. 38.1.2 Scope 37
4. 38.1.3 UHR PHY functions 37

64 38.1.3.1 General 37

65

1

2

3

4

5

6

7

8

9

10

11

12

13

14

15

16

17

18

19

20

21

22

23

24

25

26

27

28

29

30

31

32

33

34

35

36

37

38

39

40

41

42

43

44

45

46

47

48

49

50 40

51

52

53

54

55

56

57

58

59

60

61

62

63

64

65

* + - 1. PHY management entity (PLME) 37
			2. Service specification method 37

38.1.4 PPDU formats 37

* 1. UHR PHY service interface 38
		1. Introduction 38
		2. TXVECTOR and RXVECTOR parameters 38
		3. TRIGVECTOR parameters 38
		4. PHY CONFIG\_VECTOR 38
		5. Effect of CH\_BANDWIDTH parameter on PPDU format 38
		6. Support for non-HT, HT, VHT, and HE formats 38
			1. General 38
			2. Support for non-HT format 38
			3. Support for HT format 38
			4. Support for VHT format 38
			5. Support for HE format 38
			6. Support for EHT format 38
	2. UHR PHY 39
		1. Introduction 39
		2. Subcarrier and resource allocation 39
		3. Transmission of DRU 39
		4. Interference mitigation 39
		5. LDPC encoding 39
		6. UHR PPDU formats 39
		7. Enhanced long range PPDU 39
		8. Transmitter block diagram 39
		9. Overview of the PPDU encoding process 39
			1. General 39
			2. Construction of L-STF 39
			3. Construction of L-LTF 39
			4. Construction of L-SIG 39
			5. Construction of RL-SIG 40
			6. Construction of U-SIG 40
			7. Construction of UHR ELR-MARK 40
			8. Construction of UHR-SIG 40
			9. Construction of UHR-STF 40
			10. Construction of UHR-LTF 40
			11. Construction of ELR-SIG 40
			12. Construction of Data field in a UHR PPDU 40
				1. non-ELR PPDU 40
				2. ELR PPDU 40
		10. UHR modulation and coding schemes (UHR-MCSs) and Unequal modulation (UEQM)
		11. UHR-SIG modulation and coding schemes (UHR-SIG-MCSs) 40
		12. Timing-related parameters 40
		13. Mathematical description of signals 40
			1. Notation 41
			2. Subcarrier indices in use 41
			3. Channel frequencies 41
			4. Transmitted signal 41
		14. UHR preamble 41
			1. Introduction 41
			2. Cyclic shift 41
				1. Cyclic shift for pre-UHR modulated fields 41
				2. Cyclic shift for UHR modulated fields 41

1 38.3.14.3 L-STF 41

2 38.3.14.4 L-LTF 41

3 38.3.14.5 L-SIG 41

4 38.3.14.6 RL-SIG 41

5

6 38.3.14.7 U-SIG 42

7 38.3.14.7.1General 42

8 38.3.14.7.2Content 42

1. 38.3.14.7.3Encoding and modulation 42
2. 38.3.14.8 Enhanced Long Range (ELR) MARK field 42

11

12 38.3.14.8.1ELR-MARK Matrix 42

13 38.3.14.8.2Encoding and Modulation 42

14 38.3.14.9 UHR-SIG 42

15 38.3.14.9.1General 42

16 38.3.14.9.2UHR-SIG content channels 42

17

18 38.3.14.9.3Common field for OFDMA transmission 43

19 38.3.14.9.4Common field for non-OFDMA transmission 43

20 38.3.14.9.5Common field for Co-BF transmission 43

21 38.3.14.9.6User Specific field 43

22 38.3.14.9.7Encoding and modulation 43

23

24 38.3.14.10UHR-STF 43

25 38.3.14.10.1UHR-STF for DRUs 43

26 38.3.14.10.2Global CSD for DRU transmission 43

27 38.3.14.10.3Global CSD index assignment for DRU STF transmission 43

28 38.3.14.11UHR-LTF 43

29

30 38.3.14.11.1UHR-LTF for DRUs 43

31 38.3.14.12ELR-SIG 44

32 38.3.14.12.1General 44

33 38.3.14.12.2Content 44

34 38.3.14.12.3Encoding and modulation 44

35

36 38.3.15Data field 44

37 38.3.15.1 Coding 44

38 38.3.15.1.1General 44

39 38.3.15.1.2BCC coding 44

40 38.3.15.1.3LDPC coding 44

41

42 38.3.15.1.4UHR PPDU padding process 44

43 38.3.15.1.5Encoding process for a UHR MU PPDU 44

44 38.3.15.1.6Encoding process for a UHR TB PPDU 44

45 38.3.15.1.7Encoding process for a UHR ELR PPDU 44

46 38.3.15.2 Segment parser 44

47

48 38.3.15.3 BCC interleavers 45

49 38.3.15.4 LDPC tone mapper 45

50 38.3.15.5 Segment deparser 45

51 38.3.15.6 Frequency domain duplication 45

52 38.3.15.7 Pilot subcarriers 45

53

1. 38.3.15.8 OFDM modulation 45
2. 38.3.16Packet extension 45
3. 38.3.17Non-HT duplicate transmission 45
4. 38.3.18Transmit requirements for PPDUs sent in response to a triggering frame 45
5. 38.3.19Transmit requirements for a UHR ELR PPDU 45

59

1. 38.3.20Coordinated Beamforming 45
2. 38.3.21Sounding NDP for UHR 45
3. 38.3.22Transmit specification 46
4. 38.3.22.1 Transmit spectral mask 46

64 38.3.22.1.1General 46

65

1. 38.3.22.2 Spectral flatness 46
2. 38.3.22.3 Transmit center frequency and symbol clock frequency tolerance 46
3. 38.3.22.4 Modulation accuracy 46
4. 38.3.22.4.1Introduction to modulation accuracy tests 46

5

1. 38.3.22.4.2Transmit center frequency leakage 46
2. 38.3.22.4.3Transmitter modulation accuracy (EVM) test 46
3. 38.3.23Receiver specification 46

9 38.3.23.1 General 46

10 38.3.23.2 Receiver minimum input sensitivity 46

11

1. 38.3.23.3 Adjacent channel rejection 46
2. 38.3.23.4 Nonadjacent channel rejection 46
3. 38.3.23.5 Receiver maximum input level 47
4. 38.3.24UHR transmit procedure 47
5. 38.3.25UHR receive procedure 47

17

1. 38.3.26Channel numbering 47
2. 38.3.27Regulatory requirements 47
3. 38.4 UHR PLME 47
4. 38.4.1 PLME\_SAP sublayer management primitives 47
5. 38.4.2 PHY MIB 47

23

1. 38.4.3 TXTIME and PSDU\_LENGTH calculation 47
2. 38.4.4 UHR PHY 47
3. 38.5 Parameters for UHR-MCSs 47

27

28 Annex B 49

29

30

31 B.4 PICS proforma—IEEE Std 802.11-<year> 49

32 B.4.3 IUT configuration 49

33 B.4.37a Ultra High Reliability (UHR) features 49

34 B.4.37a.1UHR MAC features 49

35

36 B.4.37a.2UHR PHY features 49

37

38 Annex C 51

39

40 C.3 MIB Detail 51

41

42

43 Annex E 53

44

45 E.1 Country information and operating classes 53

46

47

48 Annex AA 55

49

50 AA.1 Introduction 55