IEEE P802.11  
Wireless LANs

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| PDT Sounding Procedure | | | | | |
| Date: 2024-12-15 | | | | | |
| Author(s): | | | | | |
| Name | Affiliation | Address | Phone | email | |
| You-Wei Chen | MediaTek | 2840 Junction Ave, San Jose, CA 95134 |  | you-wei.chen@mediatek.com | |
| Jianhan Liu | MediaTek |  |  | Jianhan.Liu@mediatek.com | |
| Shengquan Hu | MediaTek |  |  | shengquan.hu@mediatek.com | |
| Alice Chen | Qualcomm |  |  | alicel@qti.qualcomm.com | |
| Alfred Asterjadhi | Qualcomm |  |  | aasterja@qti.qualcomm.com | |
| Sameer Vermani | Qualcomm |  |  | svverman@qti.qualcomm.com | |
| Youhan Kim | Qualcomm |  |  | youhank@qti.qualcomm.com | |
| Ron Porat | Broadcom |  |  | ron.porat@broadcom.com | |
| Shubhodeep Adhikari | Broadcom |  |  | shubhodeep.adhikari@broadcom.com | |
| Tianyu Wu | Apple |  |  | tianyu@apple.com | |
| Qinghua Li | Intel |  |  | Qinghua.li@intel.com | |
| Anand Jee | Samsung |  |  | anandjee7@gmail.com | |
| Eunsung Jeon | Samsung |  |  | eunsung.jeon@samsung.com | |
| Genadiy Tsodik | Huawei |  |  | Genadiy.tsodik@huawei.com | |
| Jason Yuchen Guo | Huawei |  |  | guoyuchen@huawei.com | |
| Ross Jian Yu | Huawei |  |  | ross.yujian@huawei.com | |
| Dongguk Lim | LG Electronics |  |  | dongguk.lim@lge.com | |
| Insik Jung | LG Electronics |  |  | insik0618.jung@lge.com | |
| Jiayi Zhang | Ofinno |  |  | jzhang@ofinno.com | |
| Leonardo Lanante | Ofinno |  |  | llanante@ofinno.com | |
| Bo Cao | ZTE |  |  | cao.bo4@zte.com.cn | |
| Qisheng Huang | ZTE |  |  | Huang.qisheng@zte.com.cn | |
| Yun Li | ZTE |  |  | li.yun3@zte.com.cn | |
| Dana Ciochina | Sony |  |  | Dana.Ciochina@sony.com | |
| Kosuke Aio | Sony |  |  | kosuke.aio@sony.com | |
| Pei Zhou | TCL |  |  | zhoupei36@gmail.com | |
| Hanqing Lou | InterDigital |  |  | Hanqing.lou@interdigital.com | |
| Mahmoud Kamel | InterDigital |  |  | mahmoud.kamel@interdigital.com | |
| Rui Yang | InterDigital |  |  | rui.yang@interdigital.com | |
| Xiaofei Wang | InterDigital |  |  | Xiaofei.wang@interdigital.com |
| Ying Wang | InterDigital |  |  | Ying.Wang@interdigital.com |
| Bo Sun | Sanechips |  |  | sun.bo1@sanechips.com.cn | |
| Juhyung Lee | Nokia |  |  | juhyung.lee@nokia.com | |
| Mario Costa | Nokia |  |  | mario.costa@nokia.com |
| Okan Mutgan | Nokia |  |  | okan.mutgan@nokia.com | |
| Yeon-Geun Lim | Newracom |  |  | chaind3@gmail.com | |
| Rui Cao | NXP |  |  | rui.cao\_2@nxp.com | |
|  |  |  |  |  | |
|  |  |  |  |  | |
|  |  |  |  |  | |

Abstract

This document contains Proposed Draft Text (PDT) for the sounding procedure of the proposed TGbn (UHR, Ultra High Reliability) amendment to the 802.11 standard.

**Revision information**

The following is a summary of the important changes that occurred within each revision of this document:

|  |  |
| --- | --- |
| **Revision** | **Major changes** |
| 0 | Initial revision |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

**Introduction**

Interpretation of a Motion to Adopt.

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe Draft. The abstract, revision information, introduction, explanation of the proposed changes and references sections are not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

**Explanation of the proposed changes:**

The proposed changes to the 802.11 TGbn draft within this document are based on the following motions adopted by the TGbn task group:

**Relevant passing motions:**

[Motion #97, [1]]

* Both sequential NDP based and joint NDP based sounding options will be supported for COBF in 802.11bn.

[Motion #98, [1]]


* Two separate capabilities shall be defined for the maximum number of spatial streams supported for reception of a sounding NDP in UHR and the maximum total number of streams (across all users) supported for reception in UHR DL MU-MIMO and CoBF PPDUs
  + The only possible values for each capability are 4 and 8.

[Motion #99, [1]]

* The Coordinated beamforming (COBF) transmission phase in 802.11bn shall be limited to 2 APs.


[Motion #100, [1]]

* The sequential NDP based sounding protocol will be as shown below for COBF
  + Sounding happens one BSS at a time
  + NDPA only addresses the in-BSS STAs
  + MAC related additional frames are TBD.



[Motion #101, [1]]

* The joint NDP based sounding protocol will be as shown below for COBF
  + Sounding happens for one BSS’s STAs at a time
  + NDPA only addresses the in-BSS STAs
  + MAC related additional frames are TBD
  + Joint NDP based feedback will be based on large V-based feedback where the eigen-vectors span the antennas across both Aps



[Motion #102, [1]]

* For joint NDP based sounding, one AP will frequency synchronize to the other for both of its NDP transmissions
  + For both the NDPs, the AP doing the correction brings its frequency within a certain TBD range of the reference AP

Motion #103, [1]]

* In the UHR sounding process for COBF, for the joint sounding case as well as for the sequential sounding case, the NDP shall always carry the BSS color of the AP which transmitted the NDPA.

Motion #115, [1]]

* For the maximum number of spatial streams supported for reception of sounding NDP in UHR and the maximum total number of streams (across all users) supported for reception in UHR DL MU-MIMO and COBF PPDUs:
  + 4 is mandatory except for a non-AP STA with 20 MHz-Only Limited Capabilities Support subfield equal to 1.
  + 8 is optional for DL MU-MIMO and sounding NDP (Note: More than 4 is not allowed for COBF PPDUs

Motion #116, [1]]

* The COBF sequential sounding support to be conditional mandatory if the device supports COBF.

Motion #118, [1]]

* For sequential NDP based sounding, one AP will frequency synchronize to the other for both of its NDP transmissions
  + For both its NDPs, the AP doing the correction brings its frequency within a certain TBD range of the reference AP.

**Text to be adopted begins here.**

***TGbn editor: Please add the following new subclause for Sounding Procedure to the 802.11bn draft D0.1:***

**37.6 UHR sounding operation**

**37.6.1 General**

Transmit beamforming, DL MU-MIMO and DL COBF require knowledge of the channel state to compute a steering matrix that is applied to the transmit signal to optimize reception at one or more receivers. UHR STAs use the EHT sounding protocol as defined in 35.7 (EHT sounding operation) to determine the channel state information for transmitting SU beamforming and DL MU-MIMO. UHR STAs use the UHR sounding protocol as defined in 37.6 (UHR sounding operation) to determine the channel state information for transmitting DL COBF. The UHR sounding protocol provides explicit feedback mechanism, defined as UHR trigger-based (TB) sequential NDP sounding sequence and UHR TB joint NDP sounding sequence for DL COBF. In the UHR TB sounding sequences, the UHR beamformee measures the channel using a training signal as defined in 38.3.21 (Sounding NDP for UHR) transmitted by one or two UHR beamformers and sends back a transformed estimate of the channel state (see 37.6.3 (Rules for UHR sounding protocol sequences)). The UHR beamformer uses this estimate to derive the steering matrix.

**37.6.2 UHR sounding protocol**

**37.6.3 Rules for UHR sounding protocol sequences**

A UHR COBF beamformer that initiates a UHR TB sounding sequence shall transmit a UHR NDP Announcement frame with TBD or more STA Info fields and the RA field set to the broadcast address. STA Info fields shall only address to the responding AP and the non-AP UHR STAs associated with the initiating AP.

The UHR NDP Announcement frame shall be followed after a SIFS by EHT sounding NDP(s) transmitted from the responding AP in a UHR TB sequential NDP sounding sequence, or simultaneously from the initiating AP and the responding AP in a UHR TB joint NDP sounding sequence. The EHT sounding NDP(s) shall be followed after a SIFS by the BFRP Trigger frame from the initiating AP. Subsequent BFRP Trigger frames, if any, in the UHR TB sounding sequence shall be transmitted SIFS after the UHR TB PPDU transmitted in response to the previous BFRP Trigger frame. Each UHR COBF beamformee that is addressed by a BFRP Trigger frame shall respond after a SIFS with a UHR TB PPDU containing one or more UHR Compressed Beamforming/CQI frames.

An example of a UHR TB sequential NDP sounding is shown in Figure 37-x (An illustration of UHR TB sequential NDP sounding). A UHR COBF beamformer that initiates a UHR TB sequential NDP sounding shall transmit the UHR NDP Announcement frame to solicit the EHT NDP from the responding AP. The UHR NDP Announcement frame shall only address to the responding AP and the non-AP UHR STA associated with the initiating AP. To collect the channel state to compute a steering matrix for DL COBF transmission, both APs need to initiate an EHT TB sounding and a UHR TB sequential NDP sounding sequentially, i.e., total four sequences. For all the sounding sequences, one AP conducts the frequency correction on its EHT sounding NDPs to a TBD range of the reference AP, i.e., either AP1 or AP2.



#### Figure 37-x—UHR TB sequential NDP sounding

An example of a UHR TB joint NDP sounding is shown in Figure 37-y (An illustration of UHR TB joint NDP sounding). A UHR COBF beamformer that initiates a UHR TB joint NDP sounding shall transmit the UHR NDP Announcement frame followed after a SIFS by EHT sounding NDPs transmitted simultaneously from the initiating AP and responding AP. The UHR NDP Announcement frame shall only address to the responding AP and the non-AP UHR STAs associated with the initiating AP. To collect the channel state to compute a steering matrix for DL COBF transmission, both APs need to initiate a UHR TB joint NDP sounding sequentially, i.e., total two sequences. For both UHR TB joint NDP sounding sequences, one AP conducts the frequency correction on its EHT sounding NDPs to a TBD range of the reference AP, i.e., either AP1 or AP2.



#### Figure 37-y—UHR TB joint NDP sounding

**37.6.4 Rules for generating segmented feedback**

**37.6.5 Sounding NDP transmission for UHR TB sounding sequence**

The TXVECTOR parameters for an EHT sounding NDP shall be set as follows:

* FORMAT is set to EHT\_MU.
* APEP\_LENGTH is set to 0.
* SPATIAL\_REUSE is set to PSR\_AND\_NON\_SRG\_OBSS\_PD\_PROHIBITED (see 35.11.2 (SPATIAL\_REUSE)).
* TXOP\_DURATION set to either 127 or a value defined in Equation (35-3).

The intended recipient(s) of an EHT sounding NDP is the STA(s) addressed by the STA Info field(s) in the immediately preceding UHR NDP Announcement frame.

[TBD MAC section are covered in 24/2030 PDT-MAC-Coordinated-Beamforming, Jason Yuchen Guo (Huawei)]

[38.1 Introduction, 38.1.1 Introduction to the UHR PHY, 38.3.21 Sounding NDP for UHR are covered in 24/2015 PDT-PHY-CoBF, Ron Porat (Broadcom)]

**Text to be adopted ends here.**

**References:**

1. [11-24-0171r21](https://mentor.ieee.org/802.11/dcn/24/11-24-0171-21-00bn-tgbn-motions-list-part-1.pptx): 11-24-0171-21-00bn-tgbn-motions-list-part-1, Alfred Asterjadhi (Qualcomm Inc.)