**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) |
| Title | **Resolution for Sponsor Ballot Comments 100 and 102** |
| Date Submitted | 16th January 2013 |
| Source | [Tuncer Baykas, Shuzo Kato][Tohoku University][Japan] | Voice: [ ]Fax: [ ]E-mail: [ ] |
| Re: | [If this is a proposed revision, cite the original document.][If this is a response to a Call for Contributions, cite the name and date of the Call for Contributions to which this document responds, as well as the relevant item number in the Call for Contributions.][Note: Contributions that are not responsive to this section of the template, and contributions which do not address the topic under which they are submitted, may be refused or consigned to the “General Contributions” area.] |
| Abstract | New tables for LECIM PHYs |
| Purpose | Resolving sponsor ballot comments |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. |

**8.1.1 Operating Frequency Range**

***Change the first paragraph***

A compliant device shall operate in one or several frequency bands summarized in table 66, table 66a and table 66b. Table 66a shows frequency bands for devices supporting LECIM DSSS PHY and Table 66b shows frequency bands for devices supporting LECIM FSKPHY

**Table 66a Operating frequency ranges for LECIM DSSSPHY**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Band identifier | Frequency Range (MHz) | Bandwidth(KHz) | Modulation | Chip Rate(kchips/s) |
| 470 | 470-510 | 100  | BPSK/OQPSK | 100 |
| 780 | 779-787 | 1000  | BPSK/OQPSK | 1000  |
| 863 | 863-780 | 100  | BPSK/OQPSK | 100 |
| 915  | 902-928 | 200  | BPSK/OQPSK | 200  |
| 400  | 400  |
| 600  | 600  |
| 800  | 800  |
| 1000  | 1000  |
| 1000 | OQPSK | 2000 |
| 922 | 915-928 | 200  | BPSK/OQPSK | 200  |
| 400  | 400  |
| 600  | 600  |
| 800  | 800  |
| 1000  | 1000  |
| 917 | 917.1-923.5 | 200  | BPSK/OQPSK | 200  |
| 400  | 400  |
| 600  | 600  |
| 800  | 800  |
| 1000  | 1000  |
| 920 | 920-928 | 200  | BPSK/OQPSK | 200  |
| 400  | 400  |
| 600  | 600  |
| 800  | 800  |
| 1000  | 1000  |
| 921 | 915-928 | 200  | BPSK/OQPSK | 200  |
| 400  | 400  |
| 600  | 600  |
| 800  | 800  |
| 1000  | 1000  |
| 2450 | 2400-2485.5 | 1000 | BPSK/OQPSK | 1000 |
| 2000 | 2000 |

**Table 66b Operating frequency ranges for LECIM FSK PHY**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Band identifier | Frequency Range (MHz) | Bandwidth(KHz) | Modulation | Bit Rate(kbits/s) |
| 169 | 169.400-169.475 | 25 | FSK/GFSK/P-FSK/P-GFSK | 25 |
| 12.5  | 12.5  |
| 433 | 433.050-434.790 | 37.5 | FSK/GFSK/P-FSK/P-GFSK | 37.5 |
| 25 | 25 |
| 12.5  | 12.5  |
| 470 | 470-510 | 37.5 | FSK/GFSK/P-FSK/P-GFSK | 37.5 |
| 25 | 25 |
| 12.5  | 12.5  |
| 780 | 779-787 | 37.5 | FSK/GFSK/P-FSK/P-GFSK | 37.5 |
| 25 | 25 |
| 12.5  | 12.5  |
| 863 | 863-780 | 37.5 | FSK/GFSK/P-FSK/P-GFSK | 37.5 |
| 25 | 25 |
| 12.5  | 12.5  |
| 915 | 902-928 | 37.5 | FSK/GFSK/P-FSK/P-GFSK | 37.5 |
| 25 | 25 |
| 12.5  | 12.5  |
| 922 | 915-928 | 37.5 | FSK/GFSK/P-FSK/P-GFSK | 37.5 |
| 25 | 25 |
| 12.5  | 12.5  |
| 917 | 917.1-923.5 | 37.5 | FSK/GFSK/P-FSK/P-GFSK | 37.5 |
| 25 | 25 |
| 12.5  | 12.5  |
| 920 | 920-928 | 37.5 | FSK/GFSK/P-FSK/P-GFSK | 37.5 |
| 25 | 25 |
| 12.5  | 12.5  |
| 921 | 921-928 | 37.5 | FSK/GFSK/P-FSK/P-GFSK | 37.5 |
| 25 | 25 |
| 12.5  | 12.5  |