**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) |
| Title | **Proposed comment resolution for CID 373, 375, 376** |
| Date Submitted | 18 August 2015 |
| Source | \*[Verotiana Rabarijaona, Fumihide Kojima], †[Hiroshi Harada]\*[NICT], †[Kyoto University]\*[3-4, Hikarino-oka, Yokosuka, 239-0847 Japan], †[36-1 Yoshida-Honmachi, Sakyo-ku, Kyoto 606-8501 Japan] | Voice: [+81-46-847-5075]Fax: [+81-46-847-5089]E-mail: [rverotiana@nict.go.jp] |
| Re: | 802.15.10 Consolidated Comment Entry Form, CID 373, 375, 376 |
| Abstract | Provides a proposed resolution to CID 373, 375, 376 |
| Purpose | To be used by the technical editor to apply the necessary changes to the draft to resolve CID 373, 375, 376 |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. |

**Comment CID CID 373, 375, 376**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Name** | **Page** | **Sub-clause** | **Line #** | **Comment** | **Proposed Change** |
| 373 | Noriyuki Sato | 58 | 6.2.2.10 | 32 | Using SINR as LQM is not good idea since PQM is calculated by adding LQMs. | Consider using dB and make it integer type and some normalize to represent SINR metric. |
| 375 | Billy Verso | 58 | 6.2.2.10 | 38 | SINR is not defined anywhere | Define SINR, and describe what it is and how it is used. |
| 376 | Kiyoshi Fukui | 58 | 6.2.2.10 | 38 | Need a definition of an unit to be represented in. Maybe, dB is appropriate. If an unit is dB, the type of SINR metric should be Integer. | Refine the SINR definition. |

**Resolution: Revise**

Remove the SINR as a metric and provide a way to handle signal strength related metric

* ***Insert the following new clause before 5.2.2.1***

5.2.2.x. Signal quality scale (SQS)

An implementer may use this metric to represent a signal quality related metric such as the RSSI, SINR, SNR, etc. The values of the selected metric are mapped on a scale ranging between 1 and 10. A low value on the scale indicates a good signal quality and a high value indicates a poor signal quality. The selection of the signal quality related metric and the mapping between its values and the scale is out of the scope of this document.

* ***Replace the SINR row in Table 11 with:***

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Value** | **Name** | **Description** | **Type** | **Length in octets** |
| 1 | SQS | See 5.2.2.x | Integer | 2 |

* ***Insert a new acronym for SQS is clause 3.2***