**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |  |
| --- | --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) | |
| Title | **Proposed comment resolution for CID 2294 from LB113** | |
| Date Submitted | 18 January 2016 | |
| Source | \*[Verotiana Rabarijaona, Fumihide Kojima], †[Hiroshi Harada]  \*[NICT], †[Kyoto University]  \*[3-4, Hikarino-oka, Yokosuka, 239-0847 Japan], †[36-1 Yoshida-Honmachi, Sakyo-ku, Kyoto 606-8501 Japan] | Voice: [+81-46-847-5075]  Fax: [+81-46-847-5089]  E-mail: [rverotiana@nict.go.jp] |
| Re: | 802.15.10 Consolidated Comment Entry Form, CID 2294 | |
| Abstract | Provides a proposed resolution to CID 2294 | |
| Purpose | To be used by the technical editor to apply the necessary changes to the draft to resolve CID 2294 | |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. | |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. | |

**Comments**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Commenter** | **Page** | **Clause** | **Line** | **Comment** | **Proposed change** |
| Noriyuki Sato | 74 | 6.2.2 | 32 | If the service ID is indicated but no mesh root is indicated when the data is sent by the device other than the mesh root, the destination will be always the mesh root that provides indicated service, since that indication means, "This data frame should be sent to any mesh root which provides indicated service". Since the device automatically selects mesh if there are multiple services that provides the indicated service, the destination unnecessarily belong to the mesh which the L2R layer selects to join. Though it may belong to the same mesh at some time, the L2R layer may switch to another mesh that provides same service. In this case, the destination will not be in same mesh anymore. | "If the service ID is indicated but the mesh root is not indicated by the primitive, the destination address should not be indicated and can be ommitted for the US. |

**Resolution: Revise**

In the current draft, a device belongs to only one mesh at a time for one service. As per 5.1.2.2.1 and 5.1.2.2.2, if a device finds a mesh with a better PQM, it disconnects with the first mesh, then joins the second one.

The way the MT, the NT and the global NT are recorded, a device only knows the PQM of the neighbors in the same mesh.

If no destination address is indicated, the frame should be transmitted to the current mesh root even if the mesh root ID in the primitive is 0xffff, but we can omit the destination address in the L2R in this case.

* ***Insert a new flag in L2R-DATA.request as follows***

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Type** | **Valid Range** | **Description** |
| MeshRootData | Boolean | TRUE, FALSE | Indicates whether the data frame is to be sent to the mesh root. |

* ***Insert the following at the end of the description of "FnlDestAddr":***

Ignored if MeshRootData is TRUE.

* ***Modify the 3rd and 4th paragraph on p.75 as follows:***

If the Source Address Present field is set to 0, the Source Address field is omitted from the Addressing fields. The Source Address field is omitted when it is the same as the MAC source address. When the Source Address Present field is set to 1, the Source Address field is present.

If the Destination Address Present field is set to 0, the Destination Address field is omitted from the Addressing fields. The Destination Address is omitted when it is the same as the MAC destination address or when the data frame is to be sent to the mesh root. When the Destination Address Present field set to 1, the Destination Address field is present.

* ***Insert the following text after the fourth paragraph on p.42***

If a data frame is received from a neighbor that does not belong to the local NT of the current mesh, the frame is dropped. An OUT\_OF\_NT\_DATA notification is sent to the next higher layer with the L2R-NOTIFY.indication primitive.

* ***Rename “Neighbor Table” in the MT to “Local Neighbor Table (Local NT)” to avoid confusion. Replace NT with “local NT” where applicable.***

* ***Modify Figure 21 as follows:***



* ***Insert a new field “Mesh Root Data” in Figure 59 after Mesh Address Mode***
* ***Insert the following text after the second paragraph of 6.2.2.1***

If the Mesh Root Data field is set to 1, the current data frame is to be sent to the mesh root. The Destination Address Present is set to 0 and the Destination PAN ID and Destination Address fields are omitted. Otherwise, when the Destination Address Present is set to 1, the current data frame is to be sent to the address indicated in the Destination Address field; when the Destination Address Present is set to 0, the current data frame is to be sent to the address indicated in the Destination Address field of the MHR.