**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |  |
| --- | --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) | |
| Title | D0 Text Input – Kookmin Univ. PHY modes on table summary | |
| Date Submitted | 17 May 2016 | |
| Source | Kookmin University | Voice: [ ] Fax: [ ] E-mail: [ yjang@kookmin.ac.kr] |
| Re: | [If this is a proposed revision, cite the original document.]  [If this is a response to a Call for Contributions, cite the name and date of the Call for Contributions to which this document responds, as well as the relevant item number in the Call for Contributions.]  [Note: Contributions that are not responsive to this section of the template, and contributions which do not address the topic under which they are submitted, may be refused or consigned to the “General Contributions” area.] | |
| Abstract | [A short summary of Kookmin PHY modes following the D0 template] | |
| Purpose | [Re-format PHY mode tables] | |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. | |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. | |

**PHY Layer Operating mode(s)**

**PHY A modes**

Table 1: Kookmin PHY A modes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **PHY Operating Modes** | | | | | |
| **Modulation** | **RLL Code** | **Optical Clock Rate** | **FEC** | | **Data Rate** |
| **Outer code**  (Mismatched Frame rates FEC) | **Inner code** |
| S2-PSK | No | 200  Hz | Repeat code  (10 symbol/sec) | Code rate = (N-1)/N | Uncoded data rate is equal to the symbol rate  Rbit = (bit/symbol) x (symbol rate) = (K) x 10 |
| S8-PSK | Yes | 800  Hz | Repeat code  (10 symbol/sec) | Code rate = (N-1)/N  bad-sampling code rate = 1 | Uncoded data rate is triple the symbol rate  Rbit = (bit/symbol) x (symbol rate) = (3×N) x 10 |
| DS8-PSK | No | 800×n  Hz | Repeat code  (10 symbol/sec) | Code rate = (N-1)/N  bad-sampling code rate = 1 | Uncoded data rate is triple the symbol rate  Rbit = (bit/symbol) x (symbol rate) = (3N) x 10 |

where

symbol = (data + its repetition)

N is the number of LED (a group of LEDs) on a transmitter.

**PHY B modes**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **Previous Table. Flicker-free Rolling Shutter PHY 5 Operating Modes** | | | | | | | |
| **Modulation** | **RLL Code** | **Tx**  **optical Clock Rate** | **Rx**  **frame rate** | **Frame Length** | **FEC** | **OH** | **PHY SAP throughput (bps)** |
| C-OOK | Manchester | Clock rate = 2.2 kHz  Symbol rate = **10** | Rx(fps) >Tx (1) | DS=**100**(2) | None | Preamble  +Ab | 60 |
| 4B6B | DS=6**0**(4) | None | 150 |
| Manchester | Clock rate = 4.4 kHz  Symbol rate = **20** | Rx(fps) ~ Tx(3) | DS=**60**(4) | Outer code(5) | Preamble  +2.Ab | 580 |
| 4B6B | DS=**60**(4) | 700 |
| **Modulation** | **Coding** | **Tx**  **(freq.# /symbol rate)** | **Rx**  **frame rate** | **FEC** | | **OH** | **PHY SAP throughput (bps)** |
| CM-FSK | None | #\_of\_Freq. = 32  Symbol rate = 10 | Rx(fps) ≥ 2.Tx | None | | Ab  (per symbol) | 40 |
| 2-PSK | 50 |
| 4-PSK | #\_of\_Freq. = 64  Symbol rate = 10 | Outer FEC code(6) | | 70 |

Table 2.1: Kookmin PHY B –OOK modes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **PHY Operating Modes** | | | | | |
| **Mod.** | **RLL Code** | **Optical Clock Rate** | **FEC** | | **Data Rate**  PHY SAP throughput (bps) |
| **Outer code**  (to solve **frame rate variation** and the **time gap** between Images) | **Inner code**  (images fusion + frame drop error detection) |
| OOK | Manchester | 2.2 kHz | Repeat DS=100 | Images fusion code  (single Ab frame)  Code rate = (N-2)/N | 60 |
| 4B6B | 2.2 kHz | Repeat DS=60 | 150 |
| Manchester | 4.4 kHz | Repreat DS=60 | 2/3 missed frames detection code  (2 Ab frame)  Code rate = (N-4)/N | 580 |
| 4B6B | 4.4 kHz | Repreat DS=60 | 700 |

where N is the number of bits per data sub-packet (DS).

Table 2.2 Kookmin PHY B –FSK modes

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **PHY Operating Modes** | | | | | |
| **Mod.** | **RLL Code** | **Optical Clock Rate** | **FEC** | | **Data Rate**  PHY SAP throughput (bps) |
| **Outer code** | **Inner code**  (**Mismatched frame rates code**) |
| FSK | 32-FSK | Variable | Repeat code  (10 symbol/sec) | Code rate = 4/5 | 40 |
| 32-FSK/2-PSK | Repeat code  (10 symbol/sec) | Code rate = 5/6 | 50 |
| 62-FSK/4-PSK | Repeat code  (10 symbol/sec) | Code rate = 7/8 | 70 |

where symbol = (data + its repetition)

**PHY C modes**

Table 3.1: Kookmin PHY C modes (color code)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **PHY C Operating Modes** | | | | |
|  |  | **FEC** | |  |
| **Modulation** | **RLL code** | **Outer code** | **Inner code** | **Data Rate** |
| 2D-sequential code | None | Repeat code  (symbol/sec) | Code rate = data / (data +clock information)  = N/(N+4)  Spatial coding | (symbol rate) x (#\_data LEDs) |
| 4 color  2D-sequential code | (symbol rate) x 2.(#\_data LEDs) |
| 8 color  2D-sequential code | (symbol rate) x 3.(#\_data LEDs) |
| QR-ISC code | RQR code  - (clock transmission) |

where N is the number of data bits being transmitted through a 2D code block.

Table 3.2: Kookmin Invisible code

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **PHY Operating Modes** | | | | | |
| **Modulation**  **(m:n)** | **RLL Code** | **Optical Clock Rate** | **FEC** | | **Data Rate (bits)**  **m x n x 15 x** RS\_option x CC\_option |
| **Outer code (RS)** | **Inner code (CC)** |
| 2D-invisible sequential code 4:3 | None | 30Hz | RS\_option | CC\_option | **180** x RS\_option  x CC\_option |
| 2D-invisible sequential code 16:10 | None | 30Hz | RS\_option | CC\_option | **2400** x RS\_option  x CC\_option |
| 2D-invisible sequential code 8:5 | None | 30Hz | RS\_option | CC\_option | **600** x RS\_option  x CC\_option |
| 2D-invisible sequential code 16:9 | None | 30Hz | RS\_option | CC\_option | **2160** x RS\_option  x CC\_option |
| 2D-invisible sequential code 8:3 | None | 30Hz | RS\_option | CC\_option | **360** x RS\_option  x CC\_option |

where

N: Number of vertical cells

M: Number of horizontal cells

RS\_option: Select one RS scheme from Table 3.2b

CC\_option: Select one CC scheme from Table 3.c

Table 3.2b: Outer code (RS)

|  |  |  |
| --- | --- | --- |
| RS\_option | RS description | RS\_rate |
| 1 | None | 1 |
| 2 | RS(64,32) | 1/2 |
| 3 | RS(160,128) | 128/160 |
| 4 | RS(15,7) | 7/15 |
| 5 | RS(15,11) | 11/15 |
| 6 | RS(15,2) | 2/15 |
| 7 | RS(15,4) | 4/15 |

Table 3.2c: Inner code (CC)

|  |  |  |
| --- | --- | --- |
| CC\_option | CC description | CC\_rate |
| 1 | None | 1 |
| 2 | CC(1/4) | 1/4 |
| 3 | CC(1/3) | 1/3 |
| 4 | CC(2/3) | 2/3 |