**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) |
| Title | **Kookmin PHY constants and PHY PIB attributes** |
| Date Submitted | [September, 2016] |
| Source | Trang Nguyen, and Yeong Min Jang (Kookmin University) |
| Re: |  |
| Abstract | Kookmin PHY constants and attributes are introduced. |
| Purpose | D0 Comments Resolutions and Editorial Revision. |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. |

# **10.5.1 PHY constants**

**Table 124- PHY constants**

|  |  |  |
| --- | --- | --- |
| **Constant** | **Description** | **Value** |
| aFSKPreamble1 | The first preamble frequency used for OCC modes, including FSK and OOK modulations. | 200Hz |
| aOccDefaultSpatialResolution | The number of LEDs (light sources) at Tx in case of spatial modulation.The default spatial resolution is applied for S2-PSK, S8-PSK, and HS-PSK. | 2 light sources |
|  |  |  |

# **10.5.2 PHY PIB attributes**

**Table 125- PHY PB attributes (continued)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Attribute** | **Identifier** | **Type** | **Range** | **Description** |
| phyOccProposerID |  | integer | 0-7 (3 bits) | This attributes specifies the OCC proposers as shown in table 127.  |
| phyOccApplication SpecificMode |  | integer | 0-N  | This attributes specifies the application specific PHY modes those belong to an OCC proposer. E.g. Kookmin OCC Application specific PHY modes are shown in table 126. |
| phyOccOpticalClockRate |  | integer | 5-20 | The optical clock rate is applied for S2-PSK, S8-PSK, and the S2-PSK of HS-PSK modulation.0: 5 Hz1: 10 Hz2: 15 Hz3: 20 Hz |
| phyOccSymbolRate |  | integer | 5-10 | The symbol rate is applied for FSK, 2D-sequential color code, invisible code modulation:0: 5 Hz1: 10 Hz |
| phyOccSubPacketRate |  | integer | 60-120 | The sub-packet rate is applied for OOK modulation, indicating the number of data sub-packets (DS) repeated per second.0: 60 DS/sec1: 120 DS/sec |
|  |  |  |  |  |

**Table 127- PHY OCC Proposer ID (A -> Z proposers sorting)**

|  |  |
| --- | --- |
| **PIB Attribute Value** | **OCC Proposer** |
| 0 | Intel |
| 1 | Kookmin |
| 3 | National Taiwan University |
| 2 | Panasonic |
| 4 | SNUST |
| 5-7 | Reserved |

**Table 126- Intel OCC Application Specific PHY modes**

|  |  |  |
| --- | --- | --- |
| **phyOccProposerID** | **PHY Attribute Value** | **Mode Name** |
| 0 | 0 | First UFSOOK mode |
| 0 | 1 | Second UFSOOK mode |
| 0 | … |  |
| 0 | 10 | Twinkle VPPM mode n |
| 0 | 11- N | Reserved |

**Table 126- Kookmin OCC Application Specific PHY modes (continued)**

|  |  |  |
| --- | --- | --- |
| **phyOccProposerID** | **PHY Attribute Value** | **Mode Name** |
| 1 | 0 | S2-PSK |
| 1 | 1 | S8-PSK |
| 1 | 2 | HS-PSK |
| 1 | 3 | 32-FSK |
| 1 | 4 | 64-FSK |
| 1 | 5 | 64-FSK/2-PSK |
| 1 | 6 | OOK mode 1 |
| 1 | 7 | OOK mode 2 |
| 1 | 8 | … |
| 1 | 9 | 2D-sequential color code mode 1 |
| 1 | 10 | 2D-sequential color code mode 2 |
| 1 | 11 | Kookmin Invisible code |
| 1 | 12-16 | Reserved |

**Table 126- NTU OCC Application Specific PHY modes (continued)**

|  |  |  |
| --- | --- | --- |
| **phyOccProposerID** | **PHY Attribute Value** | **Mode Name** |
| 2 | 0 | First RS-FSK mode |
| 2 | 1 | Second RS-FSK mode |
| 2 | 2- M | Reserved |