**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |  |
| --- | --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) | |
| Title | **PHY modes and TXs/RXs (Kookmin comment)** | |
| Date Submitted | September 2016 | |
| Source | Trang Nguyen, Yeong Min Jang |  |
| Re: | [Proposed revision for Hideki contribution on PHY modes and TXs/RXs]  [Cite to 16-0540-00-007a.] | |
| Abstract | [Description of document contents.] | |
| Purpose | [Description of what the author wants P802.15 to do with the information in the document.] | |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. | |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. | |

# Annex X

(informative)

Table X1 shows that each PHY mode mainly supports what sorts of Tx.

Kookmin comments:

**Comment #1:** The PHY 4, PHY 5 and PHY 6 modes classification is already up on the types of transmitter. Table X1 may be not so necessary. Table X2 is important.

Table X1 – PHY Modes / TXs

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | | Discrete (or single) source | Surface source | 2-Dimensional / Screen | Painting |
| PHY I | | x | x |  |  |
| PHY II | | x | x |  |  |
| PHY III | | x | x |  |  |
| PHY IV | UFSOOK | x | x |  |  |
| Twinkle VPPM | x | x |  |  |
| S2-PSK | x |  |  |  |
| S2+DMS-PSK | x |  |  |  |
| Offset-VPWM | x | x |  |  |
| PHY V | RS-FSK |  | x |  |  |
| Compatible M-FSK |  | x |  |  |
| C-OOK |  | x |  |  |
| Packet PPM/PWM |  | x |  |  |
| PHY VI | 2D-sequential color code |  |  | x |  |
| VTASC |  |  | x | x |
| Kookmin Invisible code |  |  | x |  |
| Invisible Data embedded display Tx Scemes |  |  | x |  |
| PHY VII | Fraunhofer High-bandwidth PHY | x | x |  |  |
| PureLiFi Low-bandwidth PHY | x | x |  |  |

# Annex Y

(informative)

**Comment #2:** Combination of PD and Camera Receivers is fine, but too much information in a table may be not easy for reader understanding. The table information should be comprehensive.

Table X2 shows that each PHY mode mainly supports what sorts of Rx.

Table X2 – PHY Modes / RXs

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | | Photodiode | | Image sensor | | | Other characteristics |
| Monochrome | Color | Global shutter | Rolling shutter | High-speed / ROI |
| PHY I | |  |  |  |  |  |  |
| PHY II | |  |  |  |  |  |  |
| PHY III | |  |  |  |  |  |  |
| PHY IV | UFSOOK | Y1 |  | Y2 |  | Y3 |  |
| Twinkle VPPM | Y4 |  |  |  | Y5 |  |
| S2-PSK |  |  | Y6 |  | Y7 |  |
| S2+DMS-PSK |  |  |  |  | Y8 |  |
| Offset-VPWM |  |  | Y9 | Y10 |  |  |
| PHY V | RS-FSK |  |  |  | 15.1 | Y11 |  |
| Compatible M-FSK |  |  |  | 15.2 | Y12 | camera support |
| C-OOK |  |  |  | 13.3 |  |  |
| Packet PPM/PWM |  |  |  |  |  |  |
| PHY VI | 2D-sequential color code |  |  |  |  |  |  |
| VTASC |  |  |  |  |  |  |
| Kookmin Invisible code |  |  |  |  |  |  |
| Invisible Data embedded display Tx Scemes |  |  |  |  |  |  |
| PHY VII | Fraunhofer High-bandwidth PHY |  |  |  |  |  |  |
| PureLiFi Low-bandwidth PHY |  |  |  |  |  |  |

**Comment #3:** The technical descriptions are addressed after the summarized information in the table as follows. The descriptions should contain:

* The suggested parameters for system
* The demodulation technique and the numerical performance

**(Y-1). UFSOOK Monochrome Photodiode Decoder**

TBD

**(Y-2). UFSOOK Color Photodiode Decoder**

TBD

**(Y-3). UFSOOK High-speed camera/RoI Camera Decoder**

TBD

**(Y-6). S2-PSK Rolling Shutter Camera Decoder**

TBD

**(Y-7). S2-PSK High-speed camera/RoI Camera Decoder**

TBD

**(Y-10). Offset VPWM Rolling Shutter Camera Decoder**

TBD