**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) |
| Title | **NTU Revision Subsections on D1** |
| Date Submitted | [January 2017] |
| Source | Hsin-Mu (Michael) Tsai, Yen-Ting Liu, Yu-Lin Wei (NTU), Rick Roberts (Intel) |
| Re: |  |
| Abstract | Text for D1 comments’ resolution  |
| Purpose | Resolution for D1 technical comments |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. |

We wish to thank Kookmin University for initiating this document thread. This document is a modification of an original document generated by Kookmin University, 15-16-0460-03-007a.

# #1: PHY A,B,C tables

**Table 01. PHY A operating modes**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Modulation***(phyOccMcsID)* | **RLL***(phyOccRLLCode)* | **Optical clock rate***(phyOccOpticalClockRate)* | **FEC***(phyOccFec)* | **Bit Rate** |
| **PHY A operating modes** |
| UFSOOK | NA | multiple of frame rate | MIMO path dependent | (1/2)\*(code rate)\*Frame Rate) |
| Twinkle VPPM | NA | 4x bit rate | RS(15, 11) | 4 kbps |
| S2-PSK | Differential code | 10 Hz  | Temporal error correction | 5 bps |
| S8-PSK | Grey code | 10 Hz | Temporal error correction | 30 bps |
| HS-PSK | ½ code rate for S2-PSK; none for DS8-PSK | 10 kHz | Temporal error correction;Outer FEC with GF(16)  | 22 kbps |
| **PHY B operating modes** |
| NS-FSK | None | 30 Hz | XOR FEC | 60/90 bps |
| C-OOK | Manchester/ 4B6B | 2.2 kHz/ 4.4 kHz | Temporal error correction(DS rate=100/ DS rate=60) | 60/150/580/700 bps |
| CM-FSK | None | 10 Hz | Temporal error correction | 40/50/60bps |
| Packet PWM/PPM | None | 100 kHz | Temporal error correction | 5.5/ 8 kbps |
| **PHY C operating modes** |
| A-QL | None | 10 Hz | Hamming (11,15)/ None | 5.28/ 7.56 kbps(16x16 cells) |
| HA-QL | Differential code | 10 Hz | Hamming (11,15)/ None | 220/ 300 bps(8x8 cells) |
| VTASC | None |  |  |  |
| Invisible data embedded | None |  |  |  |

# #4: PHY constants and attributes table

**Table 188- PHY PIB attributes**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Attribute** | **Ident.** | **Type** | **Range** | **Description** |
| phyOccMcsID | - | Int. | 0-TBD | This attribute identifies the OCC modulation.0: S2-PSK1: S8-PSK2: HS-PSK3: C-OOK4: CM-FSK5: A-QL6: Hidden A-QL (HA-QL)7: NS-FSK8-TBD: Reserved |
| phyOccOpticalClockRate | - | Int. | 0-15 | The optical clock rate (or symbol rate) applied for S2-PSK, S8-PSK, CM-FSK, and screen modulations (A-QL, and HA-QL); C-OOK; and DSM-PSK modulations respectively.0-3: 5 Hz/10 Hz/15 Hz/20 Hz4-6: 30 Hz/ 60 Hz/ 120 Hz6-8: Reserved9-10: 2.2 kHz/ 4.4 kHz11-12: 10 kHz/ 50 kHz13-14: Reserved15: Use the value specified in phyOccCustomOpticalClockRate |
| phyOccCustomOpticalClockRate |  | float |  | Custom optical clock rate, used when phyOccOpticalClockRate = 15 |
| phyOccDim  | - | Int. | 0-1000 | Refer to *phyDim* (0x02 Identifier), IEEE 802.15.7-2011 std. OCC dimming is configured in steps of TBD %. |
| phyOccRLLCode | - | Int. | 0-7 | This specifies the RLL coding corresponding to the specific OCC modulation (phyOccMcsID):In case of S2-PSK modulation, the RLL coding is 0: None 1: Differential code ½ rate Other values: ReservedIn case of S8-PSK modulation, the RLL coding is 0: None 1: 3 bits Grey code Other values: ReservedIn case of HS-PSK, the RLL coding is 0: None  1: 1/2 code rate for S2-PSK and none for DS8-PSK Other values: ReservedIn case of C-OOK modulation, the RLL coding is 0: Manchester 1: 4B6B coding Other values: ReservedIn case of CM-FSK modulation, the RLL coding is 0: None Other values: ReservedIn case of NS-FSK modulation, the RLL coding is 0: None Other values: ReservedIn case of A-QL modulation, the RLL coding is 0: None Other values: ReservedIn case of HA-QL modulation, the RLL coding is 0: None  1: Differential ½ code  Other values: Reserved |
| phyOccFec | - | Int. | 0-7 | This attribute specifies FEC corresponding to the specific OCC modulation (phyOccMcsID):In case of S2-PSK modulation, 0: None Other values: ReservedIn case of S8-PSK modulation, 0: None Other values: ReservedIn case of HS-PSK modulation, 0: None for both S2-PSK and DS8-PSK 1: None for S2-PSK and RS (15, 11) for DS8-PSK Other values: ReservedIn case of C-OOK modulation, 0: Temporal repeating code DS rate=100 1: Temporal repeating code DS rate=60 Other values: ReservedIn case of CM-FSK modulation, 0: None Other values: ReservedIn case of NS-FSK modulation 0: XOR FEC Other values: ReservedIn case of A-QL modulation, 0: None 1: Hamming (11,15) Other values: ReservedIn case of HA-QL modulation, 0: None 1: Hamming (11,15) Other values: Reserved |
| Below PHY attributes shall be present if phyOccMcsID = 0 (i.e. S2-PSK modulation). |
| phyS2pskNoLightSources | - | Int. | 0-3 | The number of light sources used to modulate S2-PSK signal.0: two light sources1-3: Reserved |
| phyS2pskModulationRate | - | Int. | 0-7 | This attribute specifies the modulation frequency used for S2-PSK.0: 200 Hz1: 125 Hz2-7: Reserved |
| Below PHY attributes shall be present if phyOccMcsID = 1 (i.e. S8-PSK modulation). |
| phyS8pskNoLightSources | - | Int. | 0-3 | The number of light sources used to modulate S8-PSK signal.0: two light sources, each consists of 4 LEDs.1: four light sources, each consists of 4 LEDs (4x4 Digital Signage Tx).2-3: Reserved |
| phyS8pskModulationRate | - | Int. | 0-7 | This attribute specifies the modulation frequency used for S8-PSK.0: 800 Hz1-7: Reserved |
| Below PHY attributes shall be present if phyOccMcsID = 2 (i.e. HS-PSK modulation). |
| phyHSpskNoLightSources | - | Int. | 0-7 | The number of light sources used to modulate HS-PSK signal.0: two light sources, each consists of 8 LEDs.1: two light sources, each consists of 10 LEDs.1-7: Reserved |
| phyHSpskHighStreamMode | - | Int. | 0-7 | The modulation of high data stream.0: DS8-PSK mode1: DS10-PSK mode2-7: Reserved |
| phyHSpskModulationRate | - | Int. | 0-7 | This attribute specifies the modulation frequency used for S2-PSK and DSM-PSK of HS-PSK.0: 200Hz for S2-PSK and 80 kHz for DS8-PSK1: 200Hz for S2-PSK and 400 kHz for DS8-PSK2-7: Reserved |
| phyHSpskPsduLength | - | Int. | TBD | This is to specify the length of the high-speed link of HS-PSK.TBD |
| Below PHY attributes shall be present if phyOccMcsID = 3 (i.e. C-OOK modulation). |
| phyCookDSrate | - | Int. | 0-7 | This attribute specifies the data sub-frame rate (DS rate) of C-OOK.0: 60 DS/sec1: 100 DS/sec2-7: Reserved |
| phyCookSFsymbol | - | Int. | 0-7 | This attribute specifies the SF symbol of PSDU of C-OOK.0: 6B symbol1: 10B symbol2-3: Reserved |
| phyCookAb | - | Int. | 0-3 | This attribute specifies the amount of Asynchronous bit (Ab) per data sub-frame of C-OOK.0: 1 bit1: 2 bit2-3: Reserved |
| Below PHY attributes shall be present if phyOccMcsID = 4 (i.e. CM-FSK modulation). |
| phyCmfskNoFrequency | - | Int. | 0-3 | This attribute specifies the number of frequencies used to modulate data in CM-FSK.0: 32-FSK1: 64-FSK2-3: Reserved |
| phyCmfskFrequencySeparation | - | Int. | 0-7 | This attribute specifies the frequency separation in CM-FSK.0: 50 Hz1: 100 Hz2-7: Reserved |
| phyCmfskNoPhase | - | Int. | 0-3 | This attribute specifies the number of phases used to modulate data in CM-FSK.0: None1: 2-PSK2-3: Reserved |
| phyCmfskPreamble1 | - | Int. | 0-3 | This attribute specifies the frequency value of the first preamble in CM-FSK.0: 200Hz1-3: Reserved |
| phyCmfskSplitterEnable | - | Boolean | T/F | This attribute enables whether the splitter usage in between frequency symbols in CM-FSK.FALSE: Disable (Default)TRUE: Enable |
| Below PHY attributes shall be present if phyOccMcsID = 5 (i.e. A-QL modulation). |
| phyAqlNoCells | - | Int. | 0-7 | The number of individual cells on Tx in A-QL mode.0: 16x16 cells1-7: Reserved |
| phyAqlNoCellReference | - | Int. | 0-3 | The number of cells per each of four reference corners in A-QL mode.0: 1 cell reference1: 2x2 cell reference2-3: Reserved |
| phyAqlByteOrientedEnable | - | Boolean | T/F | The enabler of byte-oriented mode in A-QL mode.FALSE: Disable (bit-oriented)TRUE: Enable (byte-oriented) |
| phyAqlNoColors | - | Int. | 0-3 | The number of colors used in A-QL mode.0: Grey marking (no color)1: 2 colors2: 4 colors3: 8 colors |
| phyAqlPsduLength | - | Int. | TBD | This is to specify the length of PSDUTBD |
| Below PHY attributes shall be present if phyOccMcsID = 6 (i.e. HA-QL modulation). |
| phyHAqlNoCells | - | Int. | 0-7 | The number of individual cells on Tx in HA-QL mode.0: 8x8 cells1: 16x16 cells2-7: Reserved |
| phyHAqlNoCellReference | - | Int. | 0-3 | The number of cells per each of four reference corners in HA-QL mode.0: 1 cell reference1-3: Reserved |
| phyHAqlByteOrientedEnable | - | Boolean | T/F | The enabler of byte-oriented mode in HA-QL mode.FALSE: Disable (bit-oriented)TRUE: Enable (byte-oriented) |
| Below PHY attributes shall be present if phy OccMcsID = 7 |
| phyNsfskInvFrequencyGap |  | int | 0-3 | Indicates the frequency differences between the frequency sets. This is represented by the inverse of frequency gap. i.e. the time difference in seconds.0: 3.75e-41-2: Reserved3: Use the value specified in phyOccCustomOpticalClockRate |
| phyNsfskCustomInvFrequencyGap |  | float |  | Custom inverse frequency gap, used when phyNsfskInvFrequencyGap = 3 |
| phyNsfskGroupCount |  | int | 0-7 | Indicates the maximum sequence number. i.e., how many frequency sets exist.N: n+1 frequency set |
| phyNsfskFEC |  | int | 0-7 | Indicates the number of data symbols protected by one XOR FEC symbol.N: n+1 symbols |
| phyNsfskSplitterSymbolEnable |  | boolean | T/F | Indicates whether the device uses SSs or not. |
| phyNsfskSplitterFrequency |  | int | 0-3 | Indicates the splitter frequency. This is represented as a ratio of the splitter frequency to the preamble frequency. If the SS is already in used, it will use the original phyNsfskSplitterFrequency until next cycle.0: 1.41-2: Reserved3: Custom |
| phyNsfskCustomSplitterFrequency |  | float |  | Custom splitter frequency, used when phyNsfskSplitterFrequency = 3­ |
| phyNsfskSplitterDuration |  | int | 0-7 | Indicates the duration of the SS. This is represented as a ratio of symbol duration to splitter duration in integer.0: 151: 302: 603: 1204-7: Reserved |
| phyNsfskSymbolDurationExp |  | int | 0-7 | Indicates the duration of a data symbol in the PSDU. This is represented as a ratio of the symbol duration to 1/30 second in the base 2 exponentiation. For example, if the symbol duration is 1/120 second, then the exponent would be -2. Note that this does not affect the duration of the preamble field and the optional field.0: 01: 12: 23: -14: -25-6: Reserved7; Custom |
| phyNsfskEndSymbolEnable |  | boolean | T/F | Indicates whether the device uses end symbol or not. |