**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) |
| Title | **D3 Comments Resolution Based PHY PIB Attributes Revision** |
| Date Submitted | August, 2017 |
| Source | Jaesang Cha (SNUST), Minwoo Lee (SNUST), Soonho Jung (SNUST), Kim Chan (SNUST), Ilkyoo Lee (Kongju Nat’Univ.), Gilsik Lee (The Univ. of Texas at Dallas), Sooyoung Chang (CSUS) , Vinayagam Mariappan (SNUST) | Voice: [ ]Fax: [ ]E-mail: [chajs@seoultech.ac.kr]1 |
| Re: | PHY PIB attributes specification revision to Use of over-the-air PHY frame configuration is forbidden for PHY types IV, V and VI |
| Abstract | Details of Resolutions regarding to the submitted Comments on D3 are suggested for PHY PIB Attributes Specification Revision to use of over-the-air PHY frame configuration is forbidden for PHY types IV, V and VI. The proposed method is designed to operate on the application services like LED ID using Color/QR Code, etc, LBS, Emergency EXIT Signage, LED-IT and Digital Signage with Advertisement Information etc. |
| Purpose | D3 Comments Resolutions and Editorial Revision. |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. |

**I. PHY TYPE IV PHY PIB Attributes**

# **1. PHY PIB Attributes for Offset-VPWM**

The PHY PIB attributes for Offset-VPWM is presented in the Table 179 —PHY PIB attributes (continued for Offset-VPWM).

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Attribute** | **Identifier** | **Type** | **Range** | **Description** |
| phySMFlashLIGHTApplicationSpecificMode | 0x10 | Unsigned | 0~255 | This attribute specifies the application specific PHY mode.0 : Normal Data (Media Content, Information Content based on the Application used)1 : ID Data 2 : Authentication Data |
| phyOffsetVPWMStdPERIOD | 0x11 | Integer | 0-65535 | This attribute specify the standard PWM period used to transmit the data (in micro secs) |
| phyOffsetVPWMOffsetPERIOD | 0x12 | Integer | 0-65535 | This attribute specify the Variable offset PWM period used to transmit the data (in micro secs) |

Table 179 — PHY PIB attributes (continued for OffsetVPWM)

**II. PHY TYPE VI PHY PIB Attributes**

# **1. PHY PIB Attributes for VTASC**

The PHY PIB attributes for VATSC is presented in the Table 179 —PHY PIB attributes (continued for VTASC).

|  |
| --- |
| **PHY PIB Table 188 Additions** |
| **Attribute** | **Identifier** | **Type** | **Range** | **Description** |
| phyVTASCTxMode | 0x10 | Unsigned | 0-255 | This attribute indicates the VTASC PHY transmission modes.0 : VTASC Mode1 : SS VTASC Mode |
| phyVTASCApplicationSpecificMode | 0x10 | Unsigned | 0~255 | This attribute specifies the application specific PHY mode.0 : Normal Data (Media Content, Information Content based on the Application used for)1 : LED ID Data 2 : Authentication Data |
| phyVTASCTxCamerEnable | 0x92 | Unsigned | 0-255 | This attribute indicates the Transmitter is Enabled with Camera or not for Interactive Receiver distance specific data transfer control.0 : Camera not connected1 : Camera connected |
| phyVTASCRxDistance | 0x93 | Unsigned | 0-255 | This attribute notify the Receiver distance from Transmitter |
| PhyVTASCFreq | 0x11 | Unsigned | 0~255 | This attribute specify the frame rate of VTASC sequence Transmission |
| phyVTASCCodeArea | 0x12 | Unsigned | 0~255 | This attribute specify the coded area of the IDE0 : Full Screen1 : Partial Screen2~255 : Reserved |
| phyVTASCCodeLocation | 0x13 | Unsigned | 0~255 | This attribute specify the Coded Location of the VTASC0 : Center1 : Bottom Right2 : Bottom Left3 : Top Right4 : Top Left5~255 : Reserved |
| phyVTASCTLevel | 0x14 | Unsigned | 0~255 | This attribute specify the transparency Level of the VTASC |
| phyVTASCALevel | 0x14 | Unsigned | 0~255 | This attribute specify the block size of the VTASC |
| phyVTASCSLevel | 0x14 | Unsigned | 0~255 | This attribute specify the no of shapes used in the VTASC |
| phyVTASCCLevel | 0x14 | Unsigned | 0~255 | This attribute specify the no of colors used in the VTASC |
| phyVTASCSModel | 0x17 | Unsigned | 0~255 | This attribute specify the block shape Type used in the VTASC0 : Square1 : Circle3 : hexagon4 : star5~65535 : Reserved |
| phyVTASCAHSize | 0x15 | Unsigned | 0~255 | This attribute specify the no of Horizontal Blocks in the VTASC |
| phyVTASCAVSize | 0x16 | Unsigned | 0~255 | This attribute specify the no of Vertical Blocks in the VTASC |
| phyVTASCScalRateCtrl | 0x18 | Unsigned | 0~255 | This attribute specify the Scalable Rate control mode0 : No Scalable Bitrate control1 : Multirate Scalable Controller2: Distance Adaptive Scalable Controller3: Distance adaptive with multirate scalable controller |
| phyVTACScalRegion1OpticalClockRate | 0x19 | Unsigned | 0~255 | This attribute specify the scalable optical clock rate of VTASC region 1 |
| phyVTACScalRegion2OpticalClockRate | 0x1A | Unsigned | 0~255 | This attribute specify the scalable optical clock rate of VTASC region 2 |
| phyVTACScalRegion3OpticalClockRate | 0x1B | Unsigned | 0~255 | This attribute specify the scalable optical clock rate of VTASC region 3 |
| phyVTACScalRegion4OpticalClockRate | 0x1C | Unsigned | 0~255 | This attribute specify the scalable optical clock rate of VTASC region4 |
| phyVTACScalRegion1DistanceRange | 0x19 | Unsigned | 0~255 | This attribute specify the distance adapted on VTASC region 1 |
| phyVTACScalRegion2DistanceRange | 0x1A | Unsigned | 0~255 | This attribute specify the distance adapted on VTASC region 2 |
| phyVTACScalRegion3DistanceRange | 0x1B | Unsigned | 0~255 | This attribute specify the distance adapted on VTASC region 3 |
| phyVTACScalRegion4DistanceRange | 0x1C | Unsigned | 0~255 | This attribute specify the distance adapted on VTASC region 4 |
| PhySSCode1Len | 0x1D | Unsigned | 0~255 | This attribute specify the spreading code length for SS Code 1 |
| PhySSCode2Len | 0x1E | Unsigned | 0~255 | This attribute specify the spreading code length for SS Code 2 |
| PhySSCode3Len | 0x1F | Unsigned | 0~255 | This attribute specify the spreading code length for SS Code 3 |
| PhySSCode4Len | 0x20 | Unsigned | 0~255 | This attribute specify the spreading code length for SS Code 4 |
| PhySSCode1FP00 | 0x21 | Integer | 0~65535 | This attribute specify the SS Code 1 pair code 0  |
| PhySSCode1FP01 | 0x22 | Integer | 0~65535 | This attribute specify the SS Code 1 pair code 1 |
| PhySSCode2FP00 | 0x23 | Integer | 0~65535 | This attribute specify the SS Code 2 pair code 0  |
| PhySSCode2FP01 | 0x24 | Integer | 0~65535 | This attribute specify the SS Code 2 pair code 1 |
| PhySSCode3FP00 | 0x25 | Integer | 0~65535 | This attribute specify the SS Code 3 pair code 0  |
| PhySSCode3FP01 | 0x26 | Integer | 0~65535 | This attribute specify the SS Code 3 pair code 1 |
| PhySSCode4FP00 | 0x27 | Integer | 0~65535 | This attribute specify the SS Code 4 pair code 0  |
| PhySSCode4FP01 | 0x28 | Integer | 0~65535 | This attribute specify the SS Code 4 pair code 1 |
| phyVTASCCValue | 0x29 | Unsigned | 0~255 | This attribute specify the no of Colors used in the VTASC |
| phyVTASCTxHSize | 0x3A | Integer | 0-65535 | This attribute specify the no of Horizontal Pixel in the 2D Display Transmitter |
| phyVTASCTxVSize | 0x3B | Integer | 0-65535 | This attribute specify the no of Vertical Pixel in the 2D Display Transmitter |

Table 179 — PHY PIB attributes (continued for VTASC)

# **2. PHY PIB Attributes for SS2DC**

The PHY PIB attributes for SS2DC is presented in the Table 179 —PHY PIB attributes (continued for SS2DC).

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Attribute** | **Identifier** | **Type** | **Range** | **Description** |
| phySS2DCTxMode | 0x10 | Unsigned | 0-255 | This attribute indicates the Sequential Scalable 2D Code PHY transmission modes.0 : SS2DC Mode1 : SS SS2DC Mode |
| PhySS2DCApplicationSpecificMode | 0x10 | Unsigned | 0~255 | This attribute specifies the application specific PHY mode.0 : Normal Data (Media Content, Information Content based on the Application used for)1 : ID Data 2 : Authentication Data |
| phySS2DCTxCamerEnable | 0xA2 | Unsigned | 0-255 | This attribute indicates the Transmitter is Enabled with Camera or not for Interactive Receiver distance specific data transfer control.0 : Camera not connected1 : Camera connected |
| phySS2DCRxDistance | 0xA3 | Unsigned | 0-255 | This attribute notify the Receiver distance from Transmitter |
| PhySS2DCCodeArea | 0x11 | Unsigned | 0~255 | This attribute specify the coded area of the IDE0 : Full Screen1 : Partial Screen2~255 : Reserved |
| PhySS2DCCodeLocation | 0x12 | Unsigned | 0~255 | This attribute specify the Coded Location of the SS2DC0 : Center1 : Bottom Right2 : Bottom Left3 : Top Right4 : Top Left5~255 : Reserved |
| phySS2DCTHSize | 0x13 | Unsigned | 0~255 | This attribute specify the no of horizontal blocks in the SS2DC |
| phySS2DCTVSize | 0x14 | Unsigned | 0~255 | This attribute specify the no of vertical blocks in the SS2DC |
| PhySS2DCCODEHSIZE | 0x15 | Unsigned | 0~255 | This attribute specify the horizontal size of the 2D code in the SS2DC |
| PhySS2DCCODEVSIZE | 0x16 | Unsigned | 0~255 | This attribute specify the vertical size of the 2D code in the SS2DC |
| phySS2DCTFrequency | 0x17 | Unsigned | 0~255 | This attribute specify the frame rate of SS2DC sequence Transmission  |
| PhySS2DCTxHSize | 0x18 | Integer | 0-65535 | This attribute specify the no of Horizontal Pixel in the 2D Display Transmitter |
| PhySS2DCTxVSize | 0x19 | Integer | 0-65535 | This attribute specify the no of Vertical Pixel in the 2D Display Transmitter |

Table 179 — PHY PIB attributes (continued for SS2DC)

# **3. PHY PIB Attributes for IDE**

The PHY PIB attributes for IDE is presented in the Table 179 —PHY PIB attributes (continued for IDE).

|  |
| --- |
| **PHY PIB Table 100 Additions** |
| **Attribute** | **Identifier** | **Type** | **Range** | **Description** |
| phyIDETxMode | 0x10 | Unsigned | 0-255 | This attribute indicates the Invisible Data Embedding transmission modes.0 : IDE-BLENDING1 : IDE-WATERMARK 2 : SS IDE-BLEND3 : SS IDE-WATERMARK  |
| phyIDEApplicationSpecificMode | 0x11 | Unsigned | 0~255 | This attribute specifies the application specific PHY mode.0 : Normal Data (Media Content, Information Content based on the Application used for)1 : ID Data 2 : Authentication Data3~255: Reserved |
| phyIDETxCamerEnable | 0x12 | Unsigned | 0-255 | This attribute indicates the Transmitter is Enabled with Camera or not for Interactive Receiver distance specific data transfer control.0 : Camera not connected1 : Camera connected |
| phyIDERxDistance | 0x13 | Unsigned | 0-255 | This attribute notify the Receiver distance from Transmitter |
| phyIDEModulation | 0x14 | Unsigned | 0~255 | This attribute specifies the modulation.0 : M-FSK1 : HYBRID-MPFSK 2 : 2D Binary Code3~255: Reserved |
| phyIDENoFrequency | 0x15 | Unsigned | 0~255 | This attribute specifies the number of frequency used in M-FSK and Hybrid-MPFSK |
| phyIDENoPhase | 0x16 | Unsigned | 0~255 | This attribute specifies the number of phase used in Hybrid-MPFSK |
| phyIDEFreqBase | 0x15 | Unsigned | 0~255 | This attribute specifies the base frequency used in M-FSK and Hybrid-MPFSK |
| phyIDEFreqSeparation | 0x16 | Unsigned | 0~255 | This attribute specifies the frequency difference used in M-FSK and Hybrid-MPFSK |
| phyIDEPhaseBase | 0x15 | Unsigned | 0~255 | This attribute specifies the base Phase used in Hybrid-MPFSK |
| phyIDEPhaseSeparation | 0x16 | Unsigned | 0~255 | This attribute specifies the Phase difference used in Hybrid-MPFSK |
| phyIDECodedArea | 0x17 | Unsigned | 0~255 | This attribute specify the coded area of the IDE0 : Full Screen1 : Partial Screen2~255 : Reserved |
| phyIDECodedLocation | 0x18 | Unsigned | 0~255 | This attribute specify the Coded Location of the IDE0 : Center1 : Bottom Right2 : Bottom Left3 : Top Right4 : Top Left5~255 : Reserved |
| phyIDEHSize | 0x19 | Integer | 0-65535 | This attribute specify the no of horizontal pixel in the display  |
| phyIDEVSize | 0x1A | Integer | 0-65535 | This attribute specify the no of vertical Pixel in the display  |
| phyIDEENCHozAreaSize | 0x1B | Integer | 0-65535 | This attribute specify the no of horizontal pixel area to Encode  |
| phyIDEENCVerAreaSize | 0x1C | Integer | 0-65535 | This attribute specify the no of horizontal pixel area to Encode |
| phyIDEMxNBlockSize | 0x1D | Unsigned | 0~255 | This attribute specify the no of Horizontal pixels in Blocks in the IDE0 – 16x16 pixels1 – 32x32 pixels2 – 64x64 pixels3~255: Reserved |
| phyIDEFrequency | 0x1E | Unsigned | 0~255 | This attribute specify the frame rate of IDE sequence Transmission  |
| PhyIDETxHSize | 0x1F | Integer | 0-65535 | This attribute specify the no of Horizontal Pixel in the 2D Display Transmitter |
| PhyIDETxVSize | 0x20 | Integer | 0-65535 | This attribute specify the no of Vertical Pixel in the 2D Display Transmitter |

Table 179 - PHY PIB attributes (continued for IDE)