**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) |
| Title | **OCC operating modes - table** |
| Date Submitted | [September 2017] |
| Source | Trang Nguyen, and Yeong Min Jang (Kookmin University) |
| Re: |  |
| Abstract | Discussion on D4 comments’ resolution |
| Purpose | Resolution for D4 technical comments |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. |

# #1: PHY A,B,C tables

**Table 81. PHY IV, V, and VI operating modes**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| ***phyOccMcsID*** | **Modulation** | **RLL** | **Optical clock rate** | **FEC** | **Bit Rate** |
|  | **PHY IV operating modes** | | | | |
| 1 | UFSOOK | None | multiple of frame rate | MIMO path dependent | (1/2)\*(code rate)\*(Frame Rate) |
| 2 | Twinkle VPPM | None | 4x bit rate | RS(15, 11) | 4 kbps |
| 3 | S2-PSK | Half-rate code | 10 Hz | Temporal error correction | 5 bps |
| 4 | HS-PSK | Half-rate code for S2-PSK | 10 kHz | RS(15,7) | 22 kbps |
| 5 | Offset VPPM | None | 25 Hz | R(15,2)/RS(15,4)/None | 18bps |
|  | **PHY V operating modes** | | | | |
| 6 | NS-FSK | None | 30 Hz | XOR FEC | 60/90 bps |
| 7 | C-OOK | Manchester/ 4B6B | 2.2 kHz/ 4.4 kHz | Inner Hamming code,  Optional outer RS(15,11) | 40/110/220/400 bps |
| 8 | CM-FSK | None | 10 Hz | Optional outer RS(15,11) | 50/60/70  bps |
| 9 | MPM | None | 25 kHz | Temporal error correction | 5/ 8 kbps |
|  | **PHY VI operating modes** | | | | |
| 10 | A-QL | None | 10 Hz | Outer RS(15,11),  Inner CC(1/4) | 1.32/ 5.54 kbps |
| 11 | HA-QL | Half-rate code | 10 Hz | Outer RS(15,7), Inner CC(1/4) | 140 bps |
| 12 | VTASC | None | 30 Hz | RS(64,32)/RS(160,128)/None | 512 kbps |
| 13 | SS2DC | None | 30 Hz | RS(64,32)/RS(160,128)/None | 368 kbps |
| 14 | IDE | None | 30 Hz | RS(64,32)/RS(160,128)/None | 32 kbps |

**TBD:**

* Should we have the column of *phyOccMscID*. If yes, The TG7m committee will assign the ID.