**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |  |
| --- | --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) | |
| Title | **Proposal of FSK LECIM PHY extension** | |
| Date Submitted | [“07 September, 2018”] | |
| Source | [Thang Nguyen, Yeong Min Jang, Sangsung Choi] [Kookmin University, Woosong University] | Voice: [ ] Fax: [ ] E-mail: [yjang@kookmin.ac.kr] |
| Re: |  | |
| Abstract | [Propose to add a new lower data-rate and a narrow band FSK PHY for new spectrum in Korea.] | |
| Purpose | [Extend the IEEE 802.15.4k standard.] | |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. | |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. | |

1. **PPDU format for GFSK PHY**

The GFSK PPDU format shall support the same format in FECIM FSK PHY



Figure 1: Format of the LECIM FSK PPDU

1. **Modulation and coding for GFSK PHY**

The modulation for the LECIM FSK PHY shall be FSK or position-based FSK (P-FSK).

In the 262~264MHz band, the modulation index shall be as follows:

* 2.0 for 2.4 kb/s
* 1.0 for 4.8 kb/s

12.5 kHz channel spacing may be used as permitted by local regulations

In the 169 MHz band, the modulation index shall be as follows:

* 0.5 for 25 kb/s
* 1.0 for 12.5 kb/s

For all other LECIM FSK PHY band identifiers, the modulation index shall be as follows:

* 0.5 for 37.5 kb/s
* 1.0 for 25 kb/s
* 2.0 for 12.5 kb/s
* 2.0 for 6.25Kb/s

Either 100 kHz or 200 kHz channel spacing may be used as permitted by local regulations.

1. **Spreading**

The use of spreading is controlled by the PIB attribute *phyLecimFskSpreading*, as defined in 11.3. The spreading factor (SF) can be 1, 2, 4, 8, or 16. The variable SF is indicated by the PIB attribute *phyLecimFskSpreadingFactor*, as defined in 11.3.

For spreading, a single input bit (b0) is mapped into the spreading bits (c0, c1, …, cSF-1)

Apply sequence spreading scheme to improve SFD detection performance and maintain SHR at a level similar to the reliability of PHR and PSDU



Figure 2: Spreading procedure

We suggest three spreading factor (SF) 2, 4 and 8 to reduce transmission overhead due to extended synchronization header with SFD sequence spreading as shown. The input SFD sequence bits to SFD spreading bits mapping as shown in Table 1.

Table 1: Input to spreading bit mapping

|  |  |  |
| --- | --- | --- |
|  | Input bit  = 0 | Input bit  = 1 |
| SF = 2 | = 01 | = 10 |
| SF = 4 | = 0101 | = 1010 |
| SF = 8 | = 11010100 | = 00101011 |