**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) |
| Title | **Resolution to CID r2-0337** |
| Date Submitted | [17 October, 2019] |
| Source | Billy Verso (Decawave)  Frank Leong (NXP Semiconductors) |
| Re: | [If this is a proposed revision, cite the original document.]  [If this is a response to a Call for Contributions, cite the name and date of the Call for Contributions to which this document responds, as well as the relevant item number in the Call for Contributions.]  [Note: Contributions that are not responsive to this section of the template, and contributions which do not address the topic under which they are submitted, may be refused or consigned to the “General Contributions” area.] |
| Abstract | [Resolution to 802.15.4z comment CID r2-0337] |
| Purpose | [Resolve 802.15.4z comment CID r2-0337] |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. |

**This document provides a resolution to comment r2-0337.**

***In 7.4.4.43, replace Figure 65 as follows:***

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Bits: 1 | 1 | 1 | 1 | 1 | 1 | 1 | 1 | Octets: 1 | Variable |
| Address Present | Reply Time Present | Round-trip Time Present | TOF Present | AOA Azimuth Present | AOA Elevation Present | AOA FOM Present | Deferred Mode | RMI List Length | RMI List |

**Figure 65 - RMI IE Content field format**

***In 7.4.4.43, on Page 95, add the following after Line 22:***

The AOA FOM Present field when one indicates that the AOA Azimuth FOM field is present in each RMI List element if the AOA Azimuth field is present and that the AOA Elevation FOM field is present in each RMI List element if the AOA Elevation field is present, or when zero that neither the AOA Azimuth FOM field nor the AOA Elevation FOM field are present.

***In 7.4.4.43, replace Figure 66 as follows:***

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Octets: 0/4 | 0/4 | 0/4 | 0/2 | 0/1 | 0/2 | 0/1 | 0/2/8 |
| RX-to-TX Reply Time | TX-to-RX Round-trip Time | TOF | AOA Azimuth | AOA Azimuth FOM | AOA Elevation | AOA Elevation FOM | Address |

**Figure 66 - RMI List element format**

***In 7.4.4.43, on Page 96, add the following after Line 13:***

The AOA Azimuth FOM field is an unsigned integer that conveys the reliability of the estimated AOA in the azimuth. Higher AOA Azimuth FOM value is better, and AOA Azimuth FOM value zero means invalid AOA Azimuth estimate.

***In 7.4.4.43, on Page 96, add the following after Line 16:***

The AOA Elevation FOM field is an unsigned integer that conveys the reliability of the estimated AOA in the elevation. Higher AOA Elevation FOM value is better, and AOA Elevation FOM value zero means invalid AOA Elevation estimate.

In order for the AOA Azimuth FOM value and AOA Elevation FOM value to be meaningful, the AOA capabilities of the measuring device including details of its antenna array setup need to be known. Agreeing and communicating these system parameters is beyond the scope of this standard. Out-of-band mechanisms as well as custom messages can be used for this purpose.