**IEEE 802.15**

**Wireless Speciality Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Specialty Networks (WSNs) |
| Title | Proposal for revised tables on EVM and Rx Sensitivity Levels in Chapter 15 in 802.15.3RevB |
| Date Submitted | 14 November 2022 |
| Source | Thomas KürnerTU BraunschweigSchleinitzstr. 2238092 Braunschweig, Germany | Voice: +49 531 391 2416Fax: +49 531 391 5192E-mail: t.kuerner@tu-bs.de |
| Re: |  |
| Abstract | Proposal for revised tables on EVM and Rx Sensitivity Levels in Chapter 15 in 802.15.3RevB |
| Purpose | Resolving comments of LB191 |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. |

**Proposal for revised tables on EVM and Rx Sensitivity Levels in Chapter 15 in 802.15.3RevB**

**Starting Point:**

EVM values in Table 15-13 for the new MCS have been taken from "doc.15-22-0431-01-03ma-AWGN Simulation Results for new MCS". These simulations have been derived with a slighlty different method compared to the method used in deriving the values in IEEE Std 802.15.3d-2017 giving slightly different values for the already existing MCSs as shown in the above mentioned document. This gives inconsistent results across MCSs and has also an impact on the Reference sensitivity levels in tables 15-14 and 15-19.

**Proposed new tables**

**Table 15-14 Max EVM**

|  |  |  |  |
| --- | --- | --- | --- |
| MCS Identifier | Modulation | FEC Rate | Max. EVM (dB) |
| 0 | BPSK | 11/15 | -6 |
| 1 | BPSK | 14/15 | -7 |
| 2 | QPSK | 11/15 | -9 |
| 3 | QPSK | 14/15 | -10 |
| 4 | 8-PSK | 11/15 | -13 |
| 5 | 8-PSK | 14/15 | -15 |
| 6 | 8-APSK | 11/15 | -12 |
| 7 | 8-APSK | 14/15 | -15 |
| 8 | 16-QAM | 11/15 | -14 |
| 9 | 16-QAM | 14/15 | -17 |
| 10 | 64-QAM | 11/15 | -21 |
| 11 | 64-QAM | 14/15 | -23 |
| 12 | 16-APSK | 11/15 | -17 |
| 13 | 16-APSK | 14/15 | -22 |
| 14 | 32-APSK | 11/15 | -19 |
| 15 | 32-APSK | 14/15 | -23 |

**Table 15-14 Reference sensitivity levels for MCS for the THz-SC PHY**

|  |  |  |  |
| --- | --- | --- | --- |
| MCS Identifier | Modulation | FEC Rate | Receiver Sensitivity (dBm) depending on the bandwidth |
| 2.16 GHz | 4.32 GHz | 8.64 GHz | 12.96 GHZ | 17.28 GHZ | 25.92 GHz | 34.56 GHz | 51.84 GHz | 69.12 GHz |
| 0 | BPSK | 11/15 | -67 | -63 | -60 | -57 | -55 | -54 | -52 | -51 | -49 |
| 1 | BPSK | 14/15 | -64 | -62 | -59 | -56 | -53 | -52 | -50 | -49 | -47 |
| 2 | QPSK | 11/15 | -64 | -60 | -57 | -54 | -51 | -50 | -48 | -47 | -45 |
| 3 | QPSK | 14/15 | -61 | -59 | -56 | -53 | -50 | -49 | -47 | -46 | -44 |
| 4 | 8-PSK | 11/15 | -59 | -56 | -53 | -50 | -47 | -46 | -44 | -43 | -41 |
| 5 | 8-PSK | 14/15 | -56 | -54 | -51 | -48 | -45 | -44 | -42 | -41 | -39 |
| 6 | 8-APSK | 11/15 | -59 | -57 | -54 | -51 | -48 | -47 | -45 | -44 | -42 |
| 7 | 8-APSK | 14/15 | -56 | -54 | -51 | -48 | -45 | -44 | -42 | -41 | -39 |
| 8 | 16-QAM | 11/15 | -57 | -55 | -52 | -49 | -46 | -45 | -43 | -42 | -40 |
| 9 | 16-QAM | 14/15 | -54 | -52 | -49 | -46 | -43 | -42 | -40 | -39 | -37 |
| 10 | 64-QAM | 11/15 | -52 | -48 | -45 | -42 | -39 | -38 | -36 | -35 | -33 |
| 11 | 64-QAM | 14/15 | -48 | -46 | -43 | -40 | -37 | -36 | -34 | -33 | -31 |
| 12 | 16-APSK | 11/15 | -70 | -52 | -49 | -46 | -43 | -42 | -40 | -39 | -37 |
| 13 | 16-APSK | 14/15 | -70 | -47 | -44 | -41 | -38 | -37 | -35 | -34 | -32 |
| 14 | 32-APSK | 11/15 | -70 | -50 | -47 | -44 | -41 | -40 | -38 | -37 | -35 |
| 15 | 32-APSK | 14/15 | -70 | -46 | -43 | -40 | -37 | -36 | -34 | -33 | -31 |

**Table 15-19 Reference sensitivity levels for MCS for the THz-OOK PHY**

|  |  |  |  |
| --- | --- | --- | --- |
| MCS Identifier | Modulation | FEC Rate | Receiver Sensitivity (dBm) depending on the bandwidth |
| 2.16 GHz | 4.32 GHz | 8.64 GHz | 12.96 GHZ | 17.28 GHZ | 25.92 GHz | 34.56 GHz | 51.84 GHz | 69.12 GHz |
| 0 | OOK | 224/240 | -62 | -59 | -56 | -54 | -53 | -51 | -50 | -48 | -47 |
| 1 | OOK | 14/15 | -65 | -62 | -59 | -57 | -56 | -54 | -53 | -51 | -50 |
| 2 | OOK | 11/15 | -62 | -59 | -56 | -54 | -53 | -51 | -50 | -48 | -47 |