**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |  |
| --- | --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) | |
| Title | **Proposed Resolution for Comments #152** | |
| Date Submitted | May 15, 2024 | |
| Sources | Carlos Aldana (Meta) |  |
| Re: |  | |
| Abstract |  | |
| Purpose | To propose resolution to comment with CID #152 for “P802.15.4ab™/Draft (pre-ballot) C Draft Standard for Low-Rate Wireless Networks” | |
| Notice | This document does not represent the agreed views of the IEEE 802.15 Working Group or IEEE 802.15.4ab Task Group. It represents only the views of the participants listed in the “Sources” field above.It is offered as a basis for discussion and is not binding on the contributing individuals. The material in this document is subject to change in form and content after further study. The contributors reserve the right to add, amend or withdraw material contained herein. | |

***Comment Index #152***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Benjamin Rolfe | 152 | 134 | 10.40.3 A | 23 | "shall not" again (incorrect use of normative language). | Change to: A controlee shall send the HRP UWB Association Request command in a block when the Association Availability field is set to one. |

**Discussion**: The current text in Draft C can be improved by including the suggested change as well as fixing other parts.

**Proposed Resolution: REVISED**

Change lines 18-24 to the following:

A controller indicates its availability for associations with new controlees by setting the Association Availability field in the AC IE. A controlee shall send the HRP UWB Association Request command in a block when the Association Availability field is set to one. The HRP UWB Association Request command shall be sent in the slots specified by the Contention Slots Info field in the AC IE, described in 10.39.7.1. If the Contention Slots Info field is not present in the AC IE, the HRP UWB Association Request command may be sent in any unscheduled slot in the round.