**IEEE P802.15**

**Wireless Specialty Networks**

|  |  |  |
| --- | --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Specialty Networks (WSNs) | |
| Title | Miscellaneous Comments, Part 2 | |
| Date Submitted | 14-November-2024 | |
| Source | [Benjamin Rolfe] [Blind Creek Associates]  [Benjamin A. Rolfe]  [BCA] | E-mail: [ben.rolfe @ ieee.org ] |
| Re: | Resolving comments form LB207 | |
| Abstract | Proposed resolutions to CIDs | |
| Purpose | Make the world better by encouraging adoption and productive use of 802.15 standards based on accurate information | |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. | |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. | |

# Introduction

This document addresses the following comments:

Comments:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Page** | **Sub-clause** | **Line #** | **Comment** | **Proposed Change** |
| 283 | 15 | 6.6.3.3 | 25 | Why there is need for specific macEmdevImmAckAifsPeriod? The HRP-EMDEV will always use this different values regardless of mode (i.e., the high-rate pulse repetition frequency UWB PHY based enhanced modulations device will always use this) so it can be just be configured in the macSifsPeriod. | Or is it trying to say that high-rate pulse repetition frequency UWB PHY based enhanced modulations devices sometimes use this macEmdevImmAckAifsPeriod and sometimes uses macSifsPeriod? The HRP-EMDEV is device property, not a mode inside the device. Is the HRP-EMDEV supposed to be mode for devices not a device type itself? |
|  |  |  |  |  |  |

# Resolutions

## CID 283

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 283 | 15 | 6.6.3.3 | 25 | Why there is need for specific macEmdevImmAckAifsPeriod? The HRP-EMDEV will always use this different values regardless of mode (i.e., the high-rate pulse repetition frequency UWB PHY based enhanced modulations device will always use this) so it can be just be configured in the macSifsPeriod. | Or is it trying to say that high-rate pulse repetition frequency UWB PHY based enhanced modulations devices sometimes use this macEmdevImmAckAifsPeriod and sometimes uses macSifsPeriod? The HRP-EMDEV is device property, not a mode inside the device. Is the HRP-EMDEV supposed to be mode for devices not a device type itself? |

Recommended resolution: Revised

Resolution detail: Change

For a HRP-EMDEV sending Imm-Ack, the AIFS shall be equal to the value of the macEmdevImmAckAifsPeriod attribute in Table 8-36. The value of AIFS is equal to macSifsPeriod for all other PHYs and modes.

To

While operating as an HRP-EMDEV, for Imm-Ack, the AIFS shall be equal to *macEmdevImmAckAifsPeriod* defined in Table 8-36. Otherwise when using the HRP PHY, value of AIFS is equal to macSifsPeriod.

Discussion: The comment reveals confusion between a device type, which is a set of capabilities, and the current operating mode. In 16.1 we state that an HRP-EMDEV shall *support* at least one of HRP-SDEV, HRP-ARDEV or HRP-LLDDEV. A “mode” would for example be HPRF mode. An HRP-EMDEV may operate several different modes, including as an HRP-ERDEV (BPRF) which according to the base standard would use the IFS timing as specified for “all other PHYs”.