|  |  |  |
| --- | --- | --- |
| Project | **IEEE 802.16 Broadband Wireless Access Working Group <**<http://ieee802.org/16>**>** | |
| Title | ***Cleanup on network access entry based on group delegate for a large number of M2M devices, Revision 0*** | |
| Date Submitted | **2012-01-06.** | |
| Source(s) | Lei Zhou, Xufeng Zheng, Hai Wang,  **China Samsung Telecom R&D Center**  Hyunjeong Kang, Jaeweon Cho, Rakesh Taori  **Samsung Electronics Co., Ltd**. | E-mail: [l.zhou@samsung.com](mailto:l.zhou@samsung.com) |
| Re: | Call for contributions for 802.16 WG Letter Ballot (#36)(IEEE 802.16.1b) | |
| Abstract | This contribution proposes to cleanup network access entry based on group delegate. | |
| Purpose | To be discussed and adopted for P802.16.1b amendment working document. | |
| Notice | *This document does not represent the agreed views of the IEEE 802.16 Working Group or any of its subgroups*. It represents only the views of the participants listed in the “Source(s)” field above. It is offered as a basis for discussion. It is not binding on the contributor(s), who reserve(s) the right to add, amend or withdraw material contained herein. | |
| Copyright Policy | The contributor is familiar with the IEEE-SA Copyright Policy <http://standards.ieee.org/IPR/copyrightpolicy.html>. | |
| Patent Policy | The contributor is familiar with the IEEE-SA Patent Policy and Procedures:  <<http://standards.ieee.org/guides/bylaws/sect6-7.html#6>> and <<http://standards.ieee.org/guides/opman/sect6.html#6.3>>.  Further information is located at <<http://standards.ieee.org/board/pat/pat-material.html>> and <<http://standards.ieee.org/board/pat>>. | |

***Cleanup on network access entry based on group delegate for a large number of M2M devices, Revision 0***

Lei Zhou, Xufeng Zheng, Hai Wang,

**China Samsung Telecom R&D Center**

Hyunjeong Kang, Jaeweon Cho, Rakesh Taori

**Samsung Electronics Co., Ltd**.

1. **Introduction**

This contribution cleans up 6.2.18.7.4.2 section on ranging code and ranging channel for M2M group related on network access entry based on group delegate.

1. **The Proposed Text in AWD**

------------------------------- Text Proposal Start ---------------------------------------------------

------------------------------- Text Proposal1 Start ---------------------------------------------------

**[*Remedy1: Add proposed text from line# 58 Page 48 in IEEE P802.16.1b/D1with the followings:*]**

6.2.18.7.4.2 Ranging channel and ranging code for M2M Group

When a M2M group is expected to report their data or is paged, group delegates of the group send a ranging code based on multicast group ID (MGID) from the above ranging code set to BS.

Calculation equation on dedicated ranging code is as follows:

~~r~~~~dedicated ranging code~~~~=mod(floor (MGID/M), N~~~~ranging opportunity~~~~)~~

rdedicated ranging code=mod(floor (MGID/M), NM2Mgroup) (184b)

~~The M2M individual additional RP codes shall be used for initial network entry and association of M2M individual device.~~ The Zadoff-Chu sequences with cyclic shifts are used for the RP codes. The pth RP code xp(k) is defined and generated in equation (280) (see subclause 16.3.8.2.4.1). Ncont is the total number of initial (0~NIN-1) and handover RP codes (NIN~NIN+NHO-1) per sector for normal contention-based approach. Ndedi is the total number of dedicated handover RP code. When dedicated handover RP code set isn’t allocated, the available additional RP codes set can be used for M2M group. NM2M group is the total number of the available additional RP codes set for M2M group (Ncont + Ndedi ~ Ncont+ Ndedi+NM2M group -1) where maximum possible NM2M group per sector is 32.

For certain M2M group, 4 cases for this:

mod (MGID,M)-mod(C,M)=0 (184c)  
(184d)

M is required resource of time domain (ranging channel). αmultiplexing factor of dedicated ranging code can be carriered in S-SHF SP~~1~~3. ~~N~~ ~~ranging opportunity~~ ~~is related on configuration of ranging opportunity.~~ C is related on superframe number with ranging opportunity. MGIDtotal is the total number of MGID.

1. Configuration of ranging opportunity==0, C=4\*superframe number+i; i is expressed as frame n umber (0,1,2,3);
2. Configuration of ranging opportunity==1, C=superframe number;
3. Configuration of ranging opportunity==2, C=superframe number/2; mod(superframe number,2)==0; Configuration of ranging opportunity==3, C=superframe number/4; mod(superframe number,4)==0.
4. ------------------------------- Text Proposal1 End ---------------------------------------------------

------------------------------- Text Proposal2 Start ---------------------------------------------------

**[*Remedy2: Add proposed text from line# 11 Page 62 in IEEE P802.16.1b/D1with the followings:*]**

**6.3.8.2.4 Ranging channel**

**6.3.8.2.4.1 Ranging channel for non-synchronized AMSs Ranging preamble codes**

**Table 266—RP code partition information table, *NIN , NHO and NM2M group*, for the NS-RCH**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Partition Index | 0 | 1 | 2 | 3 | 4 | 5 | 6 | 7 | 8 | 9 | 10 | 11 | 12 | 13 | 14 | 15 |
| Number of the initial RP codes,  NIN | 8 | 8 | 8 | 8 | 16 | 16 | 16 | 16 | 24 | 24 | 24 | 24 | 32 | 32 | 32 | 32 |
| Number of the handover RP  codes, NHO | 8 | 16 | 24 | 32 | 8 | 16 | 24 | 32 | 8 | 16 | 24 | 32 | 8 | 16 | 24 | 32 |
| Number of the M2M Group codes,  NM2M Group | 8 | 8 | 8 | 8 | 16 | 16 | 16 | 16 | 24 | 24 | 24 | 24 | 32 | 32 | 32 | 32 |

------------------------------- Text Proposal2 End ---------------------------------------------------

------------------------------- Text Proposal End---------------------------------------------------