|  |  |  |
| --- | --- | --- |
| Project | **IEEE 802.16 Broadband Wireless Access Working Group <**<http://ieee802.org/16>**>** | |
| Title | **Power Control Talk-around Direct Communication** | |
| Date Submitted | **2012-03-05** | |
| Source(s) | Seokki Kim, Sungcheol Channg, Miyoung Yun, Eunkyung Kim, Won-Ik Kim, Hyun Lee, Sungkyung Kim, Chulsik Yoon, Kwangjae Lim  ETRI | Voice: +82-42-860-0626 E-mail: [kimsk0729@etri.re.kr](mailto:kimsk0729@etri.re.kr) |
| Re: | “EEE 802.16-12-0142,” in response to Letter Ballot #38 on P802.16.1a/D1 | |
| Abstract | This provides AWD text proposals for power control of talk-around communication in IEEE 802.16.1a | |
| Purpose | To be discussed and adopted by TGn | |
| Notice | *This document does not represent the agreed views of the IEEE 802.16 Working Group or any of its subgroups*. It represents only the views of the participants listed in the “Source(s)” field above. It is offered as a basis for discussion. It is not binding on the contributor(s), who reserve(s) the right to add, amend or withdraw material contained herein. | |
| Copyright Policy | The contributor is familiar with the IEEE-SA Copyright Policy <http://standards.ieee.org/IPR/copyrightpolicy.html>. | |
| Patent Policy | The contributor is familiar with the IEEE-SA Patent Policy and Procedures:  <<http://standards.ieee.org/guides/bylaws/sect6-7.html#6>> and <<http://standards.ieee.org/guides/opman/sect6.html#6.3>>.  Further information is located at <<http://standards.ieee.org/board/pat/pat-material.html>> and <<http://standards.ieee.org/board/pat>>. | |

**Power Control for Talk-around Direct Communication**

Seokki Kim, Sungcheol Chang, Miyoung Yun, Eunkyung Kim, Won-Ik Kim, Hyun Lee, Sungkyung Kim, Chulsik Yoon, Kwangjae Lim

ETRI

# Introduction

This contribution is for power control of talk-around direct communication.

# References

[1] IEEE P802.16.1a/D1, WirelessMAN-Advanced Air Interface for Broadband Access Systems – Draft Amendment: Higher Reliability Networks, Feb. 2012.

# Proposed Text for the 802.16.1a AWD

Note:

The text in **BLACK** color: the existing text in the 802.16.1a AWD

The text in **~~RED~~** color: the removal of existing 802.16.1a AWD

The text in **BLUE** color: the new text added to the 802.16.1a AWD

[-------------------------------------------------Start of Text Proposal---------------------------------------------------]

# *[Remedy1: Add new text in the section 6.2.3.65.37 in the IEEE 802.16.1a Draft]*

**6.2.3.65.37 AAI-DC-RTS**

…

**Table 1066kk – AAI-DC-RTS message field description**

|  |  |  |  |
| --- | --- | --- | --- |
| **Field** | **Size**  **(bits)** | **Value/Description** | **Condition** |
| Source DCTID | 24 | Indicates a source HR-MS address |  |
| Destination DCTID or DCGID | 24 | Indicates a destination HR-MS (Group) address |  |
| Maximum Index of Burst Size | 8 | Indicates a maximum index of burst size that the  sending HR-MS suggests the receiving HR-MS  to recommend. The receiving HR-MS selects  burst size that is less than |  |
| Maximum Number of HARQ  Retransmission | 2 | Indicates maximum number of PHY burst  retransmission for HARQ operation.  0: HARQ retransmission is disabled  1~3: HARQ retransmission is enabled |  |
| Destination Address Type | 1 | Indicates type of destination address.  0: DCTID  1: DCGID |  |
| Piggyback Message Indicator | 1 | Indicates whether a control message is  piggybacked or not  0: no piggyback  1: MAC control message |  |
| Transmit Power Level of Dedicated Channel | 6 | Unsigned integer from 1 to 64 in units of 1 dBm, where  0b000000=1 dBm and 0b111111=64 dBm. |  |
| Reserved | ~~4~~6 |  |  |
| MAC Control Message | varia  ble | MAC control messages in Table 1216 except  AAI-DC-RTS and AAI-DC-CTS messages. | Present if  Piggyback  message  indicator is set  to 1 |

# *[Remedy2: Add new section (6.12.2.3.2.9) and following text in the section in the IEEE 802.16.1a Draft]*

6.12.2.3.2.9 Power control

For synchronization channel transmission, HR-MSs shall always transmit at its maximum power. For dedicated channel and supplementary channel transmission, sending HR-MSs inform receiving HR-MS its Tx power of dedicated channel by AAI-DC-RTS message. Under certain operational circumstances, receiving HR-MSs may reduce its Tx power of supplementary channel if it determines that it is in close proximity to the current sending HR-MS. To determine the Tx power level of supplementary channel, receiving HR-MS can measure the dedicated channel power level but specific measurement mechanism is not the scope of the present document.

[-------------------------------------------------End of Text Proposal---------------------------------------------------]