|  |  |  |
| --- | --- | --- |
| Project | **IEEE 802.16 Broadband Wireless Access Working Group <**<http://ieee802.org/16>**>** | |
| Title | **Cleanup of Group Delegate Sections** | |
| Date Submitted | **2012-03-13** | |
| Source(s) | Jaesun Cha, Soojung Jung, Wooram Shin, Anseok Lee, Kwangjae Lim ETRI | E-mail: [jscha@etri.re.kr](mailto:jscha@etri.re.kr)  \*<<http://standards.ieee.org/faqs/affiliationFAQ.html>> |
| Re: | Sponsor Ballot on P802.16.1b/D2 | |
| Abstract | This contribution proposes text changes for cleanup of GD procedure. | |
| Purpose | For discussion in M2M TG and adoption into 16.1b draft | |
| Notice | *This document does not represent the agreed views of the IEEE 802.16 Working Group or any of its subgroups*. It represents only the views of the participants listed in the “Source(s)” field above. It is offered as a basis for discussion. It is not binding on the contributor(s), who reserve(s) the right to add, amend or withdraw material contained herein. | |
| Copyright Policy | The contributor is familiar with the IEEE-SA Copyright Policy <http://standards.ieee.org/IPR/copyrightpolicy.html>. | |
| Patent Policy | The contributor is familiar with the IEEE-SA Patent Policy and Procedures:  <<http://standards.ieee.org/guides/bylaws/sect6-7.html#6>> and <<http://standards.ieee.org/guides/opman/sect6.html#6.3>>.  Further information is located at <<http://standards.ieee.org/board/pat/pat-material.html>> and <<http://standards.ieee.org/board/pat>>. | |

**Cleanup of Group Delegate Sections**

Jaesun Cha, Soojung Jung, Wooram Shin, Anseok Lee, Kwangjae Lim

ETRI

# Introduction

The purpose of this contribution is to clarify some ambiguous texts about group delegate operation.

# Proposed Texts

----------------- Start of the text proposal --------------------------------------------------------------------------------------

[*Modify texts in section 6.2.18.7.4 on page 53 as follows;*]

**6.2.18.7.4 Network reentry from idle mode for M2M device group**

In order to reduce network congestion produced by a large number of M2M devices, network reentry may be initiated as~~for~~ a group of M2M devices. M2M devices in a M2M device group are~~is~~ called as group member (GM). An M2M device in a group that is authorized to act as representative for this M2M device group is called as a Group Delegate (GD). A GD initiates ~~and is expected to initiate~~ the first ranging access for this M2M device group. ~~Such M2M device that initiates ranging for an M2M device group is called as a group delegate (GD).~~ An ABS assigns a dedicated ranging code to a GD. When M2M devices in an M2M device group are expected to transmit UL data, the group delegate selects a ranging code from a ranging code set based on M2M device Group ID (MGID) and transmits the selected ranging code to an ABS.~~When an M2M device group is expected to report their data, group delegates of the group send a ranging code based on M2M Group ID (MGID) from a ranging code set to ABS.~~ On receiving this ranging code, the ABS sends AAI-RNG-ACK in response, which includes one of three ranging status (success, abort and continue) for the group. All group members shall receive ranging status response to ~~listen to confirmation for~~ the dedicated ranging code transmitted by the ~~group~~ GD in AAI-RNG-ACK message. ~~After all group members get “success” information, they will use common or dedicated ranging resource for network access.~~ There are three possible ranging status responses from the ABS provided in the AAI-RNG-ACK message. They are as follows;

~~Upon a detection of an event specific for a group (i.e., MGID), the GMs of this group shall start the T32 timer defined in 6.11. Within the T32 timer the GMs of this group await the AAI-RNG-ACK message, which is expected to be a response to the ranging code sent by this group’s GD. If GMs receive the AAI-RNG-ACK, which is the response of the ranging code transmitted by the GD, every GM initiates further action for network re-entry. If GMs do not receive such AAI-RNG-ACK message within the duration of T32, the GMs perform voluntary network re-entry upon expiry of T32. ABS shall indicate whether network support GD scheme or not and detail indication is included in AAI-SCD message.~~

* If ranging status is “success”, all GMs in this group start its network reentry procedure by transmitting a ranging code. The GMs may select a ranging code from legacy ranging code set or a new ranging code set dedicated for M2M devices. The GMs may also select a ranging channel from legacy ranging channels or new ranging channels dedicated for M2M devices.~~The ranging code chosen may be in legacy code sets for ranging or may be a new one, and the legacy initial ranging opportunity or a new one may be used for transmitting the ranging code.~~ Before transmitting the ranging code, the GM shall randomly select a back-off value within the initial backoff window for network access.
* If ranging status is “abort”, all GMs in this group shall start the ranging abort timer and abort the ranging process until the ranging abort timer expires. After abort timer expires, all M2M devices in this group shall restart the rang­ing process as done on the first entry defined in this subclause~~procedure based on GD~~.
* If ranging status is “continue”, the GD in this group shall adjust its parameters accordingly and continue the ranging process.

Upon detection of an event specific for a group (i.e., MGID), the GMs of this group shall start the T32 timer defined in 6.11. Within the T32 timer the GMs of this group await the AAI-RNG-ACK message transmitted by an ABS in response to the ranging code sent by this group’s GD. If GMs receive the AAI-RNG-ACK, every GM initiates further action for network re-entry. If GMs do not receive the AAI-RNG-ACK message within the duration of T32, the GMs perform voluntary network re-entry upon expiry of T32 timer. ABS shall indicate whether network support GD scheme or not and a detailed indication is included in AAI-SCD message.

***Add new subclause 6.2.18.7.4.1 as indicated***

**6.2.18.7.4.1 Selection of M2M device group delegate**

~~Selection of M2M device group delegate should support fix and mobility of group. Random selection rule by M2M devices can be used for supporting selection of M2M device group delegate.~~

Selection of M2M group delegate shall be supported by both fixed and mobile devices which support group delegate function, and the selection rule is described as follows;

When members of an M2M device group needs to report UL data, ~~it will~~ each member of the group should receive the value of a random selection probability from ~~by~~ broadcast message AAI-SCD, ~~and produce random number by itself and then compare produced~~ every member should compare the value of with a self-generated random number *m* ~~with random selection probability~~ ,

If ~~if~~ , ~~it can become~~ the device is designated as group delegate,

if , ~~it cannot become~~ the device cannot be designated as group delegate,

The designated group ~~Group~~ delegate ~~will choose~~ should choose a certain superframe based on MGID, and then send a dedicated ranging code to ABS in this superframe. If the group delegate receives ~~listens~~ “continue” or “abort” instruction from the information in AAI-RNG-ACK message for the dedicated ranging codeit has sent for this group ~~in AAI-RNG-ACK~~, it should continue to act as a group delegate~~group delegate won’t change its identification of delegate~~. If the group delegate receives ~~listens to~~ “success” instruction from the information in AAI-RNG-ACK message for the dedicated ranging code it has sent for this group ~~in AAI-RNG-ACK~~, it should resign from the position of group delegate and begin to act as an ordinary ~~will go back to~~ group member.

If group member cannot receive ~~listen~~ any information in AAI-RNG-ACK message for ~~on~~ dedicated ranging code for this group, ~~and~~ the ABS may have failed to ~~cannot~~ detect the dedicated ranging code for this group~~,~~. In this case, the ABS should ~~will~~ increase random selection probability , and the selection procedure elaborated above should be repeated. ~~and then~~ ~~group member will produce random number and compare it with random selection probability again~~.

~~ABS will broadcast random selection probability by~~The value of is broadcast by the ABS via the broadcast message (AAI-SCD). ~~And~~ The ABS also controls the variety of ~~random selection probability~~ , the value of which remains fixed ~~and~~ during the interval between two AAI-SCD messages~~, random selection probability is fixed~~. M2M device calculates the random data and probability based on the fol­lowing equation (184a).

(184a)

Both *m* and *n*~~,~~ *~~n~~* ~~is~~ are integers, and one of these two parameters has to be a prime number; *j* is the max value of Yrand and prime number ;

***Add new subclause 6.2.18.7.4.2 as indicated***

**6.2.18.7.4.2 Ranging channel and ranging code for M2M device group**

When an M2M device group is expected to report their data ~~or is paged~~, group delegate~~s~~ of the group ~~send~~ selects a ranging code from ranging code set based on M2M device Group ID~~multicast group ID~~ (MGID) and transmits the selected ranging code~~from the above ranging code set~~ to ABS.

Calculation equation for selection of ~~on~~ dedicated ranging code is as follows:

(184b)

The Zadoff-Chu sequences with cyclic shifts are used for the RP codes. The pth RP code xp(k) is defined and generated in Equation (291) (see 6.3.8.2.4.1). Ncont is the total number of initial (0~NIN-1) and handover RP codes (NIN~NIN+NHO-1) per sector for normal contention-based approach. Ndedi is the total number of ded­icated handover RP code. When dedicated handover RP code set is not allocated, the available additional RP codes set ~~can~~may be used for M2M device group. NM2M group is the total number of the available additional RP codes set for M2M device group (Ncont + Ndedi ~ Ncont + Ndedi + NM2M group - 1) where maximum possible NM2M group per sector is 32.

For certain M2M device group, 4 cases for this:

(184c)

(184d)

M is required resource of time domain (ranging channel). can be carried in S-SFH SP3. C is related on superframe number with ranging opportunity. MGIDtotal is the total number of MGID.

1. If Configuration of ranging opportunity==0, ; i is expressed as frame number (0,1,2,3); *Nranging opportunity* = 4
2. If Configuration of ranging opportunity==1, ; *Nranging opportunity* = 1
3. If Configuration of ranging opportunity==2, ; mod (superframe number, 2)==0; *Nranging opportunity* =1/2;
4. If Configuration of ranging opportunity==3, ; mod (superframe number, 4)==0; *Nranging opportunity* =1/4.

----------------- End of the text proposal ---------------------------------------------------------------------------------------