|  |  |
| --- | --- |
| Project | **IEEE 802.16 Broadband Wireless Access Working Group <**<http://ieee802.org/16>**>** |
| Title | **Clarification on Security Level of MAC Control Messages** |
| Date Submitted | **2012-05-03** |
| Source(s) | Jaesun Cha, Soojung Jung, Eunkyung Kim, Anseok Lee, Wooram Shin, Kwangjae Lim | E-mail: jscha@etri.re.kr \*<<http://standards.ieee.org/faqs/affiliationFAQ.html>> |
| Re: | Sponsor Ballot Recirculation on P802.16.1b/D3 |
| Abstract | This contribution proposes some modification on security level of some MAC control messages. |
| Purpose | For discussion in M2M TG and adoption into 16.1b draft |
| Notice | *This document does not represent the agreed views of the IEEE 802.16 Working Group or any of its subgroups*. It represents only the views of the participants listed in the “Source(s)” field above. It is offered as a basis for discussion. It is not binding on the contributor(s), who reserve(s) the right to add, amend or withdraw material contained herein. |
| Copyright Policy | The contributor is familiar with the IEEE-SA Copyright Policy <http://standards.ieee.org/IPR/copyrightpolicy.html>. |
| Patent Policy | The contributor is familiar with the IEEE-SA Patent Policy and Procedures:<<http://standards.ieee.org/guides/bylaws/sect6-7.html#6>> and <<http://standards.ieee.org/guides/opman/sect6.html#6.3>>.Further information is located at <<http://standards.ieee.org/board/pat/pat-material.html>> and <<http://standards.ieee.org/board/pat>>. |

**Clarification on Security Level of MAC Control Messages**

Jaesun Cha, Soojung Jung, Eunkyung Kim, Anseok Lee, Wooram Shin, Kwangjae Lim

ETRI

# Introduction

This contribution proposes some modification of security level of AAI-MTE-IND and AAI-MGMC messages.

# Proposed Texts

----------------- Start of the text proposal --------------------------------------------------------------------------------------

[***Modify Table 26 on page 9 as follows***]

Table 26 – MAC Control messages

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No. | Functionalareas | Message names | Message description | Security | Connection |
| 70 | RELAY | AAI-ARS-CONFIG-CMD | ARS configuration Command | N/A | Unicast |
| 71 | M2M | AAI-MTE-IND | M2M multicast transmission end indication | <delete>~~N/A: If Multicast SA is not established for the intended M2M device group (identified by MGID)~~~~Encrypted: If Multicast SA is established for the intended M2M device group~~</delete><insert>N/A: in broadcastnull: in multicast when multicast SA is not establishedEncrypted/ICV: in multicast when multicast SA is established</insert> | Broadcast/Multicast (using MGID) |
| 72 | M2M | AAI-MGMC | M2M device group MAC Control | <delete>~~N/A: If it carries control information for multiple M2M device groups or if it carries control information for one M2M device group and Multicast SA is not established for that M2M device group.~~~~Encrypted: If it carries control information for one M2M device group and Multicast SA is established for the that M2M device group~~</delete><insert>N/A: in broadcastnull: in multicast when multicast SA is not establishedEncrypted/ICV: in multicast when multicast SA is established</insert> | Broadcast/Multicast (using MGID) |
| 73-255 |  |  | *Reserved* |  |  |

----------------- End of the text proposal ---------------------------------------------------------------------------------------