|  |  |
| --- | --- |
| Project | **IEEE 802.16 Broadband Wireless Access Working Group <**<http://ieee802.org/16>**>** |
| Title | **Clarification on talk-around direct communication**  |
| Date Submitted | **2012-05-04** |
| Source(s) | Seokki Kim, Sungcheol Channg, Miyoung Yun, Won-Ik Kim, Hyun Lee, Eunkyung Kim, Sungkyung Kim, Chulsik YoonETRI | Voice: +82-42-860-0626E-mail: kimsk0729@etri.re.kr |
| Re: | IEEE 802.16 Working Group Letter Ballot Recirc #38a (IEEE P802.16.1a/D2) |
| Abstract | This contribution provides clarification on talk-around direct communication in IEEE P802.16.1a/D2 |
| Purpose | To be discussed and adopted by TGn |
| Notice | *This document does not represent the agreed views of the IEEE 802.16 Working Group or any of its subgroups*. It represents only the views of the participants listed in the “Source(s)” field above. It is offered as a basis for discussion. It is not binding on the contributor(s), who reserve(s) the right to add, amend or withdraw material contained herein. |
| Copyright Policy | The contributor is familiar with the IEEE-SA Copyright Policy <http://standards.ieee.org/IPR/copyrightpolicy.html>. |
| Patent Policy | The contributor is familiar with the IEEE-SA Patent Policy and Procedures:<<http://standards.ieee.org/guides/bylaws/sect6-7.html#6>> and <<http://standards.ieee.org/guides/opman/sect6.html#6.3>>.Further information is located at <<http://standards.ieee.org/board/pat/pat-material.html>> and <<http://standards.ieee.org/board/pat>>. |

**Clarification on talk-around direct communication**

Seokki Kim, Sungcheol Chang, Miyoung Yun, Won-Ik Kim, Hyun Lee, Sungkyung Kim, Chulsik Yoon

ETRI

# Introduction

This contribution provides clarification on talk-around direct communication in IEEE P802.16.1a/D2.

# References

[1] IEEE P802.16.1a/D2, WirelessMAN-Advanced Air Interface for Broadband Access Systems – Draft Amendment: Higher Reliability Networks, Apr. 2012.

# Proposed Text

Note:

The text in **BLACK** color: the existing text in the 802.16.1a AWD

The text in **~~RED~~** color: the removal of existing 802.16.1a AWD

The text in **BLUE** color: the new text added to the 802.16.1a AWD

 [-------------------------------------------------Start of Text Proposal---------------------------------------------------]

# *[Remedy1: Modify the following message in each sections in the IEEE P802.16.1a/D2]*

**6.2.3.65.37 AAI-DC-RTS**

…

**Table 106kk – AAI-DC-RTS message field description**

|  |  |  |  |
| --- | --- | --- | --- |
| **Field** | **Size****(bits)** | **Value/Description** | **Condition** |
| Source DCTID | 24 | Indicates a source HR-MS address |  |
| Destination DCTID or DCGID | 24 | Indicates a destination HR-MS (Group) address |  |
| Maximum Index of Burst Size | 8 | Indicates a maximum index of burst size that the sending HR-MS suggests to the receiving HR-MS ~~to ecommend~~. The ~~receiving~~sending HR-MS selects the maximum index of burst size ~~that is less than~~ in Table 303. |  |
| Maximum Number of HARQ Retransmission | 2 | Indicates maximum number of PHY burst retransmission for HARQ operation.0: HARQ retransmission is disabled1~3: Maximum number of HARQ retransmission ~~is enabled~~ |  |
| Destination Address Type | 1 | Indicates type of destination address.0: DCTID1: DCGID |  |
| Piggyback Message Indicator | 1 | Indicates whether a control message ispiggybacked or not0: no piggyback1: MAC control message |  |
| Transmit Power | 6 | Unsigned integer from 1 to 64 in units of 1 dBm, where0b000000=1 dBm and 0b111111=64 dBm. |  |
| *Reserved* | 6 |  |  |
| MAC Control Message | *varia**ble* | MAC control messages in Table 1216 exceptAAI-DC-RTS and AAI-DC-CTS messages. | Present if Piggybackmessageindicator is setto 1 |

**6.2.3.65.38 AAI-DC-CTS**

…

**Table 106ll – AAI-DC-CTS message field description**

|  |  |  |  |
| --- | --- | --- | --- |
| **Field** | **Size****(bits)** | **Value/Description** | **Condition** |
| Source DCTID | 24 | Indicates a source HR-MS address |  |
| Destination DCTID or DCGID | 24 | Indicates a destination HR-MS (Group) address |  |
| ~~Recommended~~ Index of Burst Size | 8 | Indicates a ~~recommended~~ index of burst size for a dedicated channel. The receiving HR-MS selects the index of burst size that is smaller than maximum index of burst size in the AAI-DC-RTS message. |  |
| Maximum Number of HARQ Retransmission | 2 | Indicates maximum number of PHY burst retransmission for HARQ operation.0: HARQ retransmission is disabled1~3: Maximum number of HARQ retransmission |  |
| Piggyback Message Indicator | 1 | Indicates whether a control message ispiggybacked or not0: no piggyback1: MAC control message |  |
| *Reserved* | 5 |  |  |
| MAC Control Message | *varia**ble* | MAC control messages in Table 1216 exceptAAI-DC-RTS and AAI-DC-CTS messages. | Present ifPiggybackmessageindicator is setto 1 |

**6.2.3.65.39 AAI-DC-MCHG-CMD**

…

**Table 106mm – AAI-DC-MCHG-CMD message field description**

|  |  |  |  |
| --- | --- | --- | --- |
| **Field** | **Size****(bits)** | **Value/Description** | **Condition** |
| ~~Maximum~~New index of burst size | 8 | Indicates a ~~maximum~~new index of burst size for a dedicated channel |  |

# *[Remedy2: Modify the following text in the section 6.12.2.3.2.4 in the IEEE P802.16.1a/D2]*

**6.12.2.3.2.4 Supplementary Channel**

…

As shown in Figure 255 ~ Figure 258, *Ci* is the *i*-th supplementary sub-channel corresponding to the *i*-th dedicated sub-channel. A supplementary sub-channel is composed of two sub-blocks distributed in the frequency domain. Since all HR-MSs should listen the supplementary channels, to obtain Tx. And Rx. Switching time, no signal is transmitted in the last OFDM symbol of supplementary channel (6-th OFDM symbol). The sub-block of supplementary sub-channel is composed of ~~3~~2 subcarriers-by- 5 OFDM symbols. The supplementary sub-channels corresponding to the dedicated sub-channels in slot 1 are located in slot 2, and the supplementary sub-channels corresponding to the dedicated sub-channels in slot 2 are located in slot 1. By assigning a dedicated sub-channel and the corresponding supplementary sub-channel in a cross way, the setup time of communication link and the retransmission latency can be minimized. For example, if an HR-MS transmits a packet by using the dedicated sub-channel 1 in slot 1, because the corresponding supplementary sub-channel is located in slot 2, the receiving HR-MS can transmit ACK/NACK signal by using the supplementary sub-channel in the same superframe, and the retransmission packet can be transmitted in the next superframe.

…

Figure 255 describes the ~~proposed~~ Sup-CH structure for TDC. Details of the Sub-CH structure are defined in 6.12.2.3.2.1. One Sup-CH is composed of four distributed mini-tiles, where a mini-tile has (2 subcarriers)Ⅹ(5 symbols) rectangular-shaped resource elements. A Sup-CH includes ranging channel, CQI channel, and feedback channel, which are transmitted in TDM (time division multiplexing) manner.

 [-------------------------------------------------End of Text Proposal---------------------------------------------------]