|  |  |  |
| --- | --- | --- |
| Project | **IEEE 802.16 Broadband Wireless Access Working Group <**<http://ieee802.org/16>**>** | |
| Title | **Clarification on HR-MS neighbor discovery** | |
| Date Submitted | **2012-07-15** | |
| Source(s) | Anh Tuan Hoang  I2R | E-mail:  [athoang@i2r.a-star.edu.sg](mailto:sjshin@chosun.ac.kr) |
| Re: | “IEEE 802.16-12-400-00-Gdoc,” in response to Letter Ballot Recirc #38b on P802.16.1a/D3 | |
| Abstract |  | |
| Purpose | To discuss and adopt the proposed text in the draft amendment document on GRIDMAN | |
| Notice | *This document does not represent the agreed views of the IEEE 802.16 Working Group or any of its subgroups*. It represents only the views of the participants listed in the “Source(s)” field above. It is offered as a basis for discussion. It is not binding on the contributor(s), who reserve(s) the right to add, amend or withdraw material contained herein. | |
| Copyright Policy | The contributor is familiar with the IEEE-SA Copyright Policy <http://standards.ieee.org/IPR/copyrightpolicy.html>. | |
| Patent Policy | The contributor is familiar with the IEEE-SA Patent Policy and Procedures:  <<http://standards.ieee.org/guides/bylaws/sect6-7.html#6>> and <<http://standards.ieee.org/guides/opman/sect6.html#6.3>>.  Further information is located at <<http://standards.ieee.org/board/pat/pat-material.html>> and <<http://standards.ieee.org/board/pat>>. | |

**Clarification on HR-MS neighbor discovery**

Anh Tuan Hoang

Institute for Infocomm Research

# Introduction

We propose some modifications to the specification of HR-MS neighbor discovery to make the description clearer.

# References

[1] IEEE P802.16nTM/D3, Air Interface for Broadband Wireless Access Systems - Draft Amendment: Higher Reliability Networks, June 2012.

[2] IEEE P802.16.1aTM/D3, WirelessMAN-Advanced Air Interface for Broadband Access Systems - Draft Amendment: Higher Reliability Networks, June 2012.

# Proposed Text for the 802.16.1a AWD

Note:

The text in **BLACK** color: the existing text in the 802.16.1a AWD

The text in **~~RED~~** color: the removal of existing 802.16.1a AWD

The text in **BLUE** color: the new text added to the 802.16.1a AWD

[-------------------------------------------------Start of Text Proposal---------------------------------------------------]

***[Remedy1: Modify Section 6.2.3.65.12 in IEEE P802.16.1a/D3 as indicated]***

* + - * 1. AAI-HR-RNG-CMD message

HR-BS/RS sends AAI-HR-RNG-CMD message to instruct ~~one or group of~~ its associated HR-MS to carry out neighbor discovery. The field “Action” in AAI-HR-RNG-CMD message tells the receiving HR-MS whether ~~it (them) should~~ to transmit or receive the specified ranging signal~~s~~. The serving HR-BS/HR-RS can allocate ranging resources to both involved HR-MSs in a single assignment. ~~This allows the receiving HR-MS to transmit back a ranging sequence right after successfully processing the ranging sequence transmitted by the other HR-MS.~~

Table 106 – AAI-HR-RNG-CMD message field description

| **~~Field~~** | **~~Size (bits)~~** | **~~Value/Description~~** | **~~Condition~~** |
| --- | --- | --- | --- |
| ~~Frame Identifier~~ | ~~4~~ | ~~Frame which contains the ranging channel. The frame identifier is the 4 least significant bits of the frame number.~~ |  |
| ~~Subframe Index~~ | ~~3~~ | ~~Indicates the subframe index of the allocated ranging opportunity.~~ |  |
| ~~Dedicated ranging code index~~ | ~~5~~ | ~~Indicates the index of dedicated ranging code.~~ |  |
| ~~Action~~ | ~~2~~ | ~~0b00: ranging for neighbor discovery and receiving node to carry out transmission~~  ~~0b01: ranging for neighbor discovery and receiving node to carry out receiving~~  ~~0b10: DC/FTN periodic ranging transmission~~  ~~0b11: Reserved~~ |  |
| ~~Reversed action offset~~ | ~~4~~ | ~~0b0001-0b1111: Indicates number of frames that this HR-MS should switch to receive the same ranging code in the same ranging slot~~  ~~0b0000: no such reversed action.~~ |  |
| ~~if (Action == 0b00||0b10) || (Reversed action offset > 0x0){~~ |  |  |  |
| ~~Transmit power level~~ | ~~5~~ | ~~Unsigned integer from 0 to 31 in units of 1 dBm, where 0b00000 = 0dBm and 0b11111 = 31dBm~~ |  |
| ~~}~~ |  |  |  |
| ~~If (Action == 0b10){~~ |  |  |  |
| ~~Periodicity~~ | ~~2~~ | ~~Indicates the periodicity of periodic ranging:~~  ~~0b00: transmit ranging signal every 2 frames~~  ~~0b01: transmit ranging signal every 4 frames~~  ~~0b10: transmit ranging signal every 16 frames~~  ~~0b11: transmit ranging signal every 32 frames~~ |  |
| ~~Tx/Rx Offset~~ | ~~1~~ | ~~Offset between transmitting and receiving ranging from the other HR-MS:~~  ~~0b0: Offset = 1 frame~~  ~~0b1: Offset = 3 frames~~ |  |
| ~~}~~ |  |  |  |
| ~~Reporting mode~~ | ~~1~~ | ~~Indicates if the report mode is exclusive or triggered by threshold.~~  ~~0b0: exclusive reporting~~  ~~0b1: triggered-based reporting~~ |  |
| ~~if(Reporting mode == 0b1){~~ |  |  |  |
| ~~SINR threshold~~ | ~~4~~ | ~~Indicates the SINR threshold for the ranging signal above which report should be made by receiving station. The 4 bit value from 0b0000 to 0b1111 represent values among {–9, –8.5, –8, –7.5, –7, –6.5,–6, –5.5, –5, –4.5, –4, –3.5, –3, –2.5,–2, –1.5} dB~~ |  |
| ~~}~~ |  |  |  |

| **Field** | **Size (bits)** | **Value/Description** | **Condition** |
| --- | --- | --- | --- |
| Frame Identifier | 4 | Frame which contains the ranging channel. The frame identifier is the 4 least significant bits of the frame number. |  |
| Subframe Index | 3 | Indicates the subframe index of the allocated ranging opportunity. |  |
| Dedicated ranging code index | 5 | Indicates the index of dedicated ranging code. |  |
| Action | 2 | 0b00: ranging for neighbor discovery and receiving node to carry out transmission  0b01: ranging for neighbor discovery and receiving node to carry out receiving  0b10: DC/FTN periodic ranging transmission  0b11: Reserved |  |
| if (Action == 0b00){ |  |  |  |
| Transmit power level | 5 | Unsigned integer from 0 to 31 in units of 1 dBm, where 0b00000 = 0dBm and 0b11111 = 31dBm |  |
| Reversed action offset | 4 | 0b0001-0b1111: Indicates the number of frames between the frame that this HR-MS transmits the ranging code until the frame that this HR-MS should try to receive the same ranging code. | Present if HR-BS assigns ranging resources in both directions. |
| Reporting mode | 1 | Indicates if the report mode is exclusive or triggered by threshold.  0b0: exclusive reporting  0b1: triggered-based reporting | Present if HR-BS assigns ranging resources in both directions. |
| if(Reporting mode == 0b1){ |  |  |  |
| SINR threshold | 4 | Indicates the SINR threshold for the ranging signal above which report should be made by receiving station. The 4 bit value from 0b0000 to 0b1111 represent values among {–9, –8.5, –8, –7.5, –7, –6.5,–6, –5.5, –5, –4.5, –4, –3.5, –3, –2.5,–2, –1.5} dB |  |
| } |  |  |  |
| }elseif (Action == 0b01){ |  |  |  |
| Reporting mode | 1 | Indicates if the report mode is exclusive or triggered by threshold.  0b0: exclusive reporting  0b1: triggered-based reporting |  |
| if(Reporting mode == 0b1){ |  |  |  |
| SINR threshold | 4 | Indicates the SINR threshold for the ranging signal above which report should be made by receiving station. The 4 bit value from 0b0000 to 0b1111 represent values among {–9, –8.5, –8, –7.5, –7, –6.5,–6, –5.5, –5, –4.5, –4, –3.5, –3, –2.5,–2, –1.5} dB |  |
| } |  |  |  |
| Reversed action offset | 4 | 0b0001-0b1111: Indicates the number of frames between the frame that this HR-MS receives the ranging code until the frame that this HR-MS should switch to transmit the same ranging code. | Present if HR-BS assigns ranging resources in both directions. |
| Transmit power level | 5 | Unsigned integer from 0 to 31 in units of 1 dBm, where 0b00000 = 0dBm and 0b11111 = 31dBm | Present if HR-BS assigns ranging resources in both directions. |
| }elseif (Action == 0b10){ |  |  |  |
| Transmit power level | 5 | Unsigned integer from 0 to 31 in units of 1 dBm, where 0b00000 = 0dBm and 0b11111 = 31dBm |  |
| Periodicity | 2 | Indicates the periodicity of periodic ranging:  0b00: transmit ranging signal every 2 frames  0b01: transmit ranging signal every 4 frames  0b10: transmit ranging signal every 16 frames  0b11: transmit ranging signal every 32 frames |  |
| Tx/Rx Offset | 1 | Offset between transmitting and receiving ranging from the other HR-MS:  0b0: Offset = 1 frame  0b1: Offset = 3 frames |  |
| } |  |  |  |

[-------------------------------------------------End of Text Proposal---------------------------------------------------]