|  |  |  |
| --- | --- | --- |
| Project | **IEEE 802.16 Broadband Wireless Access Working Group <**<http://ieee802.org/16>**>** | |
| Title | **ASN.1 coding for TDC MAC control messages in IEEE 802.16.1a/D5** | |
| Date Submitted | **2012-09-13** | |
| Source(s) | Hyun Lee, Miyoung Yun, Seokki Kim, Won-Ik Kim, Sungkyung Kim, Chulsik Yoon, Sungcheol Chang  ETRI | E-mail:  [hyunlee@etri.re.kr](mailto:hyunlee@etri.re.kr) |
| Re: | In response to Sponsor Ballot on P802.16a | |
| Abstract | This provides AWD text proposals for ASN.1 coding of TDC (talk-around direct communication) MAC control messages in IEEE 802.16.1a/D5 | |
| Purpose | To discuss and adopt the proposed text in the draft amendment document on GRIDMAN | |
| Notice | *This document does not represent the agreed views of the IEEE 802.16 Working Group or any of its subgroups*. It represents only the views of the participants listed in the “Source(s)” field above. It is offered as a basis for discussion. It is not binding on the contributor(s), who reserve(s) the right to add, amend or withdraw material contained herein. | |
| Copyright Policy | The contributor is familiar with the IEEE-SA Copyright Policy <http://standards.ieee.org/IPR/copyrightpolicy.html>. | |
| Patent Policy | The contributor is familiar with the IEEE-SA Patent Policy and Procedures:  <<http://standards.ieee.org/guides/bylaws/sect6-7.html#6>> and <<http://standards.ieee.org/guides/opman/sect6.html#6.3>>.  Further information is located at <<http://standards.ieee.org/board/pat/pat-material.html>> and <<http://standards.ieee.org/board/pat>>. | |

**ASN.1 coding for TDC MAC control messages in IEEE 802.16.1a/D5**

Hyun Lee, Miyoung Yun, Seokki Kim, Won-Ik Kim, Sungkyung Kim,

Chulsik Yoon, Sungcheol Chang

ETRI

# Introduction

This document provides the modification on ASN.1 coding of **TDC** (talk-around direct communication) **MAC control messages according to the IEEE 802.16.1a**/D5.

# References

[1] IEEE 802.16-12-0132-00, GRIDMAN System Requirement Document including SARM annex, January 2012.

[2] IEEE P802.16.1aTM/D5, WirelessMAN-Advanced Air Interface for Broadband Access Systems - Draft Amendment: Higher Reliability Networks, June 2012.

# Proposed Text for the 802.16.1a AWD

Note:

The text in **BLACK** color: the existing text in the 802.16.1a AWD

The text in **~~RED~~** color: the removal of existing 802.16.1a AWD

The text in **BLUE** color: the new text added to the 802.16.1a AWD

[-------------------------------------------------Start of Text Proposal---------------------------------------------------]

**[*Remedy 1: Adopt the following proposed modification from line #9, page #236 to line #42, page #236 in IEEE P802.16.1a/D5.*]**

-- HR talk-around direct communication

aaiDcLestReq AAI-DC-LEST-REQ,

aaiDcLestRsp AAI-DC-LEST-RSP,

aaiDcMesRep AAI-DC-MES-REP,

aaiDcRchgReq AAI-DC-RCHG-REQ,

aaiDcRchgRsp AAI-DC-RCHG-RSP,

aaiDcTknReq AAI-DC-TKN-REQ,

aaiDcTknRsp AAI-DC-TKN-RSP,

aaiDcTknHo AAI-DC-TKN-HO,

aaiDcLestCmd AAI-DC-LEST-CMD,

aaiDcLrelCmd AAI-DC-LREL-CMD,

aaiDcDsaCmd AAI-DC-DSA-CMD,

aaiDcDscCmd AAI-DC-DSC-CMD,

aaiDcDsdCmd AAI-DC-DSD-CMD,

aaiDcMesCmd AAI-DC-MES-CMD,

aaiDcRchgCmd AAI-DC-RCHG-CMD,

aaiDcTknAdv AAI-DC-TKN-ADV,

aaiDcRts AAI-DC-RTS,

aaiDcCts AAI-DC-CTS,

aaiDcCfgCmd AAI-DC-CFG-CMD,

aaiDcRelayAdv AAI-DC-RELAY-ADV,

aaiDcRelayReq AAI-DC-RELAY-REQ,

aaiDcRelayRsp AAI-DC-RELAY-RSP,

aaiDcFwdAdv AAI-DC-FWD-ADV,

aaiDcFwdJoin AAI-DC-FWD-JOIN,

**[*Remedy 2: Adopt the following proposed modification from line #27, page #252 to line #3, page #253 in IEEE P802.16.1a/D5.*]**

-- +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-

-- Direct communication link establishment request

-- +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-

AAI-DC-LEST-REQ ::= SEQUENCE {

linkChangeCount INTEGER (0..15),

flowEstablishmentRequestForTokenHandover INTEGER {

requestToEstablishForTokenHandover (o),

flowEstablishmentIsNotAllowed (1)

} (0..15),

linkList SEQUENCE (SIZE (0..1)) OF SEQUENCE {

fID FID,

trafficPriority INTEGER (0..7),

cSSpecificationParameters INTEGER {

g729a (16),

amr (17)

} (0..255),

mACHeaderType ENUMERATED {

agmh,

spmh

},

inorderDeliveryIndicator BIT STRING (SIZE(1)),

sDUReorderingTimeout INTEGER(1..16) OPTIONAL,

reserved INTEGER(0..3)

},

forwardingRequestIndicator ENUMERATED {

notRequestForwardingToNetwork,

requestForwardingToNetwork

},

targetDCGID BIT STRING (SIZE(24)),

…

}

**[*Remedy 3: Adopt the following proposed modification from line# 4, page #253 to line #30, page #253 in IEEE P802.16.1a/D5.*]**

-- +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-

-- Direct communication link establishment response

-- +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-

AAI-DC-LEST-RSP ::= SEQUENCE {

linkChangeCount INTEGER (0..15),

confirmationCode INTEGER {

accept (0),

rejectWithaRecommendedDCH (1),

reject (2)

} (0..15),

flowEstablishmentConfirmForTokenHandover INTEGER {

confirmFlowEstablismenthisForTokenHandover (o),

flowEstablishmentIsNotAllowed (1)

} (0..1),

directModeZoneType INTEGER {

cdmz (0),

cdmze (1),

csdmz (2)

} (0..3) OPTIONAL,

dCHNumber INTEGER (0..63) OPTIONAL,

linkList SEQUENCE (SIZE (0..1)) OF SEQUENCE {

fID FID,

trafficPriority INTEGER (0..7),

cSSpecificationParameters INTEGER {

g729a (16),

amr (17)

} (0..255),

mACHeaderType ENUMERATED {

agmh,

spmh

},

},

...

}

**[*Remedy 4: Adopt the following proposed modification from line# 58, page #261 to line #27, page #261 in IEEE P802.16.1a/D5.*]**

-- +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-

-- Direct communication relay request

-- +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-

AAI-DC-RELAY-REQ ::= SEQUENCE {

linkChangeCount INTEGER (0..15),

flowList SEQUENCE (SIZE (0..1)) OF SEQUENCE {

fID FID,

trafficPriority INTEGER (0..7),

cSSpecificationParameters INTEGER {

g729a (16),

amr (17)

} (0..255),

mACHeaderType ENUMERATED {

agmh,

spmh

},

inorderDeliveryIndicator BIT STRING (SIZE(1)),

sDUReorderingTimeout INTEGER(1..16) OPTIONAL,

reserved INTEGER(0..15)

},

targetDCTIDorDCGID BIT STRING(SIZE(24)),

flowEstablishmentReqForTokenHandover INTEGER {

requestToEstablishForTokenHandover (o),

flowEstablishmentIsNotAllowed (1)

} (0..15),

...

}

**[*Remedy 5: Adopt the following proposed modification from line# 29, page #262 to line #54, page #262 in IEEE P802.16.1a/D5.*]**

-- +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-

-- Direct communication relay response

-- +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-

AAI-DC-RELAY-RSP ::= SEQUENCE {

linkChangeCount INTEGER (0..15),

confirmationCode INTEGER {

accept (0),

rejectWithaRecommendedDCH (1),

waitNextResponseMessage (2)

} (0..15),

directModeZoneType INTEGER {

cdmz (0),

cdmze (1),

csdmz (2)

} (0..3) OPTIONAL,

dCHNumber INTEGER (0..63) OPTIONAL,

flowEstablishmentConfirmForTokenHandover INTEGER {

confirmFlowEstablismenthisForTokenHandover (o),

flowEstablishmentIsNotAllowed (1)

} (0..1),

linkList SEQUENCE (SIZE (0..1)) OF SEQUENCE {

fID FID,

trafficPriority INTEGER (0..7),

cSSpecificationParameters INTEGER {

g729a (16),

amr (17)

} (0..255),

mACHeaderType ENUMERATED {

agmh,

spmh

},

},

...

}

**[*Remedy 6: Adopt the following proposed modification from line# 21, page #255 to line #38, page #255 in IEEE P802.16.1a/D5.*]**

-- +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-

-- Direct communication token request

-- +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-

AAI-DC-TKN-REQ ::= SEQUENCE {

directModeZoneType INTEGER {

cdmz (0),

cdmze (1),

csdmz (2)

} (0..3),

dCHNumber INTEGER (0..15),

linkList SEQUENCE (SIZE (0..1)) OF SEQUENCE {

fID FID,

trafficPriority INTEGER (0..7),

cSSpecificationParameters INTEGER {

g729a (16),

amr (17)

} (0..255),

mACHeaderType ENUMERATED {

agmh,

spmh

},

},

...

}

**[*Remedy 7: Adopt the following proposed modification from line# 58, page #258 to line #21, page #259 in IEEE P802.16.1a/D5.*]**

-- +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-

-- Direct communication resource change command

-- +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-

AAI-DC-RCHG-CMD ::= SEQUENCE {

listOfDCHsChanged SEQUENCE (SIZE (0..36)) OF SEQUENCE {

oldDirectModeZoneType INTEGER {

cdmz (0),

cdmze (1),

csdmz (2)

} (0..3),

oldDCHNumber INTEGER (0..15),

newDirectModeZoneType INTEGER {

cdmz (0),

cdmze (1),

csdmz (2)

} (0..3),

newDCHNumber INTEGER (0..15)

},

listOfDCHsReleased SEQUENCE (SIZE (0..36)) OF SEQUENCE {

directModeZoneType INTEGER {

cdmz (0),

cdmze (1),

csdmz (2)

} (0..3),

dCHNumber INTEGER (0..15)

},

...

}

**[*Remedy 8: Adopt the following proposed modification from line# 4, page #253 to line #48, page #253 in IEEE P802.16.1a/D5.*]**

-- +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-

-- Direct communication resource change request

-- +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-

AAI-DC-RCHG-REQ ::= SEQUENCE {

listOfDCHsForCINRReport SEQUENCE (SIZE (0..36)) OF SEQUENCE {

oldDirectModeZoneType INTEGER {

cdmz (0),

cdmze (1),

csdmz (2)

} (0..3),

oldDCHNumber INTEGER (0..15),

newDirectModeZoneType INTEGER {

cdmz (0),

cdmze (1),

csdmz (2)

} (0..3),

newDCHNumber INTEGER (0..15)

} OPTIONAL,

listOfRecommendedDCHs SEQUENCE (SIZE (0..36)) OF SEQUENCE {

directModeZoneType INTEGER {

cdmz (0),

cdmze (1),

csdmz (2)

} (0..3),

dCHNumber INTEGER (0..63),

noiseAndInterferenceLevelMean INTEGER (0..255),

noiseAndInterferenceLevelVariance INTEGER (0..15)

} OPTIONAL,

listOfDCHsReleased SEQUENCE (SIZE (0..36)) OF SEQUENCE {

directModeZoneType INTEGER {

cdmz (0),

cdmze (1),

csdmz (2)

} (0..3),

dCHNumber INTEGER (0..15)

},

...

}

**[*Remedy 9: Adopt the following proposed modification from line# 50, page #254 to line #20, page #255 in IEEE P802.16.1a/D5.*]**

-- +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-

-- Direct communication resource change response

-- +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-

AAI-DC-RCHG-RSP ::= SEQUENCE {

confirmationCode INTEGER {

acceptWithNewDCHsMapping (0),

reject (1)

} (0..15),

listOfNewDCHs SEQUENCE (SIZE (0..36)) OF SEQUENCE {

oldDirectModeZoneType INTEGER {

cdmz (0),

cdmze (1),

csdmz (2)

} (0..3),

oldDCHNumber INTEGER (0..15),

newDirectModeZoneType INTEGER {

cdmz (0),

cdmze (1),

csdmz (2)

} (0..3),

newDCHNumber INTEGER (0..15)

} OPTIONAL,

listOfDCHsReleased SEQUENCE (SIZE (0..36)) OF SEQUENCE {

directModeZoneType INTEGER {

cdmz (0),

cdmze (1),

csdmz (2)

} (0..3),

dCHNumber INTEGER (0..15)

},

...

}

**[*Remedy 10: Insert the following texts after line #55, page #262 in IEEE P802.16.1a/D5.*]**

-- +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-

-- Direct communication forward advertisement

-- +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-

AAI-DC-FWD-ADV ::= SEQUENCE {

forwardingDCTID BIT STRING (SIZE(24)),

listOfCandidateDCGID SEQUENCE (SIZE (0..36)) OF SEQUENCE {

candidateDCGID BIT STRING (SIZE(24))

},

listOfOnGoingDCGID SEQUENCE (SIZE (0..36)) OF SEQUENCE {

onGoingDCGID BIT STRING (SIZE(24))

},

forwardingUnicastStatus INTEGER {

available (0),

unavailable (1)

},

messageChangeCount INTEGER (0..15),

...

}

-- +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-

-- Direct communication forward joining

-- +-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-+-

AAI-DC-FWD-JOIN ::= SEQUENCE {

listOfDCGID SEQUENCE (SIZE (0..36)) OF SEQUENCE {

dCGID BIT STRING (SIZE(24))

},

...

}

[-------------------------------------------------End of Text Proposal---------------------------------------------------]