

Radiocommunications (Low Interference Potential Devices) Class Licence Variation 2020 (No. 1)

*Radiocommunications Act 1992*

The AUSTRALIAN COMMUNICATIONS AND MEDIA AUTHORITY makes this Variation under subsection 132(1) of the *Radiocommunications Act 1992*.

Dated  2020

Member

Member/General Manager

Australian Communications and Media Authority

1 Name of instrument

 This is the *Radiocommunications (Low Interference Potential Devices) Class Licence Variation 2020 (No. 1)*.

2 Commencement

 This instrument commences at the start of the day after it is registered on the Federal Register of Legislation.

Note: The Federal Register of Legislation may be accessed, free of charge, at [www.legislation.gov.au](http://www.legislation.gov.au).

3 Authority

 This instrument is made under subsection 132(1) of the *Radiocommunications Act 1992*.

4 Variations

 The instrument that is specified in Schedule 1 is varied as set out in the items in that Schedule.

Schedule 1 Variations

(section 4)

**Radiocommunications (Low Interference Potential Devices) Class Licence 2015 [F2015L01438]**

**1 Subsection 3A(1), after the definition of community television broadcasting service**

Insert:

**controlled premises** means premises that are owned by or under the control of a person who is providing a radiocommunications service under this class licence.

**2 Subsection 3A(1), after the definition of temporary community broadcasting licence**

Insert:

**total radiated power** or **TRP** means the integral of the power transmitted in different directions over the entire radiation sphere. It is measured considering the combination of all radiating elements on an antenna panel or individual device.

**3 Schedule 1 (table item 30, column 4, paragraph (a))**

Repeal the paragraph, substitute:

The transmitter must comply with ETSI Standard EN 300 422 or ETSI Standard EN 301 840.

**4 Schedule 1 (after table item 39)**

Insert:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 39A | Telecommand or telemetry transmitters  | (a) 169.4–169.4875(b) 169.5875–169.8125 | 16.4 mW | The maximum duty cycle must not exceed 0.1% averaged over one hour on any given frequency. |
| 39B | Telecommand or telemetry transmitters  | 169.4875–169.5875 | 16.4 mW | The maximum duty cycle must not exceed 0.001% averaged over one hour on any given frequency except between the hours of 00:00 and 06:00 local time on each day when the maximum duty cycle must not exceed 0.1% averaged over one hour on any given frequency. |
| 39C | Fixed telecommand or telemetry transmitters  | 928–935 | 25 mW | 1. The maximum radiated power spectral density must not exceed ‑14.5 dBm/kHz.
2. The maximum duty cycle must not exceed 0.1% averaged over one hour on any given frequency.
 |

**5 Schedule 1 (table item 45, column 4, paragraph (a))**

Repeal the paragraph, substitute:

The transmitter must comply with ISO/IEC 18000-6:2013 and one of the following instruments: ISO/IEC 18000-61:2012; ISO/IEC 18000-62:2012; ISO/IEC 18000-63:2012; ISO/IEC 18000-64:2012.

**6 Schedule 1 (after table item 63)**

Insert:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 63A | Data communications transmitters used indoors in or on controlled premises | 24250–24700 | See limitations | 1. The maximum base station transmitter TRP must not exceed 20 dBm/200 MHz.
2. The maximum user equipment transmitter TRP must not exceed 22 dBm per occupied bandwidth.
3. Base station transmitters must comply with the unwanted and spurious emission limits described in 3GPP TS 38.104.
4. User equipment transmitters must comply with the unwanted and spurious emission limits described in 3GPP TS 38.101-2.
5. The transmitter TRP must not exceed the emission limits set out in Table 1 of ITU Resolution 750 (Rev. WRC-19) measured anywhere in the range 23.6–24 GHz.
6. The aggregate power flux-density must not exceed ‑105.4 dBW/MHz/m2 at the external boundary walls of the controlled premises.
 |
| 63B | Data communications transmitters used indoors or outdoors in or on controlled premises | 24700–25100 | See limitations | 1. The maximum base station transmitter TRP must not exceed 25 dBm/200 MHz.
2. The maximum user equipment transmitter TRP must not exceed 22 dBm per occupied bandwidth.
3. Base station transmitters must comply with the unwanted and spurious emission limits described in 3GPP TS 38.104.
4. User equipment transmitters must comply with the unwanted and spurious emission limits described in 3GPP TS 38.101-2.
5. The transmitter TRP must not exceed the emission limits set out in Table 1 of ITU Resolution 750 (Rev. WRC-19) measured anywhere in the range 23.6–24 GHz.
6. The aggregate power flux-density must not exceed ‑105.4 dBW/MHz/m2 at the external boundary walls of the controlled premises where the use is indoors or at the edges of the controlled premises where the use is outdoors.
 |

**7 Schedule 1 (after table item 66)**

Insert:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 66A | Radiodetermination transmitters  | 10000–10550  | 2 W  | The transmitter must comply with FCC Rules Title 47 Part 15 Section 245.  |

**8 Schedule 2 (after table item 1)**

Insert:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1A | 30 | EN 301 840 | *Electromagnetic Compatibility and Radio Spectrum Matters (ERM); Digital Radio Microphones Operating in the CEPT Harmonized Band 1 785 MHz to 1 800 MHz; Part 2: Harmonized EN under Article 3.2 of the R&TTE Directive* | ETSI  |

**9 Schedule 2 (table item 14)**

Repeal the table item, substitute:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 14  | 45  | ISO/IEC 18000-6:2013  | *Information technology – Radio frequency identification for item management – Part 6: Parameters for air interface communications at 860 MHz to 960 MHz General*  | International Organization for Standardisation (ISO)  |
| 14A  | 45  | ISO/IEC 18000-61:2012  | *Information technology – Radio frequency identification for item management – Part 61: Parameters for air interface communications at 860 MHz to 960 MHz Type A* | International Organization for Standardisation (ISO)  |
| 14B  | 45  | ISO/IEC 18000-62:2012  | *Information technology – Radio frequency identification for item management – Part 62: Parameters for air interface communications at 860 MHz to 960 MHz Type B* | International Organization for Standardisation (ISO)  |
| 14C  | 45  | ISO/IEC 18000-63:2012  | *Information technology – Radio frequency identification for item management – Part 63: Parameters for air interface communications at 860 MHz to 960 MHz Type C* | International Organization for Standardisation (ISO)  |
| 14D  | 45  | ISO/IEC 18000-64:2012  | *Information technology – Radio frequency identification for item management – Part 64: Parameters for air interface communications at 860 MHz to 960 MHz Type D* | International Organization for Standardisation (ISO)  |
|  |

**10 Schedule 2 (after table item 19)**

Insert:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 20 | 63A63B | 3GPP TS 38.101-2 | NR; User Equipment (UE) radio transmission and reception; Part 2: Range 2 Standalone | 3rd Generation Partnership Project(3GPP) |
| 21 | 63A63B | 3GPP TS 38.104 | NR; Base Station (BS) radio transmission and reception | 3rd Generation Partnership Project(3GPP) |
| 22 | 63A63B | ITU Resolution 750 (Rev. WRC-19) | Compatibility between the Earth exploration-satellite service (passive) and relevant active services | International Telecommunication Union (ITU) |
| 23 | 66A | Code of Federal Regulations Title 47 §15.245  | *Part 15 Section 245: Operation within the bands 902-928 MHz, 2435-2465 MHz, 5785-5815 MHz, 10500-10550 MHz, and 24075-24175 MHz.* | FCC  |

**11 Schedule 2 (after Note 5)**

Insert:

*Note 6* Copies of instruments produced by the 3rd Generation Partnership Project are available from the following website: https://www.3gpp.org.

*Note 7* Copies of Resolutions of the International Telecommunication Union are available from the following website: https://www.itu.int.