IEEE P802.19
Wireless Coexistence

|  |
| --- |
| Revision of Table 82 |
| Date: 2011-09-\* |
| Author(s): |
| Name | Company | Address | Phone | email |
| Ryo Sawai | Sony corporation | 5-1-12, Kitashinagawa, Shinagawa-ku, Tokyo 141-0001 Japan | +81-3-5448-4018 | Ryo.Sawai@jp.sony.com |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

Some notation of parameters in Table 82 are revised. The modification parts are being highlighted via revision track.

|  |  |
| --- | --- |
| Parameter | Notes |
|  (dBm) | Maximally allowed interference level of the protection service receiver in interfere-victim reference point # for the protection target frequency channel  |
|  (dBm) | Maximally permitted EIRP of TVBD # for protection target frequency channel .  |
|  (dB) | Path loss between TVBD # and interfere-victim reference point # for protection target frequency channel  |
|  (dBm) | Maximum permitted EIRP of TVBD #(  or ) for protection target frequency channel  or adjacent frequency channel  of  |
|  (dB) | Path loss between TVBD #(  or ) and the interfere-victim reference point # for frequency channel  or adjacent frequency channel  |
|  (dB) | Total gain of TVBD #(  or ) for frequency channel  or adjacent frequency channel of .Antenna gain, antenna beam pattern and so on are given in the example parameters |
|  (dB) | Total rejection level of TVBD # for adjacent frequency channel  of . ACS (Adjacent channel selectivity), ACLR (adjacent channel leakage ratio) and so on are given in the example parameters. |
| *SM* | Shadowing margin |