IEEE P802.19
Wireless Coexistence
Comment Resolution on CID#68	
Date:  2012-05-14	
Author(s):	
Name	Company	Address	Phone	Email	
Jinho Kim	LGE	LG R&D Complex 533, Hogye-1dong, Dongan-Gu, Anyang-Shi, Kyungki-Do, 431-749, Korea	+82-31-450-1867	boiler4.kim@lge.com	
Jinyoung Chun	LGE	LG R&D Complex 533, Hogye-1dong, Dongan-Gu, Anyang-Shi, Kyungki-Do, 431-749, Korea	+82-31-450-1856	jiny.chun@lge.com	
Suhwook Kim	LGE	LG R&D Complex 533, Hogye-1dong, Dongan-Gu, Anyang-Shi, Kyungki-Do, 431-749, Korea			
Wookbong Lee	LGE				
Jinsam Kwak	LGE				
Abstract

This document provides normative text related to a the CID#68 for clarification on the timing of process (of CE and CM) initiation and termination. 

	

CID	Clause	Subclause	Page	Line	Type	Comment	Suggested Remedy	Response	
68		5.2.1.1				I guess a CE is a kind of s/w agent entity. Specifically it would be a sort of process which handles TCP/IP packets.
Under what condition, how the process should be started on?   
Moreover, how the process goes to be terminated?  	need clarification. 		

Discussion 
1.	Initiation of a CE : (Two steps of initiation and discover)
	1.1. CE (as a client program) "can be" or "should be" initiated by a user. ( which one is better between may and should ? ) 
	1.2. After then, CE "shall" try to discover a CM around it. 

2. 	Termination of a CE :
	2.1. CE "can be" terminated by a user at any time. 
	2.2. CE "shall be" terminated when it has no session with any CM for a while. (connection failure)
		2.2.1. in this case, it should be re-started through the two steps initiation procedure. 

 Proposed Text

-(Editor's note) Add the descriptions in red color to the section 4.1. as shown below. 

4.1 General description 
The reference model of a CE is shown in Figure 4.  CE, as a client or agent process, can be initiated by a user. After then the CE shall try to discover CMs around it for doing authentication procedure.  The CE can be terminated by a user at any time, and it shall be terminated when it has no session with any CM for a while.