IEEE P802.19  
Wireless Coexistence

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Mobility Information Parameters | | | | |
| Date: 2013-05-15 | | | | |
| Author(s): | | | | |
| Name | Company | Address | Phone | email |
| Golnaz Farhadi | Fujitsu Labs of America | 1240 E. Arques Avenue M/S 345, Sunnyvale, CA 94085, USA | +1-408-530-4510 | gfarhadi@us.fujitsu.com |
| Tsuyoshi Shimomura | Fujitsu Labs. Ltd. | 3-2-1 Sakado, Takatsu-ku, Kawasaki, Kanagawa, Japan | +81-44-8749066 | tcsimomura@jp.fujitsu. com |

Abstract

This contribution proposes resolutions for comments CID# 37and CID# 38 to complete the mobility information parameter element in Tables A.13 and A.20 based on the definition agreed in document 19-13/001r3 in January 2013 meeting.

**Notice:** This document has been prepared to assist IEEE 802.19. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein.

**Comments CID 37and 38**

Tables A.13 and A.20 listing mobility information parameter element are not complete in standard draft IEEE P802.19.1/DF3.03.

**Proposal**

We propose to complete Table A.13 and Table A.20 as follows (based on *MobilityInformation* definition that was agreed in document 19-13/001r3).

Table A. 13– mobilityInformation parameter element

|  |  |  |
| --- | --- | --- |
| *Parameter* | *Data type* | *Value* |
| ***maxSpeed*** | ***REAL*** | Optionally present. If present, this parameter shall be set to indicate the maximum speed value of the WSO (in km/h) |
| ***speedInformation*** | ***SpeedInofrmation*** | Optionally present. If present, this parameter shall be set to indicate detailed information on the WSO speed and direction. |
| ***routeInformation*** | ***RouteInformation*** | Optionally present. If present, this parameter shall be set to indicate the WSO planned route and time, |

The SpeedInformation and RouteInformation datatypes (need to be added in Annex A) are defined as

SpeedInformation ::= SEQUENCE {

WSOSpeed REAL, -- km/h

WSODirection REAL, -- radian

}RouteInformation ::= SEQUENCE {

PlannedRoute SEQUENCE of geolocation,

PlannedTime SEQUENCE of GeneralizedTime

}

Table A. 20– mobilityInformation parameter element

|  |  |  |
| --- | --- | --- |
| *Parameter* | *Data type* | *Value* |
| ***maxSpeed*** | ***REAL*** | Optionally present. If present, this parameter shall be set to indicate the maximum speed value of the WSO (in km/h) |
| ***speedInformation*** | ***SpeedInofrmation*** | Optionally present. If present, this parameter shall be set to indicate detailed information on the WSO speed and direction. |
| ***routeInformation*** | ***RouteInformation*** | Optionally present. If present, this parameter shall be set to indicate the WSO planned route and time, |