IEEE P™/D  
Draft for Local and Metropolitan Area Networks- Part 21: Media Independent Handover Services

Amendment 3: Optimized Single Radio Handovers

Sponsor

**Committee**of the **IEEE Computer Society**

NOTE: This amendment is to be applied to the result of original 802.21-2008, 802.21a-2012, and 802.21b-2012.

Approved <XX MONTH 20XX>

**IEEE-SA Standards Board**

Copyright © 2012 by The Institute of Electrical and Electronics Engineers, Inc.

Three Park Avenue

New York, New York 10016-5997, USA

All rights reserved.

This document is an unapproved draft of a proposed IEEE Standard. As such, this document is subject to change. USE AT YOUR OWN RISK! Because this is an unapproved draft, this document must not be utilized for any conformance/compliance purposes. Permission is hereby granted for IEEE Standards Committee participants to reproduce this document for purposes of international standardization consideration. Prior to adoption of this document, in whole or in part, by another standards development organization, permission must first be obtained from the IEEE Standards Association Department (stds.ipr@ieee.org). Other entities seeking permission to reproduce this document, in whole or in part, must also obtain permission from the IEEE Standards Association Department.

IEEE Standards Association Department

445 Hoes Lane

Piscataway, NJ 08854, USA

Abstract: This standard specifies additional IEEE 802® media access independent mechanisms that optimize handovers between possibly heterogeneous IEEE 802 systems and between IEEE 802 systems and cellular systems, to enable improved handover performance for single-radio devices.

Keywords: management, media independent handover, mobile node, mobility, seamless, point of attachment, point of service, single-radio, preregistration, pre-authentication

**IEEE Standards** documents are developed within the IEEE Societies and the Standards Coordinating Committees of the IEEE Standards Association (IEEE-SA) Standards Board. The IEEE develops its standards through a consensus development process, approved by the American National Standards Institute, which brings together volunteers representing varied viewpoints and interests to achieve the final product. Volunteers are not necessarily members of the Institute and serve without compensation. While the IEEE administers the process and establishes rules to promote fairness in the consensus development process, the IEEE does not independently evaluate, test, or verify the accuracy of any of the information or the soundness of any judgments contained in its standards.

Use of an IEEE Standard is wholly voluntary. The IEEE disclaims liability for any personal injury, property or other damage, of any nature whatsoever, whether special, indirect, consequential, or compensatory, directly or indirectly resulting from the publication, use of, or reliance upon this, or any other IEEE Standard document.

The IEEE does not warrant or represent the accuracy or content of the material contained herein, and expressly disclaims any express or implied warranty, including any implied warranty of merchantability or fitness for a specific purpose, or that the use of the material contained herein is free from patent infringement. IEEE Standards documents are supplied “**AS IS**.”

The existence of an IEEE Standard does not imply that there are no other ways to produce, test, measure, purchase, market, or provide other goods and services related to the scope of the IEEE Standard. Furthermore, the viewpoint expressed at the time a standard is approved and issued is subject to change brought about through developments in the state of the art and comments received from users of the standard. Every IEEE Standard is subjected to review at least every five years for revision or reaffirmation, or every ten years for stabilization. When a document is more than five years old and has not been reaffirmed, or more than ten years old and has not been stabilized, it is reasonable to conclude that its contents, although still of some value, do not wholly reflect the present state of the art. Users are cautioned to check to determine that they have the latest edition of any IEEE Standard.

In publishing and making this document available, the IEEE is not suggesting or rendering professional or other services for, or on behalf of, any person or entity. Nor is the IEEE undertaking to perform any duty owed by any other person or entity to another. Any person utilizing this, and any other IEEE Standards document, should rely upon his or her independent judgment in the exercise of reasonable care in any given circumstances or, as appropriate, seek the advice of a competent professional in determining the appropriateness of a given IEEE standard.

Interpretations: Occasionally questions may arise regarding the meaning of portions of standards as they relate to specific applications. When the need for interpretations is brought to the attention of IEEE, the Institute will initiate action to prepare appropriate responses. Since IEEE Standards represent a consensus of concerned interests, it is important to ensure that any interpretation has also received the concurrence of a balance of interests. For this reason, IEEE and the members of its societies and Standards Coordinating Committees are not able to provide an instant response to interpretation requests except in those cases where the matter has previously received formal consideration. A statement, written or oral, that is not processed in accordance with the IEEE-SA Standards Board Operations Manual shall not be considered the official position of IEEE or any of its committees and shall not be considered to be, nor be relied upon as, a formal interpretation of the IEEE. At lectures, symposia, seminars, or educational courses, individual presenting information on IEEE standards shall make it clear that his or her views should be considered the personal views of that individual rather than the formal position, explanation, or interpretation of the IEEE.

Comments for revision of IEEE Standards are welcome from any interested party, regardless of membership affiliation with IEEE. Suggestions for changes in documents should be in the form of a proposed change of text, together with appropriate supporting comments. Recommendations to change the status of a stabilized standard should include a rationale as to why a revision or withdrawal is required. Comments and recommendations on standards, and requests for interpretations should be addressed to:

Secretary, IEEE-SA Standards Board

445 Hoes Lane

Piscataway, NJ 08854

USA

Authorization to photocopy portions of any individual standard for internal or personal use is granted by The Institute of Electrical and Electronics Engineers, Inc., provided that the appropriate fee is paid to Copyright Clearance Center. To arrange for payment of licensing fee, please contact Copyright Clearance Center, Customer Service, 222 Rosewood Drive, Danvers, MA 01923 USA; +1 978 750 8400. Permission to photocopy portions of any individual standard for educational classroom use can also be obtained through the Copyright Clearance Center.

Notice to users

Laws and regulations

Users of these documents should consult all applicable laws and regulations. Compliance with the provisions of this standard does not imply compliance to any applicable regulatory requirements. Implementers of the standard are responsible for observing or referring to the applicable regulatory requirements. IEEE does not, by the publication of its standards, intend to urge action that is not in compliance with applicable laws, and these documents may not be construed as doing so.

Copyrights

This document is copyrighted by the IEEE. It is made available for a wide variety of both public and private uses. These include both use, by reference, in laws and regulations, and use in private self-regulation, standardization, and the promotion of engineering practices and methods. By making this document available for use and adoption by public authorities and private users, the IEEE does not waive any rights in copyright to this document.

Updating of IEEE documents

Users of IEEE standards should be aware that these documents may be superseded at any time by the issuance of new editions or may be amended from time to time through the issuance of amendments, corrigenda, or errata. An official IEEE document at any point in time consists of the current edition of the document together with any amendments, corrigenda, or errata then in effect. In order to determine whether a given document is the current edition and whether it has been amended through the issuance of amendments, corrigenda, or errata, visit the IEEE Standards Association web site at <http://ieeexplore.ieee.org/xpl/standards.jsp>, or contact the IEEE at the address listed previously.

For more information about the IEEE Standards Association or the IEEE standards development process, visit the IEEE-SA web site at <http://standards.ieee.org>.

Errata

Errata, if any, for this and all other standards can be accessed at the following URL:   
<http://standards.ieee.org/findstds/errata/index.html>. Users are encouraged to check this URL for errata periodically.

Patents

Attention is called to the possibility that implementation of this standard may require use of subject matter covered by patent rights. By publication of this standard, no position is taken by the IEEE with respect to the existence or validity of any patent rights in connection therewith. If a patent holder or patent applicant has filed a statement of assurance via an Accepted Letter of Assurance, then the statement is listed on the IEEE-SA website <http://standards.ieee.org/about/sasb/patcom/patents.html>. Letters of Assurance may indicate whether the Submitter is willing or unwilling to grant licenses under patent rights without compensation or under reasonable rates, with reasonable terms and conditions that are demonstrably free of any unfair discrimination to applicants desiring to obtain such licenses.

Essential Patent Claims may exist for which a Letter of Assurance has not been received. The IEEE is not responsible for identifying Essential Patent Claims for which a license may be required, for conducting inquiries into the legal validity or scope of Patents Claims, or determining whether any licensing terms or conditions provided in connection with submission of a Letter of Assurance, if any, or in any licensing agreements are reasonable or non-discriminatory. Users of this standard are expressly advised that determination of the validity of any patent rights, and the risk of infringement of such rights, is entirely their own responsibility. Further information may be obtained from the IEEE Standards Association.

Participants

At the time this draft was submitted to the IEEE-SA Standards Board for approval, the Working Group had the following membership:

, *Chair*

, *Vice Chair*

Participant1

Participant2

Participant3

Participant4

Participant5

Participant6

Participant7

Participant8

Participant9

The following members of the <individual/entity> balloting committee voted on this. Balloters may have voted for approval, disapproval, or abstention.

***(to be supplied by IEEE)***

Balloter1

Balloter2

Balloter3

Balloter4

Balloter5

Balloter6

Balloter7

Balloter8

Balloter9

When the IEEE-SA Standards Board approved this on <XX MONTH 20XX>, it had the following membership:

***(to be supplied by IEEE)***

**<Name>,** *Chair*

**<Name>,** *Vice Chair*

**<Name>,** *Past Chair*

**<Name>,** *Secretary*

SBMember1

SBMember2

SBMember3

SBMember4

SBMember5

SBMember6

SBMember7

SBMember8

SBMember9

\*Member Emeritus

Also included are the following nonvoting IEEE-SA Standards Board liaisons:

<Name>, *DOE Representative*

<Name>, *NRC Representative*

<Name>

*IEEE Standards Program Manager, Document Development*

<Name>

*IEEE Standards Program Manager, Technical Program Development*

Introduction

This introduction is not part of IEEE P/D, Draft for Local and Metropolitan Area Networks- Part 21: Media Independent Handover Services

Amendment 3: Optimized Single Radio Handovers

.

This standard extends the media access independent mechanisms that enable the optimization of handovers between possibly heterogeneous IEEE 802 systems and may facilitate handovers between IEEE 802 systems and cellular systems. The extensions enable mobile devices with single-radio designs to improve handover latencies and avoid packet loss.

Contents

[1. Overview 2](#_Toc344427289)

[1.1 2](#_Toc344427290)

[1.2 2](#_Toc344427291)

[1.3 2](#_Toc344427292)

[1.4 Assumptions 2](#_Toc344427293)

[2. Normative references 2](#_Toc344427297)

[3. Definitions 3](#_Toc344427298)

[4. Abbreviations and Acronymns 3](#_Toc344427299)

[5. General architecture 4](#_Toc344427300)

[5.1 Introduction 4](#_Toc344427301)

[5.1.1 4](#_Toc344427302)

[5.1.2 4](#_Toc344427303)

[5.1.3 4](#_Toc344427304)

[5.1.4 4](#_Toc344427305)

[5.1.5 4](#_Toc344427306)

[5.1.6 4](#_Toc344427307)

[5.1.7 4](#_Toc344427308)

[5.1.8 4](#_Toc344427309)

[5.1.9 4](#_Toc344427310)

[5.1.10 Media independent single radio handover 4](#_Toc344427311)

[5.1.11 Securing Single-Radio messages using PoS 5](#_Toc344427312)

[5.2 General design principles 5](#_Toc344427313)

[5.2.1 5](#_Toc344427314)

[5.2.2 5](#_Toc344427315)

[5.2.3 Single Radio Handover MIHF Design Principles 5](#_Toc344427316)

[5.3 6](#_Toc344427317)

[5.4 Media independent handover reference framework 6](#_Toc344427318)

[5.4.1 6](#_Toc344427319)

[5.4.2 6](#_Toc344427320)

[5.4.3 6](#_Toc344427321)

[5.4.4 Information Repository 6](#_Toc344427322)

[5.4.5 General MIHF reference model and SAPs / Single Radio handover Control Function 6](#_Toc344427323)

[5.4.6 SR-MIHF and Proxy function at Home Network, Source Network, and Target Network 7](#_Toc344427324)

[5.5 MIHF reference models for link-layer technologies 8](#_Toc344427337)

[5.5.1 8](#_Toc344427338)

[5.5.2 8](#_Toc344427339)

[5.5.3 8](#_Toc344427340)

[5.5.4 8](#_Toc344427341)

[5.5.5 8](#_Toc344427342)

[5.5.6 8](#_Toc344427343)

[5.5.7 8](#_Toc344427344)

[5.5.8 Single radio handover reference model and signaling flow 8](#_Toc344427345)

[6. MIH Services 10](#_Toc344427346)

[6.1 10](#_Toc344427347)

[6.2 10](#_Toc344427348)

[6.3 10](#_Toc344427349)

[6.4 Media independent command service 10](#_Toc344427350)

[6.4.1 10](#_Toc344427351)

[6.4.2 10](#_Toc344427352)

[6.4.3 Command List 10](#_Toc344427353)

[6.5 Media independent information service 11](#_Toc344427354)

[6.5.1 11](#_Toc344427355)

[6.5.2 11](#_Toc344427356)

[6.5.3 11](#_Toc344427357)

[6.5.4 Information elements 11](#_Toc344427358)

[7. Service Access Point (SAP) and primitives 12](#_Toc344427359)

[7.1 12](#_Toc344427360)

[7.2 12](#_Toc344427361)

[7.3 MIH\_LINK\_SAP primitives 12](#_Toc344427362)

[7.3.1 12](#_Toc344427363)

[7.3.2 12](#_Toc344427364)

[7.3.3 12](#_Toc344427365)

[7.3.4 12](#_Toc344427366)

[7.3.5 12](#_Toc344427367)

[7.3.6 12](#_Toc344427368)

[7.3.7 12](#_Toc344427369)

[7.3.8 12](#_Toc344427370)

[7.3.9 12](#_Toc344427371)

[7.3.10 12](#_Toc344427372)

[7.3.11 12](#_Toc344427373)

[7.3.12 12](#_Toc344427374)

[7.3.13 12](#_Toc344427375)

[7.3.14 12](#_Toc344427376)

[7.3.15 Link\_IF\_PreReg\_Ready 12](#_Toc344427377)

[7.4 MIH\_SAP primitives 14](#_Toc344427378)

[7.4.1 14](#_Toc344427379)

[7.4.2 14](#_Toc344427380)

[7.4.3 14](#_Toc344427381)

[7.4.4 14](#_Toc344427382)

[7.4.5 14](#_Toc344427383)

[7.4.6 14](#_Toc344427384)

[7.4.7 14](#_Toc344427385)

[7.4.8 14](#_Toc344427386)

[7.4.9 14](#_Toc344427387)

[7.4.10 14](#_Toc344427388)

[7.4.11 14](#_Toc344427389)

[7.4.12 14](#_Toc344427390)

[7.4.13 14](#_Toc344427391)

[7.4.14 14](#_Toc344427392)

[7.4.15 14](#_Toc344427393)

[7.4.16 14](#_Toc344427394)

[7.4.17 14](#_Toc344427395)

[7.4.18 14](#_Toc344427396)

[7.4.19 14](#_Toc344427397)

[7.4.20 14](#_Toc344427398)

[7.4.21 14](#_Toc344427399)

[7.4.22 14](#_Toc344427400)

[7.4.23 14](#_Toc344427401)

[7.4.24 14](#_Toc344427402)

[7.4.25 14](#_Toc344427403)

[7.4.26 14](#_Toc344427404)

[7.4.27 14](#_Toc344427405)

[7.4.28 15](#_Toc344427406)

[7.4.29 15](#_Toc344427407)

[7.4.30 MIH\_Prereg\_Xfer 15](#_Toc344427408)

[7.4.31 MIH\_N2N\_Prereg\_Xfer 20](#_Toc344427409)

[7.4.32 MIH\_IF\_PreReg\_Ready 25](#_Toc344427410)

[7.4.33 MIH\_CTRL\_Transfer 26](#_Toc344427411)

[8. Media independent handover protocols 30](#_Toc344427413)

[8.1 30](#_Toc344427414)

[8.2 30](#_Toc344427415)

[8.3 30](#_Toc344427416)

[8.4 30](#_Toc344427417)

[8.5 30](#_Toc344427418)

[8.6 MIH protocol messages 30](#_Toc344427419)

[8.6.1 30](#_Toc344427420)

[8.6.2 30](#_Toc344427421)

[8.6.3 MIH messages for command service 30](#_Toc344427422)

[9. MIH protocol protection 34](#_Toc344427433)

[9.1 34](#_Toc344427435)

[9.2 Key establishment through an MIH service access authentication 34](#_Toc344427436)

[9.2.1 34](#_Toc344427438)

[9.2.2 Key derivation and key hierarchy 34](#_Toc344427439)

[10. Proactive Authentication 36](#_Toc344427440)

[10.1 Media specific proactive authentication 36](#_Toc344427441)

[10.2 37](#_Toc344427443)

[10.3 Establishing Security Association roaming partners for MIH 37](#_Toc344427444)

[10.3.1 Key distribution by OPoS 39](#_Toc344427445)

[10.3.2 TPoS selection by OPoS 40](#_Toc344427446)

[11. Single Radio Handover 41](#_Toc344427447)

[11.1 Introduction 41](#_Toc344427448)

[11.2 Major single radio handover processes 41](#_Toc344427449)

[12. Proxy Function 42](#_Toc344427450)

[12.1 Introduction 42](#_Toc344427451)

[12.2 Communication between the MN and the target PoA 43](#_Toc344427452)

[12.3 Transfer of Control Message 44](#_Toc344427453)

[Annex A Bibliography 45](#_Toc344427454)

[Annex B 46](#_Toc344427455)

[Annex C 46](#_Toc344427456)

[Annex D 46](#_Toc344427457)

[Annex E 46](#_Toc344427458)

[Annex F 46](#_Toc344427459)

[F.1 46](#_Toc344427460)

[F.2 46](#_Toc344427461)

[F.3 Derived data types 46](#_Toc344427462)

[F.3.1 46](#_Toc344427463)

[F.3.2 46](#_Toc344427464)

[F.3.3 46](#_Toc344427465)

[F.3.4 Data types for link identification and manipulation 46](#_Toc344427466)

[F.3.5 47](#_Toc344427467)

[F.3.6 47](#_Toc344427468)

[F.3.7 47](#_Toc344427469)

[F.3.8 Data types for information elements 47](#_Toc344427470)

[F.3.9 48](#_Toc344427471)

[F.3.10 48](#_Toc344427472)

[F.3.11 48](#_Toc344427473)

[F.3.12 48](#_Toc344427474)

[F.3.13 48](#_Toc344427475)

[F.3.14 48](#_Toc344427476)

[F.3.15 48](#_Toc344427477)

[F.3.16 Data type for security 48](#_Toc344427478)

[F.3.17 Data types for delivery of control messages 48](#_Toc344427479)

[Annex G 49](#_Toc344427480)

[Annex H 49](#_Toc344427481)

[Annex I 49](#_Toc344427482)

[Annex J 49](#_Toc344427483)

[Annex K 49](#_Toc344427484)

[Annex L 49](#_Toc344427485)

[Annex M 50](#_Toc344427486)

[Annex N 50](#_Toc344427487)

[N.1 50](#_Toc344427488)

[N.2 50](#_Toc344427489)

[N.3 50](#_Toc344427490)

[N.4 50](#_Toc344427491)

[N.5 Terminating Phase 50](#_Toc344427492)

[N.6 Use of MIH\_Prereg\_Xfer messages for the exchange of L2 frames, including Optimized SA Establishment 50](#_Toc344427493)

[N.6.1 OPoS Distributing MIRK to TPoS and MN 50](#_Toc344427494)

[N.6.2 OPoS relays additional Preregistration signaling 53](#_Toc344427495)

[N.6.3 OPoS key distribution when OPoS is same as TPoS 54](#_Toc344427496)

[N.6.4 OPoS relay preregistration when OPoS is same as TPoS 55](#_Toc344427497)

[Annex O 56](#_Toc344427498)

[Annex P MN’s Network Access Identifier Format 56](#_Toc344427499)

[Annex Q Network discovery for single radio handover 56](#_Toc344427500)

[Q.1 Network discovery: listening to the target link 56](#_Toc344427501)

[Q.2 Network discovery: using location information 57](#_Toc344427502)

[Q.3 Network discovery: using user schedule information 58](#_Toc344427503)

[Annex R Examples of SRHO 59](#_Toc344427504)

[R.1 WLAN to WiMAX single radio handover 59](#_Toc344427505)

[R.1.1 Reference model 59](#_Toc344427506)

[R.1.2 Transport of WiMAX L2 control frames between MN and the WiMAX ASN 61](#_Toc344427507)

[R.1.3 WLAN to WiMAX Single Radio Handover processes 64](#_Toc344427508)

[R.2 3GPP to WiMAX single radio handover 65](#_Toc344427509)

[R.2.1 Reference model 65](#_Toc344427510)

[R.2.2 Transport of WiMAX L2 control frames between MN and the WiMAX ASN with SRHO-capable devices 66](#_Toc344427511)

[R.2.3 3GPP to WiMAX Single Radio Handover processes 69](#_Toc344427512)

[R.3 WiMAX to WLAN single radio handover 71](#_Toc344427513)

[R.3.1 Reference model 71](#_Toc344427514)

[R.3.2 Transport of WLAN L2 control frames between MN and the WLAN AN 72](#_Toc344427515)

[R.3.3 WiMAX to WLAN Single Radio Handover processes 75](#_Toc344427516)

[R.4 WiMAX to 3GPP single radio handover 76](#_Toc344427517)

[R.4.1 Reference model 76](#_Toc344427518)

[R.4.2 Transport of 3GPP L2 control frames between MN and the 3GPP network with SRHO-capable devices 78](#_Toc344427519)

[R.4.3 WiMAX to 3GPP Single Radio Handover processes 81](#_Toc344427520)

[R.5 WLAN to 3GPP single radio handover 83](#_Toc344427521)

[R.5.1 Reference model 83](#_Toc344427522)

[R.5.2 Transport of 3GPP L2 control frames between MN and the 3GPP network 84](#_Toc344427523)

[R.5.3 Non-trusted WLAN AN to 3GPP Single Radio Handover processes 87](#_Toc344427524)

[Annex S Handover Decision 89](#_Toc344427525)

[S.1 Weak SINR of the source link 89](#_Toc344427526)

[S.2 QoS and/or cost check 90](#_Toc344427527)

[S.3 Power consumption comparison of the link interfaces 90](#_Toc344427528)

[Annex T 91](#_Toc344427529)

Draft for Local and Metropolitan Area Networks- Part 21: Media Independent Handover Services

Amendment 3: Optimized Single Radio Handovers

***IMPORTANT NOTICE: This standard is not intended to ensure safety, security, health, or environmental protection. Implementers of the standard are responsible for determining appropriate safety, security, environmental, and health practices or regulatory requirements.***

***This IEEE document is made available for use subject to important notices and legal disclaimers.   
These notices and disclaimers appear in all publications containing this document and may   
be found under the heading “Important Notice” or “Important Notices and Disclaimers   
Concerning IEEE Documents.” They can also be obtained on request from IEEE or viewed at*** [***http://standards.ieee.org/IPR/disclaimers.html***](http://standards.ieee.org/IPR/disclaimers.html)***.***

NOTE—The editing instructions contained in this <amendment/corrigendum> define how to merge the material contained therein into the existing base standard and its amendments to form the comprehensive standard.

The editing instructions are shown in ***bold italic***. Four editing instructions are used: change, delete, insert, and replace. ***Change*** is used to make corrections in existing text or tables. The editing instruction specifies the location of the change and describes what is being changed by using ~~strikethrough~~ (to remove old material) and underscore (to add new material). ***Delete*** removes existing material. ***Insert*** adds new material without disturbing the existing material. Insertions may require renumbering. If so, renumbering instructions are given in the editing instruction. ***Replace*** is used to make changes in figures or equations by removing the existing figure or equation and replacing it with a new one. Editing instructions, change markings, and this NOTE will not be carried over into future editions because the changes will be incorporated into the base standard.

1. Overview



   4. Assumptions

***Insert at end of subclause 1.4***



The following assumptions apply during the single radio handover:

1. While the source radio is transmitting, the target radio cannot transmit.

The mobile device can transmit on only one radio at a time. Prior to handover completion, the source radio link is used to support data transfer so that the priority to transmit is given to the source radio. [CEP: what does this mean?]

1. It shall be possible that while the source radio is receiving, the target radio shall not transmit at a frequency interfering with the frequency of the source radio receiver..
2. It shall be possible that while the source radio is receiving, the target radio shall receive at a frequency not interfering with the frequency of the source radio receiver..
3. The mobile node (MN) and the target network may communicate with each other via the source network using the source link.

It is possible that the source point of attachment and the target point of attachment may: (a) belong to the same access network, (b) belong to different access networks connecting to the same backhaul network, or (c) belong to different access networks connecting to different backhaul networks. In (a) and (b), the capability to communicate between the source radio and the target network usually does not utilize internetwork interfaces. In (c), the two networks may require internetwork addresses in order to be able to communicate with each other.

1. Normative references

***Insert reference in appropriate order***

IETF RFC 5677 (2009-12) IEEE 802.21 Mobility Services Framework Design (MSFD)

1. Definitions

*Insert these definitions in appropriate order*

**Originating network PoS**: The Point of Service in the network of the Mobile Node’s current Point of Attachment

**Preregistration:** preparatory handover signaling (including security establishment) which is accomplished before the handover actually occurs.

**Proxy function**: A function to bridge the mobility signaling between a mobile node and a target point of attachment via the source network. To the MN, the Proxy function appears to be a virtual point of attachment (PoA) to the target network. It enables such functions as preregistration and proactive authentication of the MN.

**Single radio handover (SRHO)**: A handover among (possibly heterogeneous) radio access technologies during which a mobile node can transmit on only one radio at a time.

**Single Radio handover MIHF (SR-MIHF)**: A media independent control function to enable MN and Target PoA to exchange the link-layer PDUs without depending on the existence of the target radio’s physical channel. It uses the available radio’s IP transport to deliver the deactivated target radio’s L2 PDUs. It interfaces with the transport layer (e.g., TCP or UDP) through the Media Independent Handover Service Access Point (MIH\_SAP) so that it may exchange SR-MIHF frames with remote SR-MIHF entities through IP transport. The exchanged SR-MIHF frames are processed by the SR-MIHF which has the assigned transport layer protocol’s port number [RFC 5677]. SR-MIHF also interfaces with the link-layer (L2) through the Media Independent Handover Link-layer Service Access Point (MIH\_LINK\_SAP) so that it may provide transport of L2 frames of a deactivated target radio to and from a remote SR-MIHF entity.

**Single radio MIH frame**: A packet which contains the target radio’s network PDUs in its payload. [CEP: note MIH\_Prereg\_Xfer commands can work even without containing link-layer PDUs]

**Source network PoA**: A Point of Attachment in the source network, to which a Mobile Node is attached after a handover has been completed

**SRHO-capable device:** A network node that implements one or more commands from this specification document. For instance, a mobile node MN is SRHO-capable if it implements at least MIH\_Prereg\_Xfer commands.

**Target network PoA**: A Point of Attachment in the target network,, to which a Mobile Node will be attached after a handover has been completed

**Target network PoS**: A Point of Service in the target network of the target Point of Attachment, to which a Mobile Node will be attached after a handover has been completed

1. Abbreviations and Acronymns

*Insert these definitions in appropriate order*

ANDSF Access network discovery selection functions

MIHF media independent handover function

MIH\_SAP media independent handover service access point

MIH\_LINK\_SAP media independent handover link-layer service access point

OPoS originating PoS

PoS point of serviceSPoA source PoA

SR-MIHF Single radio - media independent handover function

SRHO single radio handover

TPoA target PoA

TPoS target PoS

1. General architecture
   1. Introduction

***Insert subclauses 5.1.10 and 5.1.11***

* + 1. Media independent single radio handover

The concept of media independence applies to single radio handover just as it does to the multi-radio handover. A media independent handover may be accomplished in a media independent way, but the signaling messages for a single radio handover may differ from that for a multi-radio handover.

Security is indispensable to mobility management (see section 10.2), but it has been typically quite time consuming because of reliance on distant authentication agents. Improving the security model and reducing authentication delay enables crucial improvements in handover performance. For the single radio handover design using media independent messages, the same transport possibilities as MIHF may apply. For single-radio performance improvement, it is important to accomplish as much of the handover signaling (including security establishment) before the handover actually occurs; this preparatory signaling is called preregistration. The exact signaling steps included in the preregistration process naturally depend on the requirements of the target network, and can be quite independent of the nature of the network (as above, the "source network") providing the current point of attachment for the MN. As a general rule, preregistration typically involves one or more of the following steps:

* pre-authentication -- that is, authenticating the MN before it arrives in the target network,
* address allocation -- one or more IP addresses to be used by the MN after it arrives in the target network.
* data path setup -- establishing tunnels and forwarding entries for the MN in the target network, and
* context establishment -- building all necessary state information such as QoS parameters and access permissions within target core network entities.

Each of these operations can be time-consuming, and if they had to be carried out after the MN had returned to the target network radio access, smooth handover might be impossible because of the dead time before packets could start flowing again (break-before-make). Moreover, each of the operations must be carried out securely to prevent hijacking attempts or mismanagement of target network resources. As long as handovers occur only between access points within the same operator network, it is often possible to guarantee that signaling packets are never exposed to attack. On the other hand, for access networks belonging to different operators, the data path between neighboring access points of originating and target access networks are more likely to traverse the Internet, potentially exposing preregistration signaling to attack. See section 5.1.11.

* + 1. Securing Single-Radio messages using PoS

Enabling movement between the networks of roaming partners for single-radio smartphones and Internet enabled wireless devices can be facilitated by enabling preregistration via the Point of Service (PoS) and making use of certain functions as developed in the WiMAX Forum, 3GPP2, and 3GPP . Using the PoS along with some signaling to transmit security information between roaming partners enables a low-latency, optimized handover for even the single-radio devices. Since communication between the source and target networks may traverse the Internet, these communications must be secured; but this can be quite time consuming because of reliance on distant authentication agents A method is defined to establish a secure communication channel between source and target networks as part of handover preregistration procedures (see subclause ). Improving the security model and reducing authentication delay enables crucial improvements in handover performance. [CEP: How is this related to 802.21c?]

* 1. General design principles

***Insert subclause 5.2.3***

* + 1. Single Radio Handover MIHF Design Principles

The following requirements facilitate single radio handover between different radio access technology networks.

**Functional Requirements for SR-MIHF:**

1. tunneling mechanism to deliver the pre-registration messages
2. control for pre-registered states and delivery for pre-registered contexts.
3. capabilities exchange between mobile station and SR-MIHF at the network.
   1. Supported radio access technology (RAT) types (3GPP, WiMAX, WiFi, 3GPP2, etc.)
   2. Supported target network capabilities
   3. Any required layer-2 parameters
   5. Media independent handover reference framework

***Insert subclause 5.4.4 and subclause 5.4.5 and subclause 5.4.6***

* + 1. Information Repository

The network service information and the location information, such as the availability of candidate target network etc., are needed to make handover decisions. For example, the Information Repository may be implemented as part of a media independent information server (MIIS). Alternatively, as another example, IR may be implemented in conjunction with the Access Network Discovery and Selection Function (ANDSF) defined in 3GPP standard [3GPP TS23.402], using methods outside the scope of this document.

The type of information needed in the mobility management protocol depends on the mobility management protocol being used. For example, when mobile IP is used for the inter-network management protocol, the location of the MN in the network is the care-of-address (CoA) and the identity of the MN is the home address in the home network of the MN. The location management information for mobile IP may then be the binding of the home address to the care-of-address. Furthermore, in accordance with existing procedures for subscriber management, mobility management may also require access to policy information controlling the allowable behavior of the mobile devices.

The distributed database of the Information Repository allows flexibility for different owners to manage their data separately. For example each network will typically host the master copy of the data that is most convenient to be managed by that network. The servers in the different networks constitute a distributed database of the Information Repository, organized so that each server knows which data belongs to which component of the Repository.

* + 1. General MIHF reference model and SAPs / Single Radio handover Control Function

To prepare for handover, the MN’s target radio exchanges link-layer PDUs with the target PoA at the target network. These network entry PDUs can be the same PDUs that would be exchanged if the target link were active. There is no guarantee that the target link is available during a single radio handover. A proxy function is used here to enable the MN and the target PoA to exchange the network entry link-layer PDUs without depending on the existence of the target radio’s physical channel but with the help of the active source radio.

In figure 4 (in subclause 5.5.2) the Single Radio MIHF in a multiple interface node is implemented using the media independent control function (MIHF) in the control plane.

The SR-MIHF uses MIH\_SAP for communication via TCP/IP or UDP/IP. The SR-MIHF similarly interfaces with the link-layer (L2) MIH\_LINK\_SAP as before. During a single radio handover, an L2 frame may be encapsulated in an MIH message to constitute a SR-MIHF frame, which is then exchanged via an active link between the SR-MIHFs of a local and a remote node using MIH protocol over L3 transport (TCP or UDP).

* + 1. SR-MIHF and Proxy function at Home Network, Source Network, and Target Network



**Figure 3a An architecture of distributed mobility management.**

This distributed mobility management architecture also works for single radio management. Because the logical functions for distributed mobility management must already reside in some physical network elements, new physical network elements are not necessarily needed with this single radio handover reference model.[CEP: note that this does not mandate use of Proxy for distributed mobility mgmt.]

* 1. MIHF reference models for link-layer technologies

***Insert subclause 5.5.8***

* + 1. Single radio handover reference model and signaling process

The reference model for single radio handover is shown in Figure 10a.



**Figure 10a Single radio handover reference model.**

The functions in originating network are: OPoS and the proxy function. The functions in target network are: TPoS and the proxy function.

The proxy functions enable signaling between the MN and the target PoA: MN signals with target PoA via OPoS/proxy function, which in turn signals with target PoA via TPoS/proxy function. Target PoA signals with MN (possibly via TPoS proxy function), which in turn signals with MN via OPoS or OPoS proxy function. [CEP: must allow for MIH functions that are NOT necessarily proxy functions]

The signaling process for single radio handover is shown in Figure 10b and is described in the following.



**Figure 10b Signaling process for Single radio handover via proxy functions**

1. MN sends a MIH\_PreReg\_Xfer message to the OPoS which may have a payload of a target network L2 handover frame.
2. Upon receiving this message from MN,
   1. OPoS queries the Information Repository to discover a suitable target network if not already known.
   2. OPoS signals with the TPoA via the TPoS proxy function, that is, OPoS proxy function sends the message to TPoS.
3. Upon receiving this message from MN (either directly or via the OPoS, if the message is received directly from the MN the OPoS is bypassed).
   1. If the target PoA supports SR-MIHF messages, TPoS proxy function sends the MIH\_PreReg\_Xfer to the target PoA .
   2. Else, TPoS performs proxy TPoA function by signaling with this target PoA using other message out of scope of this specification. If the MIH\_PreReg\_Xfer fails because such signaling between TPoS and the TPoA, the MIH\_PreReg\_Xfer\_response will include the indication to show that the fail is owing to TPoA not supporting MIH.