IEEE P802.21
Media Independent Handover Services

|  |
| --- |
| Proposed Remedy for Comment #117 of the WG LB9 on IEEE P802.21.1/D01 draft |
| Date: 2016-01-20 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Hyeong-Ho Lee,Hyunho Park | ETRI |  |  | holee@etri.re.kr hyunhopark@etri.re.kr |

Abstract

This document contains proposed remedy for Comment #117 of the WG LB9 on IEEE P802.21.1 /D01 draft based on the LB9 comments file(DCN: 21-16-0008-01-SAUC).

**Proposed Remedy for Comment #117 of the WG LB9 on IEEE P802.21.1/D01 draft**

Comment #117: Assign appropriate one ("L", "R", or "L, R") to each of MIS commands (MIS\_Prereg\_Xfer, MIS\_N2N\_Prereg\_Xfer, MIS\_Prereg\_ready, and MIS\_CTRL\_Transfer) in Table 4 of page 31

Table 4—MIS commands for handover services

|  |  |  |  |
| --- | --- | --- | --- |
| **MIS command** | **(L) ocal,(R) emote** | **Comments** | **Definedin** |
| MIS\_Net\_HO\_Candidate\_Query | R | Network initiates handover and sends a list of suggested networks and associated points of attachment. | 5.11.3 |
| MIS\_MN\_HO\_Candidate\_Query | R | Command used by MN to query and obtain handover related information about possible candidate networks. | 5.11.4 |
| MIS\_N2N\_HO\_Query\_Resources | R | This command is sent by the serving MISF entity to the target MISF entity to allow for resource query. | 5.11.5 |
| MIS\_MN\_HO\_Commit | R | Command used by MN to notify the serving net- work of the decided target network information. | 5.11.6 |
| MIS\_Net\_HO\_Commit | R | Command used by the network to notify the MN of the decided target network information. | 5.11.7 |
| MIS\_N2N\_HO\_Commit | R | Command used by a serving network to inform a target network that an MN is about to move toward that network, initiate context transfer (if applicable), and perform handover preparation. | 5.11.8 |
| MIS\_MN\_HO\_Complete | R | Notification from MISF of the MN to the target or source MISF indicating the status of handover completion. | 5.11.9 |
| MIS\_N2N\_HO\_Complete | R | Notification from either source or target MISF to the other (i.e., peer) MISF indicating the status of the handover completion. | 5.11.10 |
| MIS\_Net\_HO\_Bcst\_Commit | R | Command used by the network to notify the specific group of MNs of the decided target network information. | 5.11.11 |
| MIS\_Prereg\_Xfer | R | Transport parameters and link layer frames. | 5.11.12 |
| MIS\_N2N\_Prereg\_Xfer | R | Transport link layer frames between the SPoS and the TPos. | 5.12.1 |
| MIS\_Prereg\_Ready | R | Check readiness of preregistration on a target link. | 5.11.13 |
| MIS\_CTRL\_Transfer | R | Deliver control message encapsulated by the MIS header | 5.11.14 |